From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Muhammed Efe Cetin <efectn@protonmail.com>
Date: Tue, 10 Dec 2024 21:10:02 +0300
Subject: arm64: dts: rockchip: mark led as heartbeat indicator for Orange Pi
 5+

---
 arch/arm64/boot/dts/rockchip/rk3588-orangepi-5.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5.dtsi b/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5.dtsi
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5.dtsi
+++ b/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5.dtsi
@@ -93,7 +93,7 @@ led_blue_pwm: led-1 {
 
 		led_green_pwm: led-2 {
 			color = <LED_COLOR_ID_GREEN>;
-			function = LED_FUNCTION_INDICATOR;
+			function = LED_FUNCTION_HEARTBEAT;
 			function-enumerator = <2>;
 			max-brightness = <255>;
 		};
-- 
Armbian

From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Muhammed Efe Cetin <efectn@protonmail.com>
Date: Tue, 10 Dec 2024 21:11:02 +0300
Subject: arm64: dts: rockchip: add bluetooth rfkill node for Orange Pi 5+

---
 arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts b/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
@@ -238,6 +238,13 @@ ir_receiver_pin: ir-receiver-pin {
 		};
 	};
 
+	rfkill-bt {
+		compatible = "rfkill-gpio";
+		label = "rfkill-m2-bt";
+		radio-type = "bluetooth";
+		shutdown-gpios = <&gpio0 RK_PC5 GPIO_ACTIVE_HIGH>;
+	};
+
 	sound {
 		hp_detect: hp-detect {
 			rockchip,pins = <1 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>;
-- 
Armbian

From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Muhammed Efe Cetin <efectn@protonmail.com>
Date: Tue, 10 Dec 2024 21:11:43 +0300
Subject: arm64: dts: rockchip: fix hym8563 pinctrl for Orange Pi 5+

---
 arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts b/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
@@ -222,7 +222,7 @@ &pcie2x1l2 {
 &pinctrl {
 	hym8563 {
 		hym8563_int: hym8563-int {
-			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_none>;
+			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>;
 		};
 	};
 
-- 
Armbian

From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Muhammed Efe Cetin <efectn@protonmail.com>
Date: Thu, 26 Dec 2024 23:45:39 +0300
Subject: arm64: dts: rockchip: add support for HDMI1 port to OPi5+

---
 arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts | 38 ++++++++++
 1 file changed, 38 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts b/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-orangepi-5-plus.dts
@@ -26,6 +26,17 @@ hdmi0_con_in: endpoint {
 		};
 	};
 
+	hdmi1-con {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi1_con_in: endpoint {
+				remote-endpoint = <&hdmi1_out_con>;
+			};
+		};
+	};
+
 	ir-receiver {
 		compatible = "gpio-ir-receiver";
 		gpios = <&gpio4 RK_PB3 GPIO_ACTIVE_LOW>;
@@ -125,10 +136,30 @@ hdmi0_out_con: endpoint {
 	};
 };
 
+&hdmi1 {
+	status = "okay";
+};
+
+&hdmi1_in {
+	hdmi1_in_vp1: endpoint {
+		remote-endpoint = <&vp1_out_hdmi1>;
+	};
+};
+
+&hdmi1_out {
+	hdmi1_out_con: endpoint {
+		remote-endpoint = <&hdmi1_con_in>;
+	};
+};
+
 &hdptxphy0 {
 	status = "okay";
 };
 
+&hdptxphy1 {
+	status = "okay";
+};
+
 &hym8563 {
 	interrupt-parent = <&gpio0>;
 	interrupts = <RK_PB0 IRQ_TYPE_LEVEL_LOW>;
@@ -349,3 +380,10 @@ vp0_out_hdmi0: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
 		remote-endpoint = <&hdmi0_in_vp0>;
 	};
 };
+
+&vp1 {
+	vp1_out_hdmi1: endpoint@ROCKCHIP_VOP2_EP_HDMI1 {
+		reg = <ROCKCHIP_VOP2_EP_HDMI1>;
+		remote-endpoint = <&hdmi1_in_vp1>;
+	};
+};
-- 
Armbian

