// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2020 Rockchip Electronics Co., Ltd.
 *
 */
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/pwm/pwm.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/soc/rockchip,vop2.h>
#include "rk3568.dtsi"

/ {
	model = "Youyeetoo YY3568";
	compatible = "youyeetoo,yy3568", "rockchip,rk3568";

	aliases {
		ethernet0 = &gmac0;
		ethernet1 = &gmac1;
		mmc2 = &sdmmc2;
		mmc1 = &sdmmc0;
		mmc0 = &sdhci;
	};

	gpio-leds {
		compatible = "gpio-leds";

		led_user: led-0 {
			gpios = <&gpio3 RK_PA4 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "heartbeat";
			pinctrl-names = "default";
			pinctrl-0 = <&led_user_en>;
		};
		led_power: led-1 {
			gpios = <&gpio2 RK_PB2 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "heartbeat";
			pinctrl-names = "default";
			pinctrl-0 = <&led_power_en>;
		};
	};

	hdmi-con {
		compatible = "hdmi-connector";
		type = "a";

		port {
			hdmi_con_in: endpoint {
				remote-endpoint = <&hdmi_out_con>;
			};
		};
	};

	rk809-sound {
		compatible = "simple-audio-card";
		pinctrl-names = "default";
		pinctrl-0 = <&hp_det>;
		hp-det-gpio = <&gpio3 RK_PC2 GPIO_ACTIVE_LOW>;
		simple-audio-card,format = "i2s";
		simple-audio-card,name = "Analog RK809";
		simple-audio-card,mclk-fs = <256>;

		simple-audio-card,cpu {
			sound-dai = <&i2s1_8ch>;
		};
		simple-audio-card,codec {
			sound-dai = <&rk809>;
		};
	};

	vcc5v0_otg: regulator-vbus-typec {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PB7 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_otg_en>;
		regulator-name = "vcc5v0_otg";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_sys>;
	};

	/* actually fed by vcc5v0_sys, dependent
	 * on pi6c clock generator
	 */

	vcc5v0_host: vcc5v0-host-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PD6 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_host_en>;
		regulator-name = "vcc5v0_host";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vcc3v3_pcie30x1: regulator-vcc3v3-pcie30x1 {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PC5 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&pcie30x1_enable_h>;
		regulator-name = "vcc3v3_pcie30x1";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vcc3v3_pi6c_05: regulator-vcc3v3-pi6c-05 {
		compatible = "regulator-fixed";
		enable-active-high;
		gpios = <&gpio0 RK_PC7 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&pcie_enable_h>;
		regulator-name = "vcc3v3_pcie";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vcc5v0_sys>;
	};

    pcie30_avdd0v9: regulator-pcie30-avdd0v9 {
		compatible = "regulator-fixed";
		regulator-name = "pcie30_avdd0v9";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <900000>;
		regulator-max-microvolt = <900000>;
		vin-supply = <&vcc3v3_sys>;
	};

	pcie30_avdd1v8: regulator-pcie30-avdd1v8 {
		compatible = "regulator-fixed";
		regulator-name = "pcie30_avdd1v8";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		vin-supply = <&vcc3v3_sys>;
	};

	vcc3v3_sys: regulator-vcc3v3-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vcc12v_input>;
	};

	vcc5v0_sys: regulator-vcc5v0-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc12v_input>;
	};

	/* labeled +12v_input in schematic */
	vcc12v_input: regulator-vcc5v-input {
		compatible = "regulator-fixed";
		regulator-name = "vcc12v_input";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
	};
};

&combphy1 {
	phy-supply = <&vcc3v3_pcie30x1>;
	status = "okay";
};

&combphy0 {
	status = "okay";
};

&combphy2 {
	status = "okay";
};

&cpu0 {
	cpu-supply = <&vdd_cpu>;
};

&cpu1 {
	cpu-supply = <&vdd_cpu>;
};

&cpu2 {
	cpu-supply = <&vdd_cpu>;
};

&cpu3 {
	cpu-supply = <&vdd_cpu>;
};

&gpu {
	mali-supply = <&vdd_gpu>;
	status = "okay";
};

&vop {
	assigned-clocks = <&cru DCLK_VOP0>, <&cru DCLK_VOP1>;
	assigned-clock-parents = <&pmucru PLL_HPLL>, <&cru PLL_VPLL>;
	status = "okay";
};

&vop_mmu {
	status = "okay";
};

&vp0 {
	vp0_out_hdmi: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
		reg = <ROCKCHIP_VOP2_EP_HDMI0>;
		remote-endpoint = <&hdmi_in_vp0>;
	};
};

&hdmi {
	assigned-clocks = <&cru CLK_HDMI_CEC>;
	assigned-clock-rates = <32768>;
	avdd-0v9-supply = <&vdda0v9_image>;
	avdd-1v8-supply = <&vcca1v8_image>;
	status = "okay";
};

&hdmi_in {
	hdmi_in_vp0: endpoint {
		remote-endpoint = <&vp0_out_hdmi>;
	};
};

&hdmi_out {
	hdmi_out_con: endpoint {
		remote-endpoint = <&hdmi_con_in>;
	};
};

&hdmi_sound {
	status = "okay";
};

&hdmi_sound {
	status = "okay";
};

&pcie2x1 {
	pinctrl-names = "default";
	reset-gpios = <&gpio1 RK_PB2 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_pi6c_05>;
	status = "okay";
};

&pcie30phy {
	data-lanes = <1 2>;
	status = "okay";
};

&pcie3x2 {
	num-lanes = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&pcie30x2_reset_h>;
	reset-gpios = <&gpio2 RK_PD6 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_pi6c_05>;
	status = "okay";
};

&i2c0 {
	status = "okay";

	vdd_cpu: regulator@1c {
		compatible = "tcs,tcs4525";
		reg = <0x1c>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <800000>;
		regulator-max-microvolt = <1150000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc12v_input>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	rk809: pmic@20 {
		compatible = "rockchip,rk809";
		reg = <0x20>;
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PA3 IRQ_TYPE_LEVEL_LOW>;
		#clock-cells = <1>;
		pinctrl-names = "default";
		pinctrl-0 = <&pmic_int>;
		system-power-controller;
		wakeup-source;

		vcc1-supply = <&vcc3v3_sys>;
		vcc2-supply = <&vcc3v3_sys>;
		vcc3-supply = <&vcc3v3_sys>;
		vcc4-supply = <&vcc3v3_sys>;
		vcc5-supply = <&vcc3v3_sys>;
		vcc6-supply = <&vcc3v3_sys>;
		vcc7-supply = <&vcc3v3_sys>;
		vcc8-supply = <&vcc3v3_sys>;
		vcc9-supply = <&vcc3v3_sys>;

		regulators {
			vdd_logic: DCDC_REG1 {
				regulator-name = "vdd_logic";
				regulator-always-on;
				regulator-boot-on;
				regulator-initial-mode = <0x2>;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_gpu: DCDC_REG2 {
				regulator-name = "vdd_gpu";
				regulator-always-on;
				regulator-initial-mode = <0x2>;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_ddr: DCDC_REG3 {
				regulator-name = "vcc_ddr";
				regulator-always-on;
				regulator-boot-on;
				regulator-initial-mode = <0x2>;

				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vdd_npu: DCDC_REG4 {
				regulator-name = "vdd_npu";
				regulator-initial-mode = <0x2>;
				regulator-min-microvolt = <500000>;
				regulator-max-microvolt = <1350000>;
				regulator-ramp-delay = <6001>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8: DCDC_REG5 {
				regulator-name = "vcc_1v8";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdda0v9_image: LDO_REG1 {
				regulator-name = "vdda0v9_image";
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdda_0v9: LDO_REG2 {
				regulator-name = "vdda_0v9";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdda0v9_pmu: LDO_REG3 {
				regulator-name = "vdda0v9_pmu";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <900000>;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <900000>;
				};
			};

			vccio_acodec: LDO_REG4 {
				regulator-name = "vccio_acodec";
				regulator-always-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vccio_sd: LDO_REG5 {
				regulator-name = "vccio_sd";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v3_pmu: LDO_REG6 {
				regulator-name = "vcc3v3_pmu";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vcca_1v8: LDO_REG7 {
				regulator-name = "vcca_1v8";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcca1v8_pmu: LDO_REG8 {
				regulator-name = "vcca1v8_pmu";
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcca1v8_image: LDO_REG9 {
				regulator-name = "vcca1v8_image";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_3v3: SWITCH_REG1 {
				regulator-name = "vcc_3v3";
				regulator-always-on;
				regulator-boot-on;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc3v3_sd: SWITCH_REG2 {
				regulator-name = "vcc3v3_sd";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&pinctrl {
	leds {
		led_user_en: led_user_en {
			rockchip,pins = <0 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
		};
		led_power_en: led_power_en {
			rockchip,pins = <2 RK_PB2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	headphone {
		hp_det: hp-det {
			rockchip,pins = <3 RK_PC2 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	pmic {
		pmic_int: pmic_int {
			rockchip,pins = <0 RK_PA3 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	pcie {
		pcie30x1_enable_h: pcie30x1-enable-h {
			rockchip,pins = <0 RK_PC5 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		pcie30x2_reset_h: pcie30x2-reset-h {
			rockchip,pins = <2 RK_PD6 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		pcie_enable_h: pcie-enable-h {
			rockchip,pins = <0 RK_PC7 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb {
		vcc5v0_host_en: vcc5v0-host-en {
			rockchip,pins = <0 RK_PD6 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		vcc5v0_otg_en: vcc5v0_otg_en {
			rockchip,pins = <0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&i2s1_8ch {
	rockchip,trcm-sync-tx-only;
	status = "okay";
};

&pmu_io_domains {
	pmuio1-supply = <&vcc3v3_pmu>;
	pmuio2-supply = <&vcc3v3_pmu>;
	vccio1-supply = <&vccio_acodec>;
	vccio2-supply = <&vcc_1v8>;
	vccio3-supply = <&vccio_sd>;
	vccio4-supply = <&vcc_1v8>;
	vccio5-supply = <&vcc_3v3>;
	vccio6-supply = <&vcc_1v8>;
	vccio7-supply = <&vcc_3v3>;
	status = "okay";
};

&saradc {
	vref-supply = <&vcca_1v8>;
	status = "okay";
};

&sdhci {
	bus-width = <8>;
	max-frequency = <200000000>;
	non-removable;
	pinctrl-names = "default";
	pinctrl-0 = <&emmc_bus8 &emmc_clk &emmc_cmd &emmc_datastrobe>;
	vmmc-supply = <&vcc_3v3>;
	vqmmc-supply = <&vcc_1v8>;
	status = "okay";
};

&tsadc {
	rockchip,hw-tshut-mode = <1>;
	rockchip,hw-tshut-polarity = <0>;
	status = "okay";
};

&uart2 {
	status = "okay";
};

&sdmmc0 {
	bus-width = <4>;
	cap-sd-highspeed;
	cd-gpios = <&gpio0 RK_PA4 GPIO_ACTIVE_LOW>;
	/* Also used in pcie30x1_clkreqnm0 */
	disable-wp;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc0_bus4 &sdmmc0_clk &sdmmc0_cmd>;
	sd-uhs-sdr104;
	vmmc-supply = <&vcc3v3_sd>;
	vqmmc-supply = <&vccio_sd>;
	status = "okay";
};

&sdmmc2 {
	bus-width = <4>;
	cap-sd-highspeed;
	cd-gpios = <&gpio3 RK_PD5 GPIO_ACTIVE_LOW>;
	disable-wp;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc2m0_bus4 &sdmmc2m0_clk &sdmmc2m0_cmd>;
	sd-uhs-sdr104;
	status = "okay";
};

&mdio0 {
	rgmii_phy0: ethernet-phy@0 {
		compatible = "ethernet-phy-id001c.c916";
		reg = <0x0>;
		reset-assert-us = <20000>;
		reset-deassert-us = <100000>;
		reset-gpios = <&gpio2 RK_PD3 GPIO_ACTIVE_LOW>;
	};
};

&mdio1 {
	rgmii_phy1: ethernet-phy@0 {
		compatible = "ethernet-phy-id001c.c916";
		reg = <0x0>;
		reset-assert-us = <20000>;
		reset-deassert-us = <100000>;
		reset-gpios = <&gpio2 RK_PD1 GPIO_ACTIVE_LOW>;
	};
};

&gmac0 {
	assigned-clocks = <&cru SCLK_GMAC0_RX_TX>, <&cru SCLK_GMAC0>;
	assigned-clock-parents = <&cru SCLK_GMAC0_RGMII_SPEED>;
	assigned-clock-rates = <0>, <125000000>;
	clock_in_out = "output";
	phy-handle = <&rgmii_phy0>;
	phy-mode = "rgmii";
	pinctrl-names = "default";
	pinctrl-0 = <&gmac0_miim
		     &gmac0_tx_bus2
		     &gmac0_rx_bus2
		     &gmac0_rgmii_clk
		     &gmac0_rgmii_bus>;
	status = "okay";
};

&gmac1 {
	assigned-clocks = <&cru SCLK_GMAC1_RX_TX>, <&cru SCLK_GMAC1>;
	assigned-clock-parents = <&cru SCLK_GMAC1_RGMII_SPEED>;
	assigned-clock-rates = <0>, <125000000>;
	clock_in_out = "output";
	phy-handle = <&rgmii_phy1>;
	phy-mode = "rgmii";
	pinctrl-names = "default";
	pinctrl-0 = <&gmac1m1_miim
				&gmac1m1_tx_bus2
				&gmac1m1_rx_bus2
				&gmac1m1_rgmii_clk
				&gmac1m1_rgmii_bus>;
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&usb_host0_xhci {
	dr_mode = "host";
	extcon = <&usb2phy0>;
	status = "okay";
};

&usb_host1_ehci {
	status = "okay";
};

&usb_host1_ohci {
	status = "okay";
};

&usb_host1_xhci {
	status = "okay";
};

&usb2phy0 {
	status = "okay";
};

&usb2phy0_host {
	phy-supply = <&vcc5v0_host>;
	status = "okay";
};

&usb2phy1 {
	status = "okay";
};

&usb2phy1_host {
	phy-supply = <&vcc5v0_host>;
	status = "okay";
};

&usb2phy1_otg {
	phy-supply = <&vcc5v0_host>;
	status = "okay";
};