From ad81b4fe119c8d10e47fc7aa721f5505103176ea Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Sun, 14 Apr 2019 23:46:47 +0800
Subject: arm64: dts: sun50i-a64-pinetab: enable RTL8723CS bluetooth

PineTab has a RTL8723CS Wi-Fi/BT combo chip on board, the bluetooth part
of it communicates with A64 via UART, and the power of it is controlled
with some GPIO at PL bank.

Enable the bluetooth in the device tree.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 .../boot/dts/allwinner/sun50i-a64-pinetab.dts      | 14 ++++++++++++++
 1 file changed, 14 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
index 8c91ed7083d7..419fe19b4a6f 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
@@ -511,6 +511,20 @@ &uart0 {
 	status = "okay";
 };
 
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>, <&uart1_rts_cts_pins>;
+	status = "okay";
+
+	bluetooth {
+		compatible = "realtek,rtl8723cs-bt";
+		reset-gpios = <&r_pio 0 4 GPIO_ACTIVE_LOW>; /* PL4 */
+		device-wake-gpios = <&r_pio 0 5 GPIO_ACTIVE_LOW>; /* PL5 */
+		host-wake-gpios = <&r_pio 0 6 GPIO_ACTIVE_HIGH>; /* PL6 */
+		firmware-postfix = "pinebook";
+	};
+};
+
 &usb_otg {
 	dr_mode = "otg";
 	status = "okay";
-- 
2.35.3

