From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Fri, 28 Jan 2022 16:12:37 +0300
Subject: arm:dts: sunxi-h3-h5.dtsi force mmc0 bus-width

---
 arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi b/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi
index 111111111111..222222222222 100644
--- a/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi
+++ b/arch/arm/boot/dts/allwinner/sunxi-h3-h5.dtsi
@@ -221,6 +221,7 @@ mmc0: mmc@1c0f000 {
 			resets = <&ccu RST_BUS_MMC0>;
 			reset-names = "ahb";
 			interrupts = <GIC_SPI 60 IRQ_TYPE_LEVEL_HIGH>;
+			bus-width = <0x4>;
 			status = "disabled";
 			#address-cells = <1>;
 			#size-cells = <0>;
-- 
Armbian

