From a5de8971554d5cd8ff1bb665d7e5c58087a7f1a8 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Wed, 2 Feb 2022 13:02:10 +0300
Subject: arm64:dts:allwinner:overlay: Add Overlays for sunxi64

---
 arch/arm64/boot/dts/allwinner/Makefile        |   2 +
 .../arm64/boot/dts/allwinner/overlay/Makefile |  58 ++++
 .../overlay/README.sun50i-a64-overlays        | 196 ++++++++++++++
 .../overlay/README.sun50i-h5-overlays         | 250 ++++++++++++++++++
 .../overlay/sun50i-a64-fixup.scr-cmd          |  95 +++++++
 .../allwinner/overlay/sun50i-a64-i2c0.dtso    |  32 +++
 .../allwinner/overlay/sun50i-a64-i2c1.dtso    |  22 ++
 .../overlay/sun50i-a64-pps-gpio.dtso          |  29 ++
 .../overlay/sun50i-a64-spi-add-cs1.dtso       |  41 +++
 .../overlay/sun50i-a64-spi-jedec-nor.dtso     |  34 +++
 .../overlay/sun50i-a64-spi-spidev.dtso        |  42 +++
 .../allwinner/overlay/sun50i-a64-uart1.dtso   |  22 ++
 .../allwinner/overlay/sun50i-a64-uart2.dtso   |  37 +++
 .../allwinner/overlay/sun50i-a64-uart3.dtso   |  32 +++
 .../allwinner/overlay/sun50i-a64-uart4.dtso   |  37 +++
 .../allwinner/overlay/sun50i-a64-w1-gpio.dtso |  29 ++
 .../overlay/sun50i-h5-analog-codec.dtso       |  17 ++
 .../dts/allwinner/overlay/sun50i-h5-cir.dtso  |  15 ++
 .../allwinner/overlay/sun50i-h5-fixup.scr-cmd | 110 ++++++++
 .../dts/allwinner/overlay/sun50i-h5-i2c0.dtso |  20 ++
 .../dts/allwinner/overlay/sun50i-h5-i2c1.dtso |  20 ++
 .../dts/allwinner/overlay/sun50i-h5-i2c2.dtso |  20 ++
 .../allwinner/overlay/sun50i-h5-pps-gpio.dtso |  29 ++
 .../dts/allwinner/overlay/sun50i-h5-pwm.dtso  |  39 +++
 .../overlay/sun50i-h5-spdif-out.dtso          |  38 +++
 .../overlay/sun50i-h5-spi-add-cs1.dtso        |  41 +++
 .../overlay/sun50i-h5-spi-jedec-nor.dtso      |  42 +++
 .../overlay/sun50i-h5-spi-spidev.dtso         |  42 +++
 .../allwinner/overlay/sun50i-h5-uart1.dtso    |  22 ++
 .../allwinner/overlay/sun50i-h5-uart2.dtso    |  32 +++
 .../allwinner/overlay/sun50i-h5-uart3.dtso    |  32 +++
 .../allwinner/overlay/sun50i-h5-usbhost0.dtso |  27 ++
 .../allwinner/overlay/sun50i-h5-usbhost1.dtso |  27 ++
 .../allwinner/overlay/sun50i-h5-usbhost2.dtso |  27 ++
 .../allwinner/overlay/sun50i-h5-usbhost3.dtso |  27 ++
 .../allwinner/overlay/sun50i-h5-w1-gpio.dtso  |  29 ++
 .../allwinner/overlay/sun50i-h6-fixup.scr-cmd | 110 ++++++++
 .../dts/allwinner/overlay/sun50i-h6-i2c0.dtso |  20 ++
 .../dts/allwinner/overlay/sun50i-h6-i2c1.dtso |  20 ++
 .../dts/allwinner/overlay/sun50i-h6-i2c2.dtso |  20 ++
 .../allwinner/overlay/sun50i-h6-ruart.dtso    |  13 +
 .../overlay/sun50i-h6-spi-add-cs1.dtso        |  41 +++
 .../overlay/sun50i-h6-spi-jedec-nor.dtso      |  42 +++
 .../overlay/sun50i-h6-spi-spidev.dtso         |  42 +++
 .../overlay/sun50i-h6-spi-spidev1.dtso        |  30 +++
 .../allwinner/overlay/sun50i-h6-uart1.dtso    |  22 ++
 .../allwinner/overlay/sun50i-h6-uart2.dtso    |  32 +++
 .../allwinner/overlay/sun50i-h6-uart3.dtso    |  32 +++
 .../allwinner/overlay/sun50i-h6-w1-gpio.dtso  |  29 ++
 49 files changed, 2067 insertions(+)
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/Makefile
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/README.sun50i-a64-overlays
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/README.sun50i-h5-overlays
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-fixup.scr-cmd
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-i2c0.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-i2c1.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-pps-gpio.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-add-cs1.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-jedec-nor.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-spidev.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart1.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart2.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart3.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart4.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-w1-gpio.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-analog-codec.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-cir.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-fixup.scr-cmd
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c0.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c1.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c2.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-pps-gpio.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-pwm.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spdif-out.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-add-cs1.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-jedec-nor.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-spidev.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart1.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart2.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart3.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost0.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost1.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost2.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost3.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-w1-gpio.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-fixup.scr-cmd
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c0.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c1.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c2.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-ruart.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-add-cs1.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-jedec-nor.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-spidev.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-spidev1.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart1.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart2.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart3.dtso
 create mode 100644 arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-w1-gpio.dtso

diff --git a/arch/arm64/boot/dts/allwinner/Makefile b/arch/arm64/boot/dts/allwinner/Makefile
index f80ea3d3ecec..80098fa014ac 100644
--- a/arch/arm64/boot/dts/allwinner/Makefile
+++ b/arch/arm64/boot/dts/allwinner/Makefile
@@ -57,3 +57,5 @@ dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h700-anbernic-rg35xx-2024.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h700-anbernic-rg35xx-h.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h700-anbernic-rg35xx-plus.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h700-anbernic-rg35xx-sp.dtb
+
+subdir-y	:= $(dts-dirs) overlay
diff --git a/arch/arm64/boot/dts/allwinner/overlay/Makefile b/arch/arm64/boot/dts/allwinner/overlay/Makefile
new file mode 100644
index 000000000000..ae404a5258a9
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/Makefile
@@ -0,0 +1,58 @@
+# SPDX-License-Identifier: GPL-2.0
+dtb-$(CONFIG_ARCH_SUNXI) += \
+	sun50i-a64-i2c0.dtbo \
+	sun50i-a64-i2c1.dtbo \
+	sun50i-a64-pps-gpio.dtbo \
+	sun50i-a64-spi-add-cs1.dtbo \
+	sun50i-a64-spi-jedec-nor.dtbo \
+	sun50i-a64-spi-spidev.dtbo \
+	sun50i-a64-uart1.dtbo \
+	sun50i-a64-uart2.dtbo \
+	sun50i-a64-uart3.dtbo \
+	sun50i-a64-uart4.dtbo \
+	sun50i-a64-w1-gpio.dtbo \
+	sun50i-h5-analog-codec.dtbo \
+	sun50i-h5-cir.dtbo \
+	sun50i-h5-i2c0.dtbo \
+	sun50i-h5-i2c1.dtbo \
+	sun50i-h5-i2c2.dtbo \
+	sun50i-h5-pps-gpio.dtbo \
+	sun50i-h5-pwm.dtbo \
+	sun50i-h5-spdif-out.dtbo \
+	sun50i-h5-spi-add-cs1.dtbo \
+	sun50i-h5-spi-jedec-nor.dtbo \
+	sun50i-h5-spi-spidev.dtbo \
+	sun50i-h5-uart1.dtbo \
+	sun50i-h5-uart2.dtbo \
+	sun50i-h5-uart3.dtbo \
+	sun50i-h5-usbhost0.dtbo \
+	sun50i-h5-usbhost1.dtbo \
+	sun50i-h5-usbhost2.dtbo \
+	sun50i-h5-usbhost3.dtbo \
+	sun50i-h5-w1-gpio.dtbo \
+	sun50i-h6-i2c0.dtbo \
+	sun50i-h6-i2c1.dtbo \
+	sun50i-h6-i2c2.dtbo \
+	sun50i-h6-ruart.dtbo \
+	sun50i-h6-spi-add-cs1.dtbo \
+	sun50i-h6-spi-jedec-nor.dtbo \
+	sun50i-h6-spi-spidev.dtbo \
+	sun50i-h6-spi-spidev1.dtbo \
+	sun50i-h6-uart1.dtbo \
+	sun50i-h6-uart2.dtbo \
+	sun50i-h6-uart3.dtbo \
+	sun50i-h6-w1-gpio.dtbo
+
+scr-$(CONFIG_ARCH_SUNXI) += \
+	sun50i-a64-fixup.scr \
+	sun50i-h5-fixup.scr \
+	sun50i-h6-fixup.scr
+
+dtbotxt-$(CONFIG_ARCH_SUNXI) += \
+	README.sun50i-a64-overlays \
+	README.sun50i-h5-overlays
+
+targets += $(dtb-y) $(scr-y) $(dtbotxt-y)
+
+always		:= $(dtb-y) $(scr-y) $(dtbotxt-y)
+clean-files	:= *.dtbo *.scr
diff --git a/arch/arm64/boot/dts/allwinner/overlay/README.sun50i-a64-overlays b/arch/arm64/boot/dts/allwinner/overlay/README.sun50i-a64-overlays
new file mode 100644
index 000000000000..cd9dbc686412
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/README.sun50i-a64-overlays
@@ -0,0 +1,196 @@
+This document describes overlays provided in the kernel packages
+For generic Armbian overlays documentation please see
+https://docs.armbian.com/Hardware_Allwinner_overlays/
+
+### Platform:
+
+sun50i-a64 (Allwinner A64)
+
+### Platform details:
+
+Supported pin banks: PB, PC, PD, PH
+
+Both SPI controllers have only one hardware CS pin exposed,
+adding fixed software (GPIO) chip selects is possible with a separate overlay
+
+I2C controller 2 (PE14, PE15) pins are used for non-I2C CSI functions or are not available
+on supported boards, so this controller is not supported in provided overlays
+
+### Provided overlays:
+
+- i2c0
+- i2c1
+- pps-gpio
+- spi-add-cs1
+- spi-jedec-nor
+- spi-spidev
+- uart1
+- uart2
+- uart3
+- uart4
+- w1-gpio
+
+### Overlay details:
+
+### i2c0
+
+Activates TWI/I2C bus 0
+
+I2C0 pins (SCL, SDA): PH0, PH1
+
+### i2c1
+
+Activates TWI/I2C bus 1
+
+I2C1 pins (SCL, SDA): PH2, PH3
+
+### pps-gpio
+
+Activates pulse-per-second GPIO client
+
+Parameters:
+
+param_pps_pin (pin)
+	Pin PPS source is connected to
+	Optional
+	Default: PD4
+
+param_pps_falling_edge (bool)
+	Assert by falling edge
+	Optional
+	Default: 0
+	When set (to 1), assert is indicated by a falling edge
+		(instead of by a rising edge)
+
+### spi-add-cs1
+
+Adds support for using SPI chip select 1 with GPIO for both SPI controllers
+Respective GPIO will be claimed only if controller is enabled by another overlay
+This overlay is required for using chip select 1 with other SPI overlays
+
+SPI 0 pins (CS1): PB6
+SPI 1 pins (CS1): PD6
+
+### spi-jedec-nor
+
+Activates MTD support for JEDEC compatible SPI NOR flash chips on SPI bus
+supported by the kernel SPI NOR driver
+
+SPI 0 pins (MOSI, MISO, SCK, CS): PC0, PC1, PC2, PC3
+SPI 1 pins (MOSI, MISO, SCK, CS): PD2, PD3, PD1, PD0
+
+Parameters:
+
+param_spinor_spi_bus (int)
+	SPI bus to activate SPI NOR flash support on
+	Required
+	Supported values: 0, 1
+
+param_spinor_spi_cs (int)
+	SPI chip select number
+	Optional
+	Default: 0
+	Supported values: 0, 1
+	Using chip select 1 requires using "spi-add-cs1" overlay
+
+param_spinor_max_freq (int)
+	Maximum SPI frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### spi-spidev
+
+Activates SPIdev device node (/dev/spidevX.Y) for userspace SPI access,
+where X is the bus number and Y is the CS number
+
+SPI 0 pins (MOSI, MISO, SCK, CS): PC0, PC1, PC2, PC3
+SPI 1 pins (MOSI, MISO, SCK, CS): PD2, PD3, PD1, PD0
+
+Parameters:
+
+param_spidev_spi_bus (int)
+	SPI bus to activate SPIdev support on
+	Required
+	Supported values: 0, 1
+
+param_spidev_spi_cs (int)
+	SPI chip select number
+	Optional
+	Default: 0
+	Supported values: 0, 1
+	Using chip select 1 requires using "spi-add-cs1" overlay
+
+param_spidev_max_freq (int)
+	Maximum SPIdev frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### uart1
+
+Activates serial port 1 (/dev/ttyS1)
+
+UART 1 pins (TX, RX, RTS, CTS): PG6, PG7, PG8, PG9
+
+Parameters:
+
+param_uart1_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable
+
+### uart2
+
+Activates serial port 2 (/dev/ttyS2)
+
+UART 2 pins (TX, RX, RTS, CTS): PB0, PB1, PB2, PB3
+
+Parameters:
+
+param_uart2_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
+
+### uart3
+
+Activates serial port 3 (/dev/ttyS3)
+
+UART 3 pins (TX, RX): PD0, PD1
+
+### uart4
+
+Activates serial port 4 (/dev/ttyS4)
+
+UART 4 pins (TX, RX, RTS, CTS): PD2, PD3, PD4, PD5
+
+Parameters:
+
+param_uart2_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
+
+### w1-gpio
+
+Activates 1-Wire GPIO master
+Requires external pull-up resistor on data pin
+
+Parameters:
+
+param_w1_pin (pin)
+	Data pin for 1-Wire master
+	Optional
+	Default: PD4
+
+param_w1_pin_int_pullup (bool)
+	Enable internal pull-up for the data pin
+	Optional
+	Default: 0
+	Set to 1 to enable the pull-up
+	This option should not be used with multiple devices, parasite power setup
+		or long wires -	please use external pull-up resistor instead
diff --git a/arch/arm64/boot/dts/allwinner/overlay/README.sun50i-h5-overlays b/arch/arm64/boot/dts/allwinner/overlay/README.sun50i-h5-overlays
new file mode 100644
index 000000000000..1ac7fbcf62d1
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/README.sun50i-h5-overlays
@@ -0,0 +1,250 @@
+This document describes overlays provided in the kernel packages
+For generic Armbian overlays documentation please see
+https://docs.armbian.com/User-Guide_Allwinner_overlays/
+
+### Platform:
+
+sun50i-h5 (Allwinner H5)
+
+### Platform details:
+
+Supported pin banks: PA, PC, PD, PG
+
+Both SPI controllers have only one hardware CS pin exposed,
+adding fixed software (GPIO) chip selects is possible with a separate overlay
+
+### Provided overlays:
+
+- analog-codec
+- cir
+- i2c0
+- i2c1
+- i2c2
+- pps-gpio
+- pwm
+- spdif-out
+- spi-add-cs1
+- spi-jedec-nor
+- spi-spidev
+- uart1
+- uart2
+- uart3
+- usbhost0
+- usbhost1
+- usbhost2
+- usbhost3
+- w1-gpio
+
+### Overlay details:
+
+### analog-codec
+
+Activates SoC analog codec driver that provides Line Out and Mic In
+functionality
+
+### cir
+
+Activates CIR (Infrared remote) receiver
+
+CIR pin: PL11
+
+### i2c0
+
+Activates TWI/I2C bus 0
+
+I2C0 pins (SCL, SDA): PA11, PA12
+
+### i2c1
+
+Activates TWI/I2C bus 1
+
+I2C1 pins (SCL, SDA): PA18, PA19
+
+### i2c2
+
+Activates TWI/I2C bus 2
+
+I2C2 pins (SCL, SDA): PE12, PE13
+
+On most board this bus is wired to Camera (CSI) socket
+
+### pps-gpio
+
+Activates pulse-per-second GPIO client
+
+Parameters:
+
+param_pps_pin (pin)
+	Pin PPS source is connected to
+	Optional
+	Default: PD14
+
+param_pps_falling_edge (bool)
+	Assert by falling edge
+	Optional
+	Default: 0
+	When set (to 1), assert is indicated by a falling edge
+		(instead of by a rising edge)
+
+### pwm
+
+Activates hardware PWM controller
+
+PWM pin: PA5
+
+Pin PA5 is used as UART0 RX by default, so if this overlay is activated,
+UART0 and kernel console on ttyS0 will be disabled
+
+### spdif-out
+
+Activates SPDIF/Toslink audio output
+
+SPDIF pin: PA17
+
+### spi-add-cs1
+
+Adds support for using SPI chip select 1 with GPIO for both SPI controllers
+Respective GPIO will be claimed only if controller is enabled by another
+overlay
+This overlay is required for using chip select 1 with other SPI overlays
+Due to the u-boot limitations CS1 pin can't be customized by a parameter, but
+it can be changed by using an edited copy of this overlay
+A total of 4 chip selects can be used with custom overlays (1 HW + 3 GPIO)
+
+SPI 0 pins (CS1): PA21
+SPI 1 pins (CS1): PA10
+
+### spi-jedec-nor
+
+Activates MTD support for JEDEC compatible SPI NOR flash chips on SPI bus
+supported by the kernel SPI NOR driver
+
+SPI 0 pins (MOSI, MISO, SCK, CS): PC0, PC1, PC2, PC3
+SPI 1 pins (MOSI, MISO, SCK, CS): PA15, PA16, PA14, PA13
+
+Parameters:
+
+param_spinor_spi_bus (int)
+	SPI bus to activate SPI NOR flash support on
+	Required
+	Supported values: 0, 1
+
+param_spinor_spi_cs (int)
+	SPI chip select number
+	Optional
+	Default: 0
+	Supported values: 0, 1
+	Using chip select 1 requires using "spi-add-cs1" overlay
+
+param_spinor_max_freq (int)
+	Maximum SPI frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### spi-spidev
+
+Activates SPIdev device node (/dev/spidevX.Y) for userspace SPI access,
+where X is the bus number and Y is the CS number
+
+SPI 0 pins (MOSI, MISO, SCK, CS): PC0, PC1, PC2, PC3
+SPI 1 pins (MOSI, MISO, SCK, CS): PA15, PA16, PA14, PA13
+
+Parameters:
+
+param_spidev_spi_bus (int)
+	SPI bus to activate SPIdev support on
+	Required
+	Supported values: 0, 1
+
+param_spidev_spi_cs (int)
+	SPI chip select number
+	Optional
+	Default: 0
+	Supported values: 0, 1
+	Using chip select 1 requires using "spi-add-cs1" overlay
+
+param_spidev_max_freq (int)
+	Maximum SPIdev frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### uart1
+
+Activates serial port 1 (/dev/ttyS1)
+
+UART 1 pins (TX, RX, RTS, CTS): PG6, PG7, PG8, PG9
+
+Parameters:
+
+param_uart1_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable
+
+### uart2
+
+Activates serial port 2 (/dev/ttyS2)
+
+UART 2 pins (TX, RX, RTS, CTS): PA0, PA1, PA2, PA3
+
+Parameters:
+
+param_uart2_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
+
+### uart3
+
+Activates serial port 3 (/dev/ttyS3)
+
+UART 3 pins (TX, RX, RTS, CTS): PA13, PA14, PA15, PA16
+
+Parameters:
+
+param_uart3_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
+
+### usbhost0
+
+Activates USB host controller 0
+
+### usbhost1
+
+Activates USB host controller 1
+
+### usbhost2
+
+Activates USB host controller 2
+
+### usbhost3
+
+Activates USB host controller 3
+
+### w1-gpio
+
+Activates 1-Wire GPIO master
+Requires an external pull-up resistor on the data pin
+or enabling the internal pull-up
+
+Parameters:
+
+param_w1_pin (pin)
+	Data pin for 1-Wire master
+	Optional
+	Default: PD14
+
+param_w1_pin_int_pullup (bool)
+	Enable internal pull-up for the data pin
+	Optional
+	Default: 0
+	Set to 1 to enable the pull-up
+	This option should not be used with multiple devices, parasite power setup
+		or long wires -	please use external pull-up resistor instead
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-fixup.scr-cmd b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-fixup.scr-cmd
new file mode 100644
index 000000000000..9b34c05ecf18
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-fixup.scr-cmd
@@ -0,0 +1,95 @@
+# overlays fixup script
+# implements (or rather substitutes) overlay arguments functionality
+# using u-boot scripting, environment variables and "fdt" command
+
+# setexpr test_var ${tmp_bank} - A
+# works only for hex numbers (A-F)
+
+setenv decompose_pin 'setexpr tmp_bank sub "P(B|C|D|H)\\d+" "\\1";
+setexpr tmp_pin sub "P\\S(\\d+)" "\\1";
+test "${tmp_bank}" = "B" && setenv tmp_bank 1;
+test "${tmp_bank}" = "C" && setenv tmp_bank 2;
+test "${tmp_bank}" = "D" && setenv tmp_bank 3;
+test "${tmp_bank}" = "H" && setenv tmp_bank 7'
+
+if test -n "${param_spinor_spi_bus}"; then
+	test "${param_spinor_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c68000"
+	test "${param_spinor_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c69000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spiflash@0 status "okay"
+	if test -n "${param_spinor_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spiflash@0 spi-max-frequency "<${param_spinor_max_freq}>"
+	fi
+	if test "${param_spinor_spi_cs}" = "1"; then
+		fdt set /soc/${tmp_spi_path}/spiflash@0 reg "<1>";
+	fi
+	env delete tmp_spi_path
+fi
+
+if test -n "${param_spidev_spi_bus}"; then
+	test "${param_spidev_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c68000"
+	test "${param_spidev_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c69000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spidev status "okay"
+	if test -n "${param_spidev_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spidev spi-max-frequency "<${param_spidev_max_freq}>"
+	fi
+	if test "${param_spidev_spi_cs}" = "1"; then
+		fdt set /soc/${tmp_spi_path}/spidev reg "<1>";
+	fi
+fi
+
+if test -n "${param_pps_pin}"; then
+	setenv tmp_bank "${param_pps_pin}"
+	setenv tmp_pin "${param_pps_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@1c20800/pps_pins pins "${param_pps_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@1c20800 phandle
+	fdt set /pps@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test "${param_pps_falling_edge}" = "1"; then
+	fdt set /pps@0 assert-falling-edge
+fi
+
+if test -n "${param_w1_pin}"; then
+	setenv tmp_bank "${param_w1_pin}"
+	setenv tmp_pin "${param_w1_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@1c20800/w1_pins pins "${param_w1_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@1c20800 phandle
+	fdt set /onewire@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test "${param_w1_pin_int_pullup}" = "1"; then
+	fdt set /soc/pinctrl@1c20800/w1_pins bias-pull-up
+fi
+
+if test "${param_uart1_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart1-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart1-rts-cts-pins phandle
+	fdt set /soc/serial@1c28400 pinctrl-names "default" "default"
+	fdt set /soc/serial@1c28400 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@1c28400 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
+
+if test "${param_uart2_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart2-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart2-rts-cts-pins phandle
+	fdt set /soc/serial@1c28800 pinctrl-names "default" "default"
+	fdt set /soc/serial@1c28800 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@1c28800 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
+
+if test "${param_uart4_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart4-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart4-rts-cts-pins phandle
+	fdt set /soc/serial@1c29000 pinctrl-names "default" "default"
+	fdt set /soc/serial@1c29000 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@1c29000 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-i2c0.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-i2c0.dtso
new file mode 100644
index 000000000000..37bdb2c2fae3
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-i2c0.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-a64";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c0 = "/soc/i2c@1c2ac00";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			i2c0_pins: i2c0_pins {
+				pins = "PH0", "PH1";
+				function = "i2c0";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c0>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c0_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-i2c1.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-i2c1.dtso
new file mode 100644
index 000000000000..b2483c9cd7b2
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-i2c1.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-a64";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c1 = "/soc/i2c@1c2b000";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c1_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-pps-gpio.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-pps-gpio.dtso
new file mode 100644
index 000000000000..5fa161c4718e
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-pps-gpio.dtso
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-a64";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			pps_pins: pps_pins {
+				pins = "PD4";
+				function = "gpio_in";
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			pps@0 {
+				compatible = "pps-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&pps_pins>;
+				gpios = <&pio 3 4 0>; /* PD4 */
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-add-cs1.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-add-cs1.dtso
new file mode 100644
index 000000000000..4432aac51f2e
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-add-cs1.dtso
@@ -0,0 +1,41 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-a64";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			spi0_cs1: spi0_cs1 {
+				pins = "PB6";
+				function = "gpio_out";
+				output-high;
+			};
+
+			spi1_cs1: spi1_cs1 {
+				pins = "PD6";
+				function = "gpio_out";
+				output-high;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			pinctrl-names = "default", "default";
+			pinctrl-1 = <&spi0_cs1>;
+			cs-gpios = <0>, <&pio 1 6 0>; /* PB6 */
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			pinctrl-names = "default", "default";
+			pinctrl-1 = <&spi1_cs1>;
+			cs-gpios = <0>, <&pio 3 6 0>; /* PD6 */
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-jedec-nor.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-jedec-nor.dtso
new file mode 100644
index 000000000000..31d73e572281
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-jedec-nor.dtso
@@ -0,0 +1,34 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-a64";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+				status = "disabled";
+			};
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-spidev.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-spidev.dtso
new file mode 100644
index 000000000000..84a435b79bee
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-spi-spidev.dtso
@@ -0,0 +1,42 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-a64";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc/spi@1c68000";
+			spi1 = "/soc/spi@1c69000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart1.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart1.dtso
new file mode 100644
index 000000000000..4d8dac1a59cb
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart1.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-a64";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial1 = "/soc/serial@1c28800";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart1>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart1_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart2.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart2.dtso
new file mode 100644
index 000000000000..7286d7360df1
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart2.dtso
@@ -0,0 +1,37 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-a64";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial2 = "/soc/serial@1c28800";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart2_pins: uart2-pins {
+				pins = "PB0", "PB1";
+				function = "uart2";
+			};
+
+			uart2_rts_cts_pins: uart2-rts-cts-pins {
+				pins = "PB2", "PB3";
+				function = "uart2";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart2>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart2_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart3.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart3.dtso
new file mode 100644
index 000000000000..c5729b9d2568
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart3.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-a64";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial3 = "/soc/serial@1c28c00";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart3_pins: uart3-pins {
+				pins = "PD0", "PD1";
+				function = "uart3";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart3>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart3_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart4.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart4.dtso
new file mode 100644
index 000000000000..21c9b738aa93
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-uart4.dtso
@@ -0,0 +1,37 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-a64";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial4 = "/soc/serial@1c29000";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart4_pins: uart4-pins {
+				pins = "PD2", "PD3";
+				function = "uart4";
+			};
+
+			uart4_rts_cts_pins: uart4-rts-cts-pins {
+				pins = "PD4", "PD5";
+				function = "uart4";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart4>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart4_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-w1-gpio.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-w1-gpio.dtso
new file mode 100644
index 000000000000..d230469135de
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-a64-w1-gpio.dtso
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-a64";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			w1_pins: w1_pins {
+				pins = "PD4";
+				function = "gpio_in";
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			onewire@0 {
+				compatible = "w1-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&w1_pins>;
+				gpios = <&pio 3 4 0>; /* PD4 */
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-analog-codec.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-analog-codec.dtso
new file mode 100644
index 000000000000..aaa66d5e7ca1
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-analog-codec.dtso
@@ -0,0 +1,17 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target = <&codec>;
+		__overlay__ {
+			allwinner,audio-routing =
+				"Line Out", "LINEOUT",
+				"MIC1", "Mic",
+				"Mic",  "MBIAS";
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-cir.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-cir.dtso
new file mode 100644
index 000000000000..90c264a0ab78
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-cir.dtso
@@ -0,0 +1,15 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target = <&ir>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&r_ir_rx_pin>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-fixup.scr-cmd b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-fixup.scr-cmd
new file mode 100644
index 000000000000..7abb64d84a8a
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-fixup.scr-cmd
@@ -0,0 +1,110 @@
+# overlays fixup script
+# implements (or rather substitutes) overlay arguments functionality
+# using u-boot scripting, environment variables and "fdt" command
+
+# setexpr test_var ${tmp_bank} - A
+# works only for hex numbers (A-F)
+
+setenv decompose_pin 'setexpr tmp_bank sub "P(A|C|D|G)\\d+" "\\1";
+setexpr tmp_pin sub "P\\S(\\d+)" "\\1";
+test "${tmp_bank}" = "A" && setenv tmp_bank 0;
+test "${tmp_bank}" = "C" && setenv tmp_bank 2;
+test "${tmp_bank}" = "D" && setenv tmp_bank 3;
+test "${tmp_bank}" = "G" && setenv tmp_bank 6'
+
+if test -n "${param_spinor_spi_bus}"; then
+	test "${param_spinor_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c68000"
+	test "${param_spinor_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c69000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spiflash@0 status "okay"
+	if test -n "${param_spinor_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spiflash@0 spi-max-frequency "<${param_spinor_max_freq}>"
+	fi
+	if test "${param_spinor_spi_cs}" = "1"; then
+		fdt set /soc/${tmp_spi_path}/spiflash@0 reg "<1>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test -n "${param_spidev_spi_bus}"; then
+	test "${param_spidev_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c68000"
+	test "${param_spidev_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c69000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spidev status "okay"
+	if test -n "${param_spidev_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spidev spi-max-frequency "<${param_spidev_max_freq}>"
+	fi
+	if test "${param_spidev_spi_cs}" = "1"; then
+		fdt set /soc/${tmp_spi_path}/spidev reg "<1>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test -n "${param_pps_pin}"; then
+	setenv tmp_bank "${param_pps_pin}"
+	setenv tmp_pin "${param_pps_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@1c20800/pps_pins pins "${param_pps_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@1c20800 phandle
+	fdt set /pps@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test "${param_pps_falling_edge}" = "1"; then
+	fdt set /pps@0 assert-falling-edge
+fi
+
+for f in ${overlays}; do
+	if test "${f}" = "pwm"; then
+		setenv bootargs_new ""
+		for arg in ${bootargs}; do
+			if test "${arg}" = "console=ttyS0,115200"; then
+				echo "Warning: Disabling ttyS0 console due to enabled PWM overlay"
+			else
+				setenv bootargs_new "${bootargs_new} ${arg}"
+			fi
+		done
+		setenv bootargs "${bootargs_new}"
+	fi
+done
+
+if test -n "${param_w1_pin}"; then
+	setenv tmp_bank "${param_w1_pin}"
+	setenv tmp_pin "${param_w1_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@1c20800/w1_pins pins "${param_w1_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@1c20800 phandle
+	fdt set /onewire@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test "${param_w1_pin_int_pullup}" = "1"; then
+	fdt set /soc/pinctrl@1c20800/w1_pins bias-pull-up
+fi
+
+if test "${param_uart1_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart1-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart1-rts-cts-pins phandle
+	fdt set /soc/serial@1c28400 pinctrl-names "default" "default"
+	fdt set /soc/serial@1c28400 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@1c28400 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
+
+if test "${param_uart2_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart2-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart2-rts-cts-pins phandle
+	fdt set /soc/serial@1c28800 pinctrl-names "default" "default"
+	fdt set /soc/serial@1c28800 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@1c28800 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
+
+if test "${param_uart3_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart3-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart3-rts-cts-pins phandle
+	fdt set /soc/serial@1c28c00 pinctrl-names "default" "default"
+	fdt set /soc/serial@1c28c00 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@1c28c00 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c0.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c0.dtso
new file mode 100644
index 000000000000..87fbd7e51a11
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c0.dtso
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c0 = "/soc/i2c@1c2ac00";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c1.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c1.dtso
new file mode 100644
index 000000000000..6008b9a0853e
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c1.dtso
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c1 = "/soc/i2c@1c2b000";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c2.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c2.dtso
new file mode 100644
index 000000000000..2980dbf34300
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-i2c2.dtso
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c2 = "/soc/i2c@1c2b400";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c2>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-pps-gpio.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-pps-gpio.dtso
new file mode 100644
index 000000000000..46e067562e3d
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-pps-gpio.dtso
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			pps_pins: pps_pins {
+				pins = "PD14";
+				function = "gpio_in";
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			pps@0 {
+				compatible = "pps-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&pps_pins>;
+				gpios = <&pio 3 14 0>; /* PD14 */
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-pwm.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-pwm.dtso
new file mode 100644
index 000000000000..6d12e8420de9
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-pwm.dtso
@@ -0,0 +1,39 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target-path = "/chosen";
+		__overlay__ {
+			/delete-property/ stdout-path;
+		};
+	};
+
+	fragment@1 {
+		target = <&uart0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&pio>;
+		__overlay__ {
+			pwm0_pin: pwm0 {
+				pins = "PA5";
+				function = "pwm0";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&pwm>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&pwm0_pin>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spdif-out.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spdif-out.dtso
new file mode 100644
index 000000000000..65bc51b0218e
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spdif-out.dtso
@@ -0,0 +1,38 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target = <&spdif>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&spdif_tx_pin>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			sound {
+				compatible = "simple-audio-card";
+				simple-audio-card,name = "On-board SPDIF";
+
+				simple-audio-card,cpu {
+					sound-dai = <&spdif>;
+				};
+
+				simple-audio-card,codec {
+					sound-dai = <&spdif_out>;
+				};
+			};
+
+			spdif_out: spdif-out {
+				#sound-dai-cells = <0>;
+				compatible = "linux,spdif-dit";
+			};
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-add-cs1.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-add-cs1.dtso
new file mode 100644
index 000000000000..8e3eab295f49
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-add-cs1.dtso
@@ -0,0 +1,41 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			spi0_cs1: spi0_cs1 {
+				pins = "PA21";
+				function = "gpio_out";
+				output-high;
+			};
+
+			spi1_cs1: spi1_cs1 {
+				pins = "PA10";
+				function = "gpio_out";
+				output-high;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			pinctrl-names = "default", "default";
+			pinctrl-1 = <&spi0_cs1>;
+			cs-gpios = <0>, <&pio 0 21 0>; /* PA21 */
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			pinctrl-names = "default", "default";
+			pinctrl-1 = <&spi1_cs1>;
+			cs-gpios = <0>, <&pio 0 10 0>; /* PA10 */
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-jedec-nor.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-jedec-nor.dtso
new file mode 100644
index 000000000000..5a45808c11a5
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-jedec-nor.dtso
@@ -0,0 +1,42 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc/spi@1c68000";
+			spi1 = "/soc/spi@1c69000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+				status = "disabled";
+			};
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-spidev.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-spidev.dtso
new file mode 100644
index 000000000000..69a14b2c60e4
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-spi-spidev.dtso
@@ -0,0 +1,42 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc/spi@1c68000";
+			spi1 = "/soc/spi@1c69000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart1.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart1.dtso
new file mode 100644
index 000000000000..92e3eb4d9b66
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart1.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial1 = "/soc/serial@1c28400";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart1>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart1_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart2.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart2.dtso
new file mode 100644
index 000000000000..92bee1a9600a
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart2.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial2 = "/soc/serial@1c28800";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart2_rts_cts: uart2-rts-cts-pins {
+				pins = "PA2", "PA3";
+				function = "uart2";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart2>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart2_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart3.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart3.dtso
new file mode 100644
index 000000000000..a2197f1668fb
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-uart3.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial3 = "/soc/serial@1c28c00";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart3_rts_cts: uart3-rts-cts-pins {
+				pins = "PA15", "PA16";
+				function = "uart3";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart3>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart3_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost0.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost0.dtso
new file mode 100644
index 000000000000..c1d79c232fa4
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost0.dtso
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target = <&ehci0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&ohci0>;
+		 __overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&usbphy>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost1.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost1.dtso
new file mode 100644
index 000000000000..2b4f245bf297
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost1.dtso
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target = <&ehci1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&ohci1>;
+		 __overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&usbphy>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost2.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost2.dtso
new file mode 100644
index 000000000000..54800e729538
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost2.dtso
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target = <&ehci2>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&ohci2>;
+		 __overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&usbphy>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost3.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost3.dtso
new file mode 100644
index 000000000000..a99524ea38f3
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-usbhost3.dtso
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target = <&ehci3>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&ohci3>;
+		 __overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&usbphy>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-w1-gpio.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-w1-gpio.dtso
new file mode 100644
index 000000000000..6e99626ac660
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h5-w1-gpio.dtso
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h5";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			w1_pins: w1_pins {
+				pins = "PD14";
+				function = "gpio_in";
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			onewire@0 {
+				compatible = "w1-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&w1_pins>;
+				gpios = <&pio 3 14 0>; /* PD14 */
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-fixup.scr-cmd b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-fixup.scr-cmd
new file mode 100644
index 000000000000..d8e79ba4531b
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-fixup.scr-cmd
@@ -0,0 +1,110 @@
+# overlays fixup script
+# implements (or rather substitutes) overlay arguments functionality
+# using u-boot scripting, environment variables and "fdt" command
+
+# setexpr test_var ${tmp_bank} - A
+# works only for hex numbers (A-F)
+
+setenv decompose_pin 'setexpr tmp_bank sub "P(A|C|D|G)\\d+" "\\1";
+setexpr tmp_pin sub "P\\S(\\d+)" "\\1";
+test "${tmp_bank}" = "A" && setenv tmp_bank 0;
+test "${tmp_bank}" = "C" && setenv tmp_bank 2;
+test "${tmp_bank}" = "D" && setenv tmp_bank 3;
+test "${tmp_bank}" = "G" && setenv tmp_bank 6'
+
+if test -n "${param_spinor_spi_bus}"; then
+	test "${param_spinor_spi_bus}" = "0" && setenv tmp_spi_path "spi@5010000"
+	test "${param_spinor_spi_bus}" = "1" && setenv tmp_spi_path "spi@5011000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spiflash@0 status "okay"
+	if test -n "${param_spinor_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spiflash@0 spi-max-frequency "<${param_spinor_max_freq}>"
+	fi
+	if test "${param_spinor_spi_cs}" = "1"; then
+		fdt set /soc/${tmp_spi_path}/spiflash@0 reg "<1>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test -n "${param_spidev_spi_bus}"; then
+	test "${param_spidev_spi_bus}" = "0" && setenv tmp_spi_path "spi@5010000"
+	test "${param_spidev_spi_bus}" = "1" && setenv tmp_spi_path "spi@5011000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spidev status "okay"
+	if test -n "${param_spidev_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spidev spi-max-frequency "<${param_spidev_max_freq}>"
+	fi
+	if test "${param_spidev_spi_cs}" = "1"; then
+		fdt set /soc/${tmp_spi_path}/spidev reg "<1>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test -n "${param_pps_pin}"; then
+	setenv tmp_bank "${param_pps_pin}"
+	setenv tmp_pin "${param_pps_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@300b000/pps_pins pins "${param_pps_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@300b000 phandle
+	fdt set /pps@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test "${param_pps_falling_edge}" = "1"; then
+	fdt set /pps@0 assert-falling-edge
+fi
+
+for f in ${overlays}; do
+	if test "${f}" = "pwm"; then
+		setenv bootargs_new ""
+		for arg in ${bootargs}; do
+			if test "${arg}" = "console=ttyS0,115200"; then
+				echo "Warning: Disabling ttyS0 console due to enabled PWM overlay"
+			else
+				setenv bootargs_new "${bootargs_new} ${arg}"
+			fi
+		done
+		setenv bootargs "${bootargs_new}"
+	fi
+done
+
+if test -n "${param_w1_pin}"; then
+	setenv tmp_bank "${param_w1_pin}"
+	setenv tmp_pin "${param_w1_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@300b000/w1_pins pins "${param_w1_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@300b000 phandle
+	fdt set /onewire@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test "${param_w1_pin_int_pullup}" = "1"; then
+	fdt set /soc/pinctrl@300b000/w1_pins bias-pull-up
+fi
+
+if test "${param_uart1_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@300b000/uart1-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@300b000/uart1-rts-cts-pins phandle
+	fdt set /soc/serial@5000400 pinctrl-names "default" "default"
+	fdt set /soc/serial@5000400 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@5000400 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
+
+if test "${param_uart2_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@300b000/uart2-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@300b000/uart2-rts-cts-pins phandle
+	fdt set /soc/serial@5000800 pinctrl-names "default" "default"
+	fdt set /soc/serial@5000800 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@5000800 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
+
+if test "${param_uart3_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@300b000/uart3-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@300b000/uart3-rts-cts-pins phandle
+	fdt set /soc/serial@5000c00 pinctrl-names "default" "default"
+	fdt set /soc/serial@5000c00 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@5000c00 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c0.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c0.dtso
new file mode 100644
index 000000000000..7e7ee8c46e9c
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c0.dtso
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h6";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c0 = "/soc/i2c@5002000";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c1.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c1.dtso
new file mode 100644
index 000000000000..111769821262
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c1.dtso
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h6";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c1 = "/soc/i2c@5002400";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c2.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c2.dtso
new file mode 100644
index 000000000000..b627529c2144
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-i2c2.dtso
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h6";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c2 = "/soc/i2c@5002800";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c2>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-ruart.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-ruart.dtso
new file mode 100644
index 000000000000..6430cb083370
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-ruart.dtso
@@ -0,0 +1,13 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h6";
+
+	fragment@0 {
+		target = <&r_uart>;
+		 __overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-add-cs1.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-add-cs1.dtso
new file mode 100644
index 000000000000..0fa060fa1eff
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-add-cs1.dtso
@@ -0,0 +1,41 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h6";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			spi0_cs1: spi0_cs1 {
+				pins = "PA10";
+				function = "gpio_out";
+				output-high;
+			};
+
+			spi1_cs1: spi1_cs1 {
+				pins = "PA21";
+				function = "gpio_out";
+				output-high;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			pinctrl-names = "default", "default";
+			pinctrl-1 = <&spi0_cs1>;
+			cs-gpios = <0>, <&pio 0 10 0>; /* PA10 */
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			pinctrl-names = "default", "default";
+			pinctrl-1 = <&spi1_cs1>;
+			cs-gpios = <0>, <&pio 0 21 0>; /* PA21 */
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-jedec-nor.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-jedec-nor.dtso
new file mode 100644
index 000000000000..4f81dbb9924c
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-jedec-nor.dtso
@@ -0,0 +1,42 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h6";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc/spi@5010000";
+			spi1 = "/soc/spi@5011000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+				status = "disabled";
+			};
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-spidev.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-spidev.dtso
new file mode 100644
index 000000000000..1f077ea80ae5
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-spidev.dtso
@@ -0,0 +1,42 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3-spi";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc/spi@5010000";
+			spi1 = "/soc/spi@5011000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-spidev1.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-spidev1.dtso
new file mode 100644
index 000000000000..5e6b70530fae
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-spi-spidev1.dtso
@@ -0,0 +1,30 @@
+// Enable the spidev interface
+/dts-v1/;
+/plugin/;
+
+/ {
+    compatible = "allwinner,sun8i-h3-spi";
+
+    fragment@0 {
+	target-path = "/aliases";
+	__overlay__ {
+            /* Path to the SPI controller nodes */
+            spi1 = "/soc/spi@5011000";
+        };
+    };
+    fragment@1 {
+        target = <&spi1>;
+        __overlay__ {
+            pinctrl-names = "default";
+            pinctrl-0 = <&spi1_pins>;
+            status = "okay";
+            #address-cells = <1>;
+            #size-cells = <0>;
+            spidev@0 {
+                compatible = "armbian,spi-dev";
+                reg = <0x0>;
+                spi-max-frequency = <1000000>;
+            };
+        };
+    };
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart1.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart1.dtso
new file mode 100644
index 000000000000..44aa94efdad1
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart1.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h6";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial1 = "/soc/serial@5000400";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart1>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart1_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart2.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart2.dtso
new file mode 100644
index 000000000000..bf9174bcd2e6
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart2.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h6";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial2 = "/soc/serial@5000800";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart2_rts_cts: uart2-rts-cts-pins {
+				pins = "PD21", "PD22";
+				function = "uart2";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart2>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart2_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart3.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart3.dtso
new file mode 100644
index 000000000000..418edc14a0e4
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-uart3.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h6";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial3 = "/soc/serial@5000c00";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart3_rts_cts: uart3-rts-cts-pins {
+				pins = "PD25", "PD26";
+				function = "uart3";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart3>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart3_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-w1-gpio.dtso b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-w1-gpio.dtso
new file mode 100644
index 000000000000..3043c87780e4
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/overlay/sun50i-h6-w1-gpio.dtso
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun50i-h6";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			w1_pins: w1_pins {
+				pins = "PC9";
+				function = "gpio_in";
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			onewire@0 {
+				compatible = "w1-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&w1_pins>;
+				gpios = <&pio 2 9 0>; /* PC9 */
+				status = "okay";
+			};
+		};
+	};
+};
-- 
2.35.3

