From ed8e79073bb141a1f5a5b5f2b891e3c9be8079c8 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megi@xff.cz>
Date: Tue, 14 May 2024 10:47:05 +0200
Subject: arm64: dts: sun50-a64-pinephone: Define jack pins in DT

To restore pre v6.8 behavior of the sound card.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
index f0f1367c5868..d502c1392b8e 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
@@ -999,6 +999,10 @@ &sound {
 			"MIC1", "Internal Microphone",
 			"Headset Microphone", "HBIAS",
 			"MIC2", "Headset Microphone";
+	simple-audio-card,jack-pins =
+			"1c22e00.codec", "Headphone Jack",
+			"1c22e00.codec", "Headset Microphone";
+	simple-audio-card,jack-pins-mask = <1>, <2>;
 
 	simple-audio-card,dai-link@1 {
 		format = "dsp_a";
-- 
2.35.3

