From 02cd44cdcb83d7b3b4adb5908fa184cfb60a67e1 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Sun, 23 Feb 2020 00:00:00 +0100
Subject: dt-bindings: input: gpio-vibrator: Don't require enable-gpios

It is possible to turn the motor on/off just by enabling/disabling
the vcc-supply. Change the binding to require either enable-gpios
or vcc-supply or both.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 Documentation/devicetree/bindings/input/gpio-vibrator.yaml | 7 ++++++-
 1 file changed, 6 insertions(+), 1 deletion(-)

diff --git a/Documentation/devicetree/bindings/input/gpio-vibrator.yaml b/Documentation/devicetree/bindings/input/gpio-vibrator.yaml
index 2384465eaa19..082ac06471db 100644
--- a/Documentation/devicetree/bindings/input/gpio-vibrator.yaml
+++ b/Documentation/devicetree/bindings/input/gpio-vibrator.yaml
@@ -24,7 +24,12 @@ properties:
 
 required:
   - compatible
-  - enable-gpios
+
+anyOf:
+  - required:
+    - enable-gpios
+  - required:
+    - vcc-supply
 
 additionalProperties: false
 
-- 
2.35.3

