From 6f7050f399283cdef2e0a1598a41279fb1d2ab01 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Tue, 14 Nov 2017 02:47:51 +0100
Subject: ARM: dts: axp813: Add charger LED

PMIC supports charging status indication via a LED. Add support
for it.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm/boot/dts/allwinner/axp81x.dtsi | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/axp81x.dtsi b/arch/arm/boot/dts/allwinner/axp81x.dtsi
index ebaf1c3ce8db..a4b1be159b02 100644
--- a/arch/arm/boot/dts/allwinner/axp81x.dtsi
+++ b/arch/arm/boot/dts/allwinner/axp81x.dtsi
@@ -161,4 +161,9 @@ reg_drivevbus: drivevbus {
 	usb_power_supply: usb-power {
 		compatible = "x-powers,axp813-usb-power-supply";
 	};
+
+	charger_led: charger-led {
+		compatible = "x-powers,axp813-charger-led";
+		status = "disabled";
+	};
 };
-- 
2.35.3

