From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Mitko Gamishev <hehopmajieh@debian.bg>
Date: Wed, 5 Feb 2020 15:00:25 +0200
Subject: arm:dts:sun5i-a13-olinuxino-micro add panel lcd-olinuxino-4.3

---
 arch/arm/boot/dts/allwinner/sun5i-a13-olinuxino-micro.dts | 62 +++++++++-
 1 file changed, 60 insertions(+), 2 deletions(-)

diff --git a/arch/arm/boot/dts/allwinner/sun5i-a13-olinuxino-micro.dts b/arch/arm/boot/dts/allwinner/sun5i-a13-olinuxino-micro.dts
index 111111111111..222222222222 100644
--- a/arch/arm/boot/dts/allwinner/sun5i-a13-olinuxino-micro.dts
+++ b/arch/arm/boot/dts/allwinner/sun5i-a13-olinuxino-micro.dts
@@ -44,7 +44,7 @@
 /dts-v1/;
 #include "sun5i-a13.dtsi"
 #include "sunxi-common-regulators.dtsi"
-
+#include <dt-bindings/pwm/pwm.h>
 #include <dt-bindings/gpio/gpio.h>
 
 / {
@@ -70,6 +70,40 @@ led {
 			default-state = "on";
 		};
 	};
+
+	 backlight: backlight {
+		compatible = "pwm-backlight";
+		pwms = <&pwm 0 50000 PWM_POLARITY_INVERTED>;
+                brightness-levels = <0 10 20 30 40 50 60 70 80 90 100>;
+                default-brightness-level = <8>;
+
+        };
+
+	 panel: panel {
+                compatible = "olimex,lcd-olinuxino-4.3";
+                backlight = <&backlight>;
+		enable-gpios = <&pio 1 10 GPIO_ACTIVE_HIGH>; /* PB10 */
+		pinctrl-names = "default";
+                #address-cells = <1>;
+                #size-cells = <0>;
+		port {
+			panel_input: endpoint {
+				remote-endpoint = <&tcon0_out_lcd>;
+			};
+		};
+
+                };
+
+	};
+
+
+
+&be0 {
+	status = "okay";
+};
+
+&codec {
+	status = "okay";
 };
 
 &ehci0 {
@@ -117,10 +151,28 @@ &reg_usb0_vbus {
 };
 
 &reg_usb1_vbus {
-	gpio = <&pio 6 11 GPIO_ACTIVE_HIGH>;
+	gpio = <&pio 2 19 GPIO_ACTIVE_HIGH>;
 	status = "okay";
 };
 
+&tcon0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&lcd_rgb666_pins>;
+	status = "okay";
+};
+&tcon0_out {
+	tcon0_out_lcd: endpoint@0 {
+		reg = <0>;
+		remote-endpoint = <&panel_input>;
+	};
+};
+
+&pwm {
+        pinctrl-names = "default";
+        pinctrl-0 = <&pwm0_pin>;
+        status = "okay";
+};
+
 &uart1 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart1_pg_pins>;
@@ -139,3 +191,9 @@ &usbphy {
 	usb1_vbus-supply = <&reg_usb1_vbus>;
 	status = "okay";
 };
+
+&rtp {
+	allwinner,ts-attached;
+	touchscreen-inverted-x;
+};
+
-- 
Armbian

