From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Stefan Saraev <stefan@saraev.ca>
Date: Fri, 20 Mar 2020 17:31:49 +0200
Subject: arm64:dts: sun50i-a64-olinuxino-1Ge16GW: enable bluetooth

---
 arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino-1Ge16GW.dts | 21 ++++++++++
 1 file changed, 21 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino-1Ge16GW.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino-1Ge16GW.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino-1Ge16GW.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino-1Ge16GW.dts
@@ -18,3 +18,24 @@ &mmc2 {
 	mmc-hs200-1_8v;
 	allwinner,drive-data-phase = <180>;
 };
+
+&pio {
+	vcc-pc-supply = <&reg_eldo1>;
+	uart1_cts_pins: uart1_cts_pins {
+		pins = "PG8";
+		function = "uart1";
+	};
+};
+
+&uart1 {
+        pinctrl-names = "default";
+        pinctrl-0 = <&uart1_pins>, <&uart1_cts_pins>;
+        status = "okay";
+        bluetooth {
+                compatible = "realtek,rtl8723bs-bt";
+                reset-gpios = <&r_pio 0 4 GPIO_ACTIVE_LOW>; /* PL4 */
+                device-wake-gpios = <&r_pio 0 5 GPIO_ACTIVE_HIGH>; /* PL5 */
+                host-wake-gpios = <&r_pio 0 6 GPIO_ACTIVE_HIGH>; /* PL6 */
+                firmware-postfix = "olinuxino";
+        };
+};
-- 
Armbian

