From ae50dd46d3bacea389ffb447aefcf4e7cd2f3fe8 Mon Sep 17 00:00:00 2001
From: Alan <Alan>
Date: Fri, 19 May 2023 17:14:25 +0800
Subject: [PATCH 08/11] Fix: boot from MMC2(eMMC), mmc_Load_image_raw_sector:
 mmc block read error

---
 drivers/mmc/sunxi_mmc.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/mmc/sunxi_mmc.c b/drivers/mmc/sunxi_mmc.c
index 23bc7da917..c500716ee5 100644
--- a/drivers/mmc/sunxi_mmc.c
+++ b/drivers/mmc/sunxi_mmc.c
@@ -536,7 +536,7 @@ struct mmc *sunxi_mmc_init(int sdc_no)
 	cfg->b_max = CONFIG_SYS_MMC_MAX_BLK_COUNT;
 
 	cfg->f_min = 400000;
-	cfg->f_max = 52000000;
+	cfg->f_max = 20000000;
 
 	if (mmc_resource_init(sdc_no) != 0)
 		return NULL;
-- 
2.34.1

