From 3388c7e4f1d60f11b0377cfe30d0bfaaa20183ba Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Tue, 23 Jun 2020 19:15:37 +0200
Subject: ARM: dts: sun8i-a83t-tbs-a711: Add regulators to the accelerometer

The bosch,bma250 driver will fail to probe if the regulators are
not specified in DT, because it tries to set voltage on dummy
regulators, which fails with EINVAL.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts | 2 ++
 1 file changed, 2 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
index 925891a1d6d9..ce1a8d98b548 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
@@ -268,6 +268,8 @@ accelerometer@18 {
 		reg = <0x18>;
 		interrupt-parent = <&pio>;
 		interrupts = <7 10 IRQ_TYPE_EDGE_RISING>; /* PH10 / EINT10 */
+		vdd-supply = <&reg_dcdc1>;
+		vddio-supply = <&reg_dcdc1>;
 	};
 
 	/* NFC (NPC 100) */
-- 
2.35.3

