From eff7988fc46688c551cb1d18bef171cf3243905d Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Mon, 20 Jul 2020 01:11:34 +0800
Subject: arm64: allwinner: dts: a64: enable K101-IM2BYL02 panel for PineTab

Newer PineTab may switch to K101-IM2BYL02.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts | 8 +++-----
 1 file changed, 3 insertions(+), 5 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
index 50a0e1916743..6056c965baf6 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinetab.dts
@@ -200,12 +200,10 @@ &dsi {
 	status = "okay";
 
 	panel@0 {
-		compatible = "feixin,k101-im2ba02";
+		compatible = "feixin,k101-im2byl02";
 		reg = <0>;
-		avdd-supply = <&reg_dc1sw>;
-		dvdd-supply = <&reg_dc1sw>;
-		cvdd-supply = <&reg_ldo_io1>;
-		reset-gpios = <&pio 3 24 GPIO_ACTIVE_HIGH>; /* PD24 */
+		power-supply = <&reg_dc1sw>;
+		reset-gpios = <&pio 3 24 GPIO_ACTIVE_LOW>; /* PD24 */
 		backlight = <&backlight>;
 	};
 };
-- 
2.35.3

