From 44da59a4153403368ef6f295e3ff1b0b3868e90a Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Micha=C5=82=20Dzieko=C5=84ski?=
 <michal.dziekonski+github@gmail.com>
Date: Sun, 28 May 2023 00:26:43 +0000
Subject: arm64: dts: allwinner: h616 orangepi zero2: Enable expansion board
 USB ports

Signed-off-by: Michal Dziekonski <michal.dziekonski+github@gmail.com>
---
 .../dts/allwinner/sun50i-h616-orangepi-zero.dtsi  | 15 +++++++++++++++
 1 file changed, 15 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi
index b5548923b7c4..8860844a4a79 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi
@@ -72,6 +72,13 @@ &ehci1 {
 };
 
 /* USB 2 & 3 are on headers only. */
+&ehci2 {
+	status = "okay";
+};
+
+&ehci3 {
+	status = "okay";
+};
 
 &emac0 {
 	pinctrl-names = "default";
@@ -98,6 +105,14 @@ &ohci1 {
 	status = "okay";
 };
 
+&ohci2 {
+	status = "okay";
+};
+
+&ohci3 {
+	status = "okay";
+};
+
 &spi0  {
 	status = "okay";
 	pinctrl-names = "default";
-- 
2.35.3

