From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Ryzer58 <ryestar101@gmail.com>
Date: Sat, 30 Nov 2024 20:40:29 +0000
Subject: Correct perf interrupt source number as referenced in the Allwinner
 A10 User manual

to resolve conflict with UART2.

Signed-off-by: Ryzer58 <ryestar101@gmail.com>
---
 arch/arm/boot/dts/allwinner/sun4i-a10.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm/boot/dts/allwinner/sun4i-a10.dtsi b/arch/arm/boot/dts/allwinner/sun4i-a10.dtsi
index 111111111111..222222222222 100644
--- a/arch/arm/boot/dts/allwinner/sun4i-a10.dtsi
+++ b/arch/arm/boot/dts/allwinner/sun4i-a10.dtsi
@@ -185,7 +185,7 @@ de: display-engine {
 
 	pmu {
 		compatible = "arm,cortex-a8-pmu";
-		interrupts = <3>;
+		interrupts = <66>;
 	};
 
 	reserved-memory {
-- 
Armbian

