From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Lemon1151 <smile1151@foxmail.com>
Date: Mon, 3 Jun 2024 12:32:02 +0200
Subject: Adding support for the fine3399 board

> X-Git-Archeology: - Revision 8f64f0508237888dd326018fa9a392346b8ec5ab: https://github.com/armbian/build/commit/8f64f0508237888dd326018fa9a392346b8ec5ab
> X-Git-Archeology:   Date: Mon, 03 Jun 2024 12:32:02 +0200
> X-Git-Archeology:   From: Lemon1151 <smile1151@foxmail.com>
> X-Git-Archeology:   Subject: Adding support for the fine3399 board
---
 arch/arm64/boot/dts/rockchip/rk3399-fine3399.dts | 870 ++++++++++
 1 file changed, 870 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3399-fine3399.dts b/arch/arm64/boot/dts/rockchip/rk3399-fine3399.dts
new file mode 100644
index 000000000000..111111111111
--- /dev/null
+++ b/arch/arm64/boot/dts/rockchip/rk3399-fine3399.dts
@@ -0,0 +1,870 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+
+/dts-v1/;
+#include <dt-bindings/input/linux-event-codes.h>
+#include <dt-bindings/pwm/pwm.h>
+#include <dt-bindings/input/input.h>
+#include "rk3399.dtsi"
+
+
+/ {
+	model = "Rockchip Fine3399";
+	compatible = "rockchip,fine3399", "rockchip,rk3399";
+
+	aliases {
+		mmc0 = &sdio0;
+		mmc1 = &sdmmc;
+		mmc2 = &sdhci;
+	};
+
+	chosen {
+		stdout-path = "serial2:1500000n8";
+	};
+
+	clkin_gmac: external-gmac-clock {
+		compatible = "fixed-clock";
+		clock-frequency = <125000000>;
+		clock-output-names = "clkin_gmac";
+		#clock-cells = <0>;
+	};
+
+	dc_12v: dc-12v {
+		compatible = "regulator-fixed";
+		regulator-name = "dc_12v";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <12000000>;
+		regulator-max-microvolt = <12000000>;
+	};
+
+	sdio_pwrseq: sdio-pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		clocks = <&rk808 1>;
+		clock-names = "ext_clock";
+		pinctrl-names = "default";
+		pinctrl-0 = <&wifi_reg_on_h>;
+		reset-gpios = <&gpio0 RK_PB2 GPIO_ACTIVE_LOW>; // bsp
+	};
+
+	/* switched by pmic_sleep */
+	vcc1v8_s3: vcca1v8_s3: vcc1v8-s3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc1v8_s3";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		vin-supply = <&vcc_1v8>;
+	};
+
+	vcc3v3_sys: vcc3v3_pcie: vcc3v3_bl: vcc3v3-sys { // sch
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3_sys";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		vin-supply = <&dc_12v>;
+	};
+
+	vcc_sys: vcc-sys { // sch
+		compatible = "regulator-fixed";
+		regulator-name = "vcc_sys";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		vin-supply = <&dc_12v>;
+	};
+
+	vcc_phy: vcc-phy-regulator {
+		compatible = "regulator-fixed";
+		enable-active-high;
+		gpio = <&gpio0 RK_PB4 GPIO_ACTIVE_HIGH>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&vcc_phy_h>;
+		regulator-name = "vcc_phy";
+		regulator-always-on;
+		regulator-boot-on;
+	};
+
+	vdd_log: vdd-log {
+		compatible = "pwm-regulator";
+		pwms = <&pwm2 0 25000 1>;
+		regulator-name = "vdd_log";
+		regulator-always-on;
+		regulator-boot-on;
+		regulator-min-microvolt = <800000>;
+		regulator-max-microvolt = <1400000>;
+		vin-supply = <&vcc_sys>;
+	};
+
+	leds: gpio-leds {
+		compatible = "gpio-leds";
+		pinctrl-names = "default";
+		pinctrl-0 = <&user_led2>;
+
+		user_led2 {
+			label = "blue:work_led";
+			gpios = <&gpio2 RK_PD3 GPIO_ACTIVE_LOW>; // sch
+			linux,default-trigger = "heartbeat";
+		};
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		autorepeat;
+		pinctrl-names = "default";
+		pinctrl-0 = <&power_key>;
+
+		power {
+			debounce-interval = <100>;
+			gpios = <&gpio0 RK_PA5 GPIO_ACTIVE_LOW>; // bsp
+			label = "GPIO Key Power";
+			linux,code = <KEY_POWER>;
+			wakeup-source;
+		};
+	};
+
+	fan0: pwm-fan {
+		compatible = "pwm-fan";
+		cooling-levels = <0 30 60 90 120 160>;
+		#cooling-cells = <2>;
+		fan-supply = <&vcc_sys>;
+		pwms = <&pwm1 0 40000 0>;
+	};
+
+	// pwm3
+	ir-receiver {
+		compatible = "gpio-ir-receiver";
+		gpios = <&gpio0 RK_PA6 GPIO_ACTIVE_LOW>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&ir_int>;
+	};
+
+	adc-keys {
+		compatible = "adc-keys";
+		io-channels = <&saradc 1>;
+		io-channel-names = "buttons";
+		keyup-threshold-microvolt = <1750000>;
+		poll-interval = <100>;
+
+		recovery {
+			label = "Recovery";
+			linux,code = <KEY_VENDOR>; // ??
+			press-threshold-microvolt = <0>;
+		};
+	};
+
+	backlight: backlight {
+		compatible = "pwm-backlight";
+		brightness-levels = <0 4 8 16 32 64 128 255>;
+		default-brightness-level = <5>;
+		pwms = <&pwm0 0 1000000 0>;
+		status = "okay";
+	};
+
+};
+
+&cpu_l0 {
+	cpu-supply = <&vdd_cpu_l>;
+};
+
+&cpu_l1 {
+	cpu-supply = <&vdd_cpu_l>;
+};
+
+&cpu_l2 {
+	cpu-supply = <&vdd_cpu_l>;
+};
+
+&cpu_l3 {
+	cpu-supply = <&vdd_cpu_l>;
+};
+
+&cpu_b0 {
+	cpu-supply = <&vdd_cpu_b>;
+};
+
+&cpu_b1 {
+	cpu-supply = <&vdd_cpu_b>;
+};
+
+&gpu {
+	mali-supply = <&vdd_gpu>;
+	status = "okay";
+};
+
+&cpu_thermal {
+	trips {
+		cpu_warm: cpu_warm {
+			temperature = <50000>;
+			hysteresis = <2000>;
+			type = "active";
+		};
+
+		cpu_hot: cpu_hot {
+			temperature = <65000>;
+			hysteresis = <2000>;
+			type = "active";
+		};
+	};
+
+	cooling-maps {
+		map2 {
+			trip = <&cpu_warm>;
+			cooling-device = <&fan0 THERMAL_NO_LIMIT 1>;
+		};
+
+		map3 {
+			trip = <&cpu_hot>;
+			cooling-device = <&fan0 4 THERMAL_NO_LIMIT>;
+		};
+	};
+};
+
+&emmc_phy {
+	status = "okay";
+};
+
+&gmac {
+	assigned-clocks = <&cru SCLK_RMII_SRC>;
+	assigned-clock-parents = <&clkin_gmac>;
+	clock_in_out = "input";
+	phy-supply = <&vcc_phy>;
+	phy-mode = "rgmii";
+	pinctrl-names = "default";
+	pinctrl-0 = <&rgmii_pins>;
+	snps,reset-gpio = <&gpio3 RK_PB7 GPIO_ACTIVE_LOW>; // bsp
+	snps,reset-active-low;
+	snps,reset-delays-us = <0 10000 50000>;
+	tx_delay = <0x28>;
+	rx_delay = <0x11>;
+	status = "okay";
+};
+
+&gpu {
+	mali-supply = <&vdd_gpu>;
+	status = "okay";
+};
+
+&gpu_thermal {
+	trips {
+		gpu_warm: gpu_warm {
+			temperature = <50000>;
+			hysteresis = <2000>;
+			type = "active";
+		};
+
+		gpu_hot: gpu_hot {
+			temperature = <65000>;
+			hysteresis = <2000>;
+			type = "active";
+		};
+	};
+
+	cooling-maps {
+		map1 {
+			trip = <&gpu_warm>;
+			cooling-device = <&fan0 THERMAL_NO_LIMIT 1>;
+		};
+
+		map2 {
+			trip = <&gpu_hot>;
+			cooling-device = <&fan0 4 THERMAL_NO_LIMIT>;
+		};
+	};
+};
+
+&hdmi {
+	ddc-i2c-bus = <&i2c3>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&hdmi_cec>;
+	status = "okay";
+};
+
+&hdmi_sound {
+	status = "okay";
+};
+
+&i2c0 {
+	clock-frequency = <400000>;
+	i2c-scl-rising-time-ns = <168>;
+	i2c-scl-falling-time-ns = <4>;
+	status = "okay";
+
+	rk808: pmic@1b {
+		compatible = "rockchip,rk808";
+		reg = <0x1b>;
+		interrupt-parent = <&gpio1>;
+		interrupts = <RK_PC5 IRQ_TYPE_LEVEL_LOW>;
+		#clock-cells = <1>;
+		clock-output-names = "xin32k", "rk808-clkout2";
+		pinctrl-names = "default";
+		pinctrl-0 = <&pmic_int_l &pmic_dvs2>;
+		system-power-controller;
+		wakeup-source;
+
+		vcc1-supply = <&vcc3v3_sys>;
+		vcc2-supply = <&vcc3v3_sys>;
+		vcc3-supply = <&vcc3v3_sys>;
+		vcc4-supply = <&vcc3v3_sys>;
+		vcc6-supply = <&vcc3v3_sys>;
+		vcc7-supply = <&vcc3v3_sys>;
+		vcc8-supply = <&vcc3v3_sys>;
+		vcc9-supply = <&vcc3v3_sys>;
+		vcc10-supply = <&vcc3v3_sys>;
+		vcc11-supply = <&vcc3v3_sys>;
+		vcc12-supply = <&vcc3v3_sys>;
+		vddio-supply = <&vcc1v8_pmu>;
+
+		regulators {
+			vdd_center: DCDC_REG1 {
+				regulator-name = "vdd_center";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <750000>;
+				regulator-max-microvolt = <1350000>;
+				regulator-ramp-delay = <6001>;
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vdd_cpu_l: DCDC_REG2 {
+				regulator-name = "vdd_cpu_l";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <750000>;
+				regulator-max-microvolt = <1350000>;
+				regulator-ramp-delay = <6001>;
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_ddr: DCDC_REG3 {
+				regulator-name = "vcc_ddr";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+				};
+			};
+
+			vcc_1v8: DCDC_REG4 {
+				regulator-name = "vcc_1v8";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vcc1v8_dvp: LDO_REG1 {
+				regulator-name = "vcc1v8_dvp";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc3v0_tp: LDO_REG2 {
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <3000000>;
+				regulator-max-microvolt = <3000000>;
+				regulator-name = "vcc3v0_tp";
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc1v8_pmu: LDO_REG3 {
+				regulator-name = "vcc1v8_pmu";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1800000>;
+				};
+			};
+
+			vcc_sd: LDO_REG4 {
+				regulator-name = "vcc_sd";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <3300000>;
+				};
+			};
+
+			vcca3v0_codec: LDO_REG5 {
+				regulator-name = "vcca3v0_codec";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <3000000>;
+				regulator-max-microvolt = <3000000>;
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_1v5: LDO_REG6 {
+				regulator-name = "vcc_1v5";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1500000>;
+				regulator-max-microvolt = <1500000>;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <1500000>;
+				};
+			};
+
+			vcca1v8_codec: LDO_REG7 {
+				regulator-name = "vcca1v8_codec";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc_3v0: LDO_REG8 {
+				regulator-name = "vcc_3v0";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-min-microvolt = <3000000>;
+				regulator-max-microvolt = <3000000>;
+				regulator-state-mem {
+					regulator-on-in-suspend;
+					regulator-suspend-microvolt = <3000000>;
+				};
+			};
+
+			vcc3v3_s3: SWITCH_REG1 {
+				regulator-name = "vcc3v3_s3";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+
+			vcc3v3_s0: SWITCH_REG2 {
+				regulator-name = "vcc3v3_s0";
+				regulator-always-on;
+				regulator-boot-on;
+				regulator-state-mem {
+					regulator-off-in-suspend;
+				};
+			};
+		};
+	};
+
+	vdd_cpu_b: regulator@40 {
+		compatible = "silergy,syr827";
+		reg = <0x40>;
+		fcs,suspend-voltage-selector = <1>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&cpu_b_sleep>;
+		regulator-name = "vdd_cpu_b";
+		regulator-min-microvolt = <712500>;
+		regulator-max-microvolt = <1500000>;
+		regulator-ramp-delay = <1000>;
+		regulator-always-on;
+		regulator-boot-on;
+		vin-supply = <&vcc_sys>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+
+	vdd_gpu: regulator@41 {
+		compatible = "silergy,syr828";
+		reg = <0x41>;
+		fcs,suspend-voltage-selector = <1>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&gpu_sleep>;
+		regulator-name = "vdd_gpu";
+		regulator-min-microvolt = <712500>;
+		regulator-max-microvolt = <1500000>;
+		regulator-ramp-delay = <1000>;
+		regulator-always-on;
+		regulator-boot-on;
+		vin-supply = <&vcc_sys>;
+
+		regulator-state-mem {
+			regulator-off-in-suspend;
+		};
+	};
+};
+
+// Used for HDMI
+&i2c3 {
+	i2c-scl-rising-time-ns = <450>;
+	i2c-scl-falling-time-ns = <15>;
+	status = "okay";
+};
+
+// HDMI sound
+&i2s2 {
+	#sound-dai-cells = <0>;
+	status = "okay";
+};
+
+&io_domains {
+	status = "okay";
+
+	bt656-supply = <&vcc_3v0>;
+	audio-supply = <&vcca1v8_codec>;
+	sdmmc-supply = <&vcc_sd>;
+	gpio1830-supply = <&vcc_3v0>;
+};
+
+&pmu_io_domains {
+	status = "okay";
+	pmu1830-supply = <&vcc_1v8>;
+};
+
+&pcie_phy {
+	status = "okay";
+};
+
+&pcie0 {
+	ep-gpios = <&gpio4 RK_PD3 GPIO_ACTIVE_HIGH>; // sch
+	max-link-speed = <2>;
+	num-lanes = <2>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&pcie_clkreqn_cpm>;
+	status = "okay";
+};
+
+&pinctrl {
+	pmic {
+		cpu_b_sleep: cpu-b-sleep {
+			rockchip,pins = <1 RK_PC1 RK_FUNC_GPIO &pcfg_pull_down>;
+		};
+
+		gpu_sleep: gpu-sleep {
+			rockchip,pins = <1 RK_PB6 RK_FUNC_GPIO &pcfg_pull_down>;
+		};
+
+		pmic_int_l: pmic-int-l {
+			rockchip,pins = <1 RK_PB2 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+
+		pmic_dvs2: pmic-dvs2 {
+			rockchip,pins = <1 RK_PC2 RK_FUNC_GPIO &pcfg_pull_down>; // bsp
+		};
+	};
+
+	sdio-pwrseq {
+		wifi_reg_on_h: wifi-reg-on-h {
+			rockchip,pins = <0 RK_PB2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	wifi {
+		wifi_host_wake_l: wifi-host-wake-l {
+			rockchip,pins = <0 RK_PA3 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	spi2 {
+		spi2_cs0: spi2-cs0 {
+			rockchip,pins =
+				<2 RK_PB4 2 &pcfg_pull_up>;
+		};
+	};
+
+	display_pin:display-pin {
+		DC_pin: dc-pin {
+			rockchip,pins = <1 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+		reset_pin: reset-pin {
+			rockchip,pins = <1 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	bt {
+		bt_enable_h: bt-enable-h {
+			rockchip,pins = <0 RK_PB1 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+
+		bt_host_wake_l: bt-host-wake-l {
+			rockchip,pins = <0 RK_PA4 RK_FUNC_GPIO &pcfg_pull_down>;
+		};
+
+		bt_wake_l: bt-wake-l {
+			rockchip,pins = <2 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	gmac {
+		vcc_phy_h: vcc-phy-h {
+			rockchip,pins = <0 RK_PB4 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+
+	leds {
+		user_led2: user_led2 {
+			rockchip,pins =
+				<2 RK_PD3 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	ir {
+		ir_int: ir-int {
+			rockchip,pins = <0 RK_PA6 RK_FUNC_GPIO &pcfg_pull_none>;
+		};
+	};
+
+	buttons {
+		power_key: power_key {
+			rockchip,pins = 
+				<0 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>;
+		};
+	};
+};
+
+// TFT
+&pwm0 {
+	status = "okay";
+};
+
+// FAN
+&pwm1 {
+	status = "okay";
+};
+
+&pwm2 {
+	status = "okay";
+};
+
+&saradc {
+	vref-supply = <&vcca1v8_s3>;
+	status = "okay";
+};
+
+&sdio0 {
+	bus-width = <4>;
+	cap-sd-highspeed;
+	cap-sdio-irq;
+	clock-frequency = <50000000>;
+	disable-wp;
+	keep-power-in-suspend;
+	max-frequency = <50000000>;
+	mmc-pwrseq = <&sdio_pwrseq>;
+	non-removable;
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdio0_bus4 &sdio0_cmd &sdio0_clk>;
+	sd-uhs-sdr104;
+	#address-cells = <1>;
+	#size-cells = <0>;
+	status = "okay";
+
+	brcmf: wifi@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+		interrupt-parent = <&gpio0>;
+		interrupts = <RK_PA3 GPIO_ACTIVE_HIGH>;
+		interrupt-names = "host-wake";
+		brcm,drive-strength = <5>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&wifi_host_wake_l>;
+	};
+};
+
+&sdmmc {
+	bus-width = <4>;
+	cap-sd-highspeed;
+	cd-gpios = <&gpio0 RK_PA7 GPIO_ACTIVE_LOW>; // bsp
+	clock-frequency = <150000000>;
+	disable-wp;
+	sd-uhs-sdr104;
+	max-frequency = <150000000>;
+	pinctrl-names = "default";
+	pinctrl-0 = <&sdmmc_clk &sdmmc_cmd &sdmmc_cd &sdmmc_bus4>;
+	vqmmc-supply = <&vcc_sd>;
+	status = "okay";
+};
+
+&sdhci {
+	bus-width = <8>;
+	mmc-hs400-1_8v;
+	mmc-hs400-enhanced-strobe;
+	keep-power-in-suspend;
+	non-removable;
+	status = "okay";
+};
+/*
+&spi1 {
+	status = "okay";
+
+	norflash: flash@0 {
+		compatible = "jedec,spi-nor";
+		reg = <0>;
+		spi-max-frequency = <50000000>;
+	};
+};
+*/
+
+&spi2 {
+	status = "okay";
+	pinctrl-names = "default";
+	pinctrl-0 = <&spi2_clk &spi2_tx &spi2_cs0>;
+
+	st7735r@0 {
+		status = "okay";
+		compatible = "sitronix,st7735r";
+		reg = <0>;
+		rgb;
+		rotate = <270>;
+		width = <80>;
+		height = <160>;
+		fps = <30>;
+		buswidth = <8>;
+		backlight = <&backlight>;
+		dc-gpios = <&gpio4 RK_PD5 GPIO_ACTIVE_HIGH>;
+		reset-gpios = <&gpio4 RK_PD1 GPIO_ACTIVE_LOW>;
+		led-gpios = <&gpio4 RK_PC2 GPIO_ACTIVE_HIGH>;  
+		spi-max-frequency = <32000000>;
+		spi-cpol;
+		spi-cpha;
+	};
+};
+
+&tcphy0 {
+	status = "okay";
+};
+
+&tcphy1 {
+	status = "okay";
+};
+
+&tsadc {
+	/* tshut mode 0:CRU 1:GPIO */
+	rockchip,hw-tshut-mode = <1>;
+	/* tshut polarity 0:LOW 1:HIGH */
+	rockchip,hw-tshut-polarity = <1>;
+	status = "okay";
+};
+
+&u2phy0 {
+	status = "okay";
+
+	u2phy0_otg: otg-port {
+		status = "okay";
+	};
+
+	u2phy0_host: host-port {
+		status = "okay";
+	};
+};
+
+&u2phy1 {
+	status = "okay";
+
+	u2phy1_otg: otg-port {
+		status = "okay";
+	};
+
+	u2phy1_host: host-port {
+		status = "okay";
+	};
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_xfer &uart0_cts &uart0_rts>;
+	status = "okay";
+
+	bluetooth {
+		compatible = "brcm,bcm43438-bt";
+		clocks = <&rk808 1>;
+		clock-names = "lpo";
+		device-wakeup-gpios = <&gpio2 RK_PD2 GPIO_ACTIVE_HIGH>;
+		host-wakeup-gpios = <&gpio0 RK_PA4 GPIO_ACTIVE_HIGH>;
+		shutdown-gpios = <&gpio0 RK_PB1 GPIO_ACTIVE_HIGH>;
+		max-speed = <4000000>;
+		pinctrl-names = "default";
+		pinctrl-0 = <&bt_host_wake_l &bt_wake_l &bt_enable_h>;
+		vbat-supply = <&vcc3v3_sys>;
+		vddio-supply = <&vcc_1v8>;
+	};
+};
+
+// Debug TTL
+&uart2 {
+	status = "okay";
+};
+
+&usb_host0_ehci {
+	status = "okay";
+};
+
+&usb_host0_ohci {
+	status = "okay";
+};
+
+&usb_host1_ehci {
+	status = "okay";
+};
+
+&usb_host1_ohci {
+	status = "okay";
+};
+
+&usbdrd3_0 {
+	status = "okay";
+};
+
+&usbdrd_dwc3_0 {
+	status = "okay";
+	dr_mode = "host";
+};
+
+&usbdrd3_1 {
+	status = "okay";
+};
+
+&usbdrd_dwc3_1 {
+	status = "okay";
+	dr_mode = "host";
+};
+
+&vopb {
+	status = "okay";
+};
+
+&vopb_mmu {
+	status = "okay";
+};
+
+&vopl {
+	status = "okay";
+};
+
+&vopl_mmu {
+	status = "okay";
+};
+
+&iep_mmu {
+	status = "okay";
+};
-- 
Armbian

