From 230f694a6df3aad6214f652209d03b381999b4ac Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megi@xff.cz>
Date: Sat, 2 Apr 2022 02:24:26 +0200
Subject: ARM: dts: sun8i-h3-orange-pi-one: Enable all gpio header UARTs

---
 arch/arm/boot/dts/allwinner/sun8i-h3-orangepi-one.dts | 9 ++++++---
 1 file changed, 6 insertions(+), 3 deletions(-)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-h3-orangepi-one.dts b/arch/arm/boot/dts/allwinner/sun8i-h3-orangepi-one.dts
index f5476cdab8a4..64c489e356ce 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-h3-orangepi-one.dts
+++ b/arch/arm/boot/dts/allwinner/sun8i-h3-orangepi-one.dts
@@ -54,6 +54,9 @@ / {
 	aliases {
 		ethernet0 = &emac;
 		serial0 = &uart0;
+		serial1 = &uart1;
+		serial2 = &uart2;
+		serial3 = &uart3;
 	};
 
 	chosen {
@@ -183,19 +186,19 @@ &uart0 {
 &uart1 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart1_pins>;
-	status = "disabled";
+	status = "okay";
 };
 
 &uart2 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart2_pins>;
-	status = "disabled";
+	status = "okay";
 };
 
 &uart3 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart3_pins>;
-	status = "disabled";
+	status = "okay";
 };
 
 &usb_otg {
-- 
2.35.3

