// SPDX-License-Identifier: (GPL-2.0+ OR MIT)

/dts-v1/;

#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/rockchip,vop2.h>
#include "rk3588s.dtsi"

/ {
	model = "FriendlyElec NanoPi M6";
	compatible = "friendlyelec,nanopi-m6", "rockchip,rk3588s";

	aliases {
		ethernet0 = &gmac1;
		mmc0 = &sdhci;
		mmc1 = &sdmmc;
	};

	chosen {
		stdout-path = "serial2:1500000n8";
	};

	analog-sound {
		compatible = "simple-audio-card";
		pinctrl-names = "default";
		pinctrl-0 = <&hp_det>;

		simple-audio-card,format = "i2s";
		simple-audio-card,hp-det-gpios = <&gpio1 RK_PC4 GPIO_ACTIVE_LOW>;
		simple-audio-card,mclk-fs = <256>;
		simple-audio-card,name = "realtek,rt5616-codec";

		simple-audio-card,routing =
			"Headphones", "HPOL",
			"Headphones", "HPOR",
			"MIC1", "Microphone Jack",
			"Microphone Jack", "micbias1";
		simple-audio-card,widgets =
			"Headphone", "Headphones",
			"Microphone", "Microphone Jack";

		simple-audio-card,cpu {
			sound-dai = <&i2s0_8ch>;
		};

		simple-audio-card,codec {
			sound-dai = <&rt5616>;
		};
	};

	adc-keys {
		compatible = "adc-keys";
		io-channels = <&saradc 0>;
		io-channel-names = "buttons";
		keyup-threshold-microvolt = <1800000>;
		poll-interval = <100>;

		button-maskrom {
			label = "Maskrom";
			linux,code = <KEY_VENDOR>;
			press-threshold-microvolt = <1800>;
		};
	};

	adc-keys-1 {
		compatible = "adc-keys";
		io-channels = <&saradc 1>;
		io-channel-names = "buttons";
		keyup-threshold-microvolt = <1800000>;
		poll-interval = <100>;

		button-maskrom {
			label = "Recovery";
			linux,code = <KEY_VENDOR>;
			press-threshold-microvolt = <1800>;
		};
	};

	hdmi-con {
		compatible = "hdmi-connector";
		type = "a";

		port {
			hdmi_con_in: endpoint {
				remote-endpoint = <&hdmi0_out_con>;
			};
		};
	};

	leds {
		compatible = "gpio-leds";

		sys_led: led-0 {
			label = "sys_led";
			gpios = <&gpio1 RK_PA4 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "heartbeat";
			pinctrl-names = "default";
			pinctrl-0 = <&sys_led_pin>;
		};

		user_led: led-1 {
			label = "user_led";
			gpios = <&gpio1 RK_PA6 GPIO_ACTIVE_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&user_led_pin>;
		};
	};

	vcc5v0_sys: regulator-vcc5v0-sys {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};

	vcc_1v1_nldo_s3: regulator-vcc-1v1-nldo-s3 {
		compatible = "regulator-fixed";
		regulator-name = "vcc_1v1_nldo_s3";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1100000>;
		regulator-max-microvolt = <1100000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vcc_3v3_s0: regulator-vcc-3v3-s0 {
		compatible = "regulator-fixed";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-name = "vcc_3v3_s0";
		vin-supply = <&vcc_3v3_s3>;
	};

	vcc_3v3_sd_s0: regulator-vcc-3v3-sd-s0 {
		compatible = "regulator-fixed";
		enable-active-high;
		gpios = <&gpio4 RK_PB4 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&sd_s0_pwr>;
		regulator-name = "vcc_3v3_sd_s0";
		regulator-boot-on;
		regulator-max-microvolt = <3000000>;
		regulator-min-microvolt = <3000000>;
		vin-supply = <&vcc_3v3_s3>;
	};

	vcc_3v3_pcie20: regulator-vcc3v3-pcie20 {
		compatible = "regulator-fixed";
		regulator-name = "vcc_3v3_pcie20";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vcc_3v3_s3>;
	};

	vcc_3v3_pcie20_m2: regulator-vcc3v3-pcie20-m2 {
		compatible = "regulator-fixed";
		enable-active-high;
		gpios = <&gpio3 RK_PC6 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&pcie_m2_0_pwren>;
		regulator-name = "vcc_3v3_pcie20_m2";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vcc_3v3_s3>;
	};

	vcc5v0_usb: regulator-vcc5v0-usb {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_usb";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vcc5v0_host_20: regulator-vcc5v0-host-20 {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio4 RK_PB5 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_host20_en>;
		regulator-name = "vcc5v0_host_20";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_usb>;
	};

	vcc5v0_usb_otg0: regulator-vbus5v0-typec {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio3 RK_PD4 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&typec5v_pwren>;
		regulator-name = "vcc5v0_usb_otg0";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_usb>;
	};
};

&combphy0_ps {
	status = "okay";
};

&combphy2_psu {
	status = "okay";
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu_big0_s0>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu_big0_s0>;
};

&cpu_b2 {
	cpu-supply = <&vdd_cpu_big1_s0>;
};

&cpu_b3 {
	cpu-supply = <&vdd_cpu_big1_s0>;
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&gmac1 {
	clock_in_out = "output";
	phy-handle = <&rgmii_phy1>;
	phy-mode = "rgmii-rxid";
	pinctrl-0 = <&gmac1_miim
		     &gmac1_tx_bus2
		     &gmac1_rx_bus2
		     &gmac1_rgmii_clk
		     &gmac1_rgmii_bus>;
	pinctrl-names = "default";
	tx_delay = <0x42>;
	status = "okay";
};

&gpu {
	mali-supply = <&vdd_gpu_s0>;
	status = "okay";
};

&hdmi0 {
	status = "okay";
};

&hdmi0_in {
	hdmi0_in_vp0: endpoint {
		remote-endpoint = <&vp0_out_hdmi0>;
	};
};

&hdmi0_out {
	hdmi0_out_con: endpoint {
		remote-endpoint = <&hdmi_con_in>;
	};
};

&hdptxphy0 {
	status = "okay";
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0m2_xfer>;
	status = "okay";

	vdd_cpu_big0_s0: regulator@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu_big0_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_cpu_big1_s0: regulator@43 {
		compatible = "rockchip,rk8603", "rockchip,rk8602";
		reg = <0x43>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu_big1_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c2 {
	status = "okay";

	vdd_npu_s0: regulator@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_npu_s0";
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <950000>;
		regulator-ramp-delay = <2300>;
		regulator-boot-on;
		regulator-always-on;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c6 {
	clock-frequency = <200000>;
	pinctrl-names = "default";
	pinctrl-0 = <&i2c6m0_xfer>;
	status = "okay";

	hym8563: rtc@51 {
		compatible = "haoyu,hym8563";
		reg = <0x51>;
		#clock-cells = <0>;
		clock-output-names = "hym8563";
		pinctrl-names = "default";
		pinctrl-0 = <&rtc_int>;
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PB0 IRQ_TYPE_LEVEL_LOW>;
		wakeup-source;
	};
};

&i2c7 {
	clock-frequency = <200000>;
	status = "okay";

	rt5616: audio-codec@1b {
		compatible = "realtek,rt5616";
		reg = <0x1b>;
		clocks = <&cru I2S0_8CH_MCLKOUT>;
		clock-names = "mclk";
		assigned-clocks = <&cru I2S0_8CH_MCLKOUT>;
		assigned-clock-rates = <12288000>;
		pinctrl-names = "default";
		pinctrl-0 = <&i2s0_mclk>;
		status = "okay";
		#sound-dai-cells = <0>;
	};
};

&i2s0_8ch {
	pinctrl-names = "default";
	pinctrl-0 = <&i2s0_lrck
				&i2s0_sclk
				&i2s0_sdi0
				&i2s0_sdo0>;
	status = "okay";
};

&mdio1 {
	rgmii_phy1: ethernet-phy@1 {
		compatible = "ethernet-phy-id001c.c916";
		reg = <0x1>;
		pinctrl-names = "default";
		pinctrl-0 = <&rtl8211f_rst>;
		reset-assert-us = <20000>;
		reset-deassert-us = <100000>;
		reset-gpios = <&gpio3 RK_PB7 GPIO_ACTIVE_LOW>;
	};
};

&pcie2x1l1 {
	reset-gpios = <&gpio1 RK_PA7 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc_3v3_pcie20>;
	status = "okay";
};

&pcie2x1l2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pcie_m2_0_prsnt>;
	reset-gpios = <&gpio4 RK_PA5 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc_3v3_pcie20_m2>;
	status = "okay";
};

&pinctrl {
	gpio-leds {
		sys_led_pin: sys-led-pin {
			rockchip,pins =
				<1 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		user_led_pin: lan1-led-pin {
			rockchip,pins =
				<1 RK_PA6 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	headphone {
		hp_det: hp-det {
			rockchip,pins = <1 RK_PC4 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	pcie {
		pcie_m2_0_pwren: pcie-m20-pwren {
			rockchip,pins = <3 RK_PC6 RK_FUNC_GPIO &pcfg_pull_none>;
		};
		pcie_m2_0_prsnt: pcie-m20-prsnt {
			rockchip,pins = <4 RK_PA5 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	hym8563 {
		rtc_int: rtc-int {
			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	sdmmc {
		sd_s0_pwr: sd-s0-pwr {
			rockchip,pins = <4 RK_PB4 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	usb {
		typec5v_pwren: typec5v-pwren {
			rockchip,pins = <3 RK_PD4 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		vcc5v0_host20_en: vcc5v0-host20-en {
			rockchip,pins = <4 RK_PB5 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	rtl8211f {
		rtl8211f_rst: rtl8211f-rst {
			rockchip,pins = <3 RK_PB7 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&saradc {
	vref-supply = <&avcc_1v8_s0>;
	status = "okay";
};

&sdhci {
	bus-width = <8>;
	no-sdio;
	no-sd;
	non-removable;
	mmc-hs200-1_8v;
	status = "okay";
};

&sdmmc {
	bus-width = <4>;
	cap-sd-highspeed;
	cd-gpios = <&gpio0 RK_PA4 GPIO_ACTIVE_LOW>;
	disable-wp;
	max-frequency = <150000000>;
	no-mmc;
	no-sdio;
	sd-uhs-sdr104;
	vmmc-supply = <&vcc_3v3_sd_s0>;
	vqmmc-supply = <&vccio_sd_s0>;
	status = "okay";
};

&spi2 {
	status = "okay";
	assigned-clocks = <&cru CLK_SPI2>;
	assigned-clock-rates = <200000000>;
	pinctrl-names = "default";
	pinctrl-0 = <&spi2m2_cs0 &spi2m2_pins>;
	num-cs = <1>;

	pmic@0 {
		compatible = "rockchip,rk806";
		spi-max-frequency = <1000000>;
		reg = <0x0>;

		interrupt-parent = <&gpio0>;
		interrupts = <7 IRQ_TYPE_LEVEL_LOW>;

		pinctrl-names = "default";
		pinctrl-0 = <&pmic_pins>, <&rk806_dvs1_null>,
			    <&rk806_dvs2_null>, <&rk806_dvs3_null>;

		system-power-controller;

		vcc1-supply = <&vcc5v0_sys>;
		vcc2-supply = <&vcc5v0_sys>;
		vcc3-supply = <&vcc5v0_sys>;
		vcc4-supply = <&vcc5v0_sys>;
		vcc5-supply = <&vcc5v0_sys>;
		vcc6-supply = <&vcc5v0_sys>;
		vcc7-supply = <&vcc5v0_sys>;
		vcc8-supply = <&vcc5v0_sys>;
		vcc9-supply = <&vcc5v0_sys>;
		vcc10-supply = <&vcc5v0_sys>;
		vcc11-supply = <&vcc_2v0_pldo_s3>;
		vcc12-supply = <&vcc5v0_sys>;
		vcc13-supply = <&vcc_1v1_nldo_s3>;
		vcc14-supply = <&vcc_1v1_nldo_s3>;
		vcca-supply = <&vcc5v0_sys>;

		gpio-controller;
		#gpio-cells = <2>;

		rk806_dvs1_null: dvs1-null-pins {
			pins = "gpio_pwrctrl1";
			function = "pin_fun0";
		};

		rk806_dvs2_null: dvs2-null-pins {
			pins = "gpio_pwrctrl2";
			function = "pin_fun0";
		};

		rk806_dvs3_null: dvs3-null-pins {
			pins = "gpio_pwrctrl3";
			function = "pin_fun0";
		};

		regulators {
			vdd_gpu_s0: vdd_gpu_mem_s0: dcdc-reg1 {
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_gpu_s0";
				regulator-enable-ramp-delay = <400>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_cpu_lit_s0: vdd_cpu_lit_mem_s0: dcdc-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_cpu_lit_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_log_s0: dcdc-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <675000>;
				regulator-max-microvolt = <750000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_log_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <750000>;
				};
			};

			vdd_vdenc_s0: vdd_vdenc_mem_s0: dcdc-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_vdenc_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_ddr_s0: dcdc-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <675000>;
				regulator-max-microvolt = <900000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_ddr_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <850000>;
				};
			};

			vdd2_ddr_s3: dcdc-reg6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vdd2_ddr_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_2v0_pldo_s3: dcdc-reg7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <2000000>;
				regulator-max-microvolt = <2000000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_2v0_pldo_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <2000000>;
				};
			};

			vcc_3v3_s3: dcdc-reg8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_3v3_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vddq_ddr_s0: dcdc-reg9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vddq_ddr_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8_s3: dcdc-reg10 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			avcc_1v8_s0: pldo-reg1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "avcc_1v8_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc_1v8_s0: pldo-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			avdd_1v2_s0: pldo-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
				regulator-name = "avdd_1v2_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			avcc_3v3_s0: pldo-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "avcc_3v3_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vccio_sd_s0: pldo-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vccio_sd_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			pldo6_s3: pldo-reg6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "pldo6_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd_0v75_s3: nldo-reg1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "vdd_0v75_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <750000>;
				};
			};

			avdd_ddr_pll_s0: nldo-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <850000>;
				regulator-name = "avdd_ddr_pll_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <850000>;
				};
			};

			avdd_0v75_s0: nldo-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "avdd_0v75_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			avdd_0v85_s0: nldo-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <850000>;
				regulator-name = "avdd_0v85_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_0v75_s0: nldo-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "vdd_0v75_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&tsadc {
	status = "okay";
};

&u2phy0 {
	status = "okay";
};

&u2phy0_otg {
	phy-supply = <&vcc5v0_usb_otg0>;
	status = "okay";
};

&u2phy2 {
	status = "okay";
};

&u2phy2_host {
	phy-supply = <&vcc5v0_host_20>;
	status = "okay";
};

&u2phy3 {
	status = "okay";
};

&u2phy3_host {
	phy-supply = <&vcc5v0_host_20>;
	status = "okay";
};

&uart2 {
	pinctrl-0 = <&uart2m0_xfer>;
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&usb_host1_ehci {
	status = "okay";
};

&usb_host1_ohci {
	status = "okay";
};

&usb_host0_xhci {
	dr_mode = "host";
	status = "okay";
};

&usbdp_phy0 {
	status = "okay";
};

&vop {
	status = "okay";
};

&vop_mmu {
	status = "okay";
};

&vp0 {
	vp0_out_hdmi0: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
		reg = <ROCKCHIP_VOP2_EP_HDMI0>;
		remote-endpoint = <&hdmi0_in_vp0>;
	};
};
