From 183f5386ee44033042a23dcb7051572cb5a229a9 Mon Sep 17 00:00:00 2001
From: Samuel Holland <samuel@sholland.org>
Date: Sat, 29 Feb 2020 01:01:58 -0600
Subject: mfd: axp20x: Add battery IRQ resources

Signed-off-by: Samuel Holland <samuel@sholland.org>
---
 drivers/mfd/axp20x.c | 36 ++++++++++++++++++++++++++++++++++++
 1 file changed, 36 insertions(+)

diff --git a/drivers/mfd/axp20x.c b/drivers/mfd/axp20x.c
index 4e52c79f8f50..8ff8bc4a22b2 100644
--- a/drivers/mfd/axp20x.c
+++ b/drivers/mfd/axp20x.c
@@ -311,6 +311,15 @@ static const struct resource axp20x_ac_power_supply_resources[] = {
 	DEFINE_RES_IRQ_NAMED(AXP20X_IRQ_ACIN_OVER_V, "ACIN_OVER_V"),
 };
 
+static const struct resource axp20x_battery_resources[] = {
+	DEFINE_RES_IRQ_NAMED(AXP20X_IRQ_BATT_PLUGIN, "BATT_PLUGIN"),
+	DEFINE_RES_IRQ_NAMED(AXP20X_IRQ_BATT_REMOVAL, "BATT_REMOVAL"),
+	DEFINE_RES_IRQ_NAMED(AXP20X_IRQ_BATT_ENT_ACT_MODE, "BATT_HEALTH_DEAD"),
+	DEFINE_RES_IRQ_NAMED(AXP20X_IRQ_BATT_EXIT_ACT_MODE, "BATT_HEALTH_GOOD"),
+	DEFINE_RES_IRQ_NAMED(AXP20X_IRQ_CHARG, "BATT_CHARGING"),
+	DEFINE_RES_IRQ_NAMED(AXP20X_IRQ_CHARG_DONE, "BATT_CHARGING_DONE"),
+};
+
 static const struct resource axp20x_pek_resources[] = {
 	DEFINE_RES_IRQ_NAMED(AXP20X_IRQ_PEK_RIS_EDGE, "PEK_DBR"),
 	DEFINE_RES_IRQ_NAMED(AXP20X_IRQ_PEK_FAL_EDGE, "PEK_DBF"),
@@ -369,6 +378,23 @@ static const struct resource axp717_pek_resources[] = {
 	DEFINE_RES_IRQ_NAMED(AXP717_IRQ_PEK_FAL_EDGE, "PEK_DBF"),
 };
 
+static const struct resource axp803_battery_resources[] = {
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_PLUGIN, "BATT_PLUGIN"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_REMOVAL, "BATT_REMOVAL"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_ENT_ACT_MODE, "BATT_HEALTH_DEAD"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_EXIT_ACT_MODE, "BATT_HEALTH_GOOD"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_CHARG, "BATT_CHARGING"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_CHARG_DONE, "BATT_CHARGING_DONE"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_CHG_TEMP_HIGH, "BATT_CHG_TEMP_HIGH"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_CHG_TEMP_HIGH_END, "BATT_CHG_TEMP_HIGH_END"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_CHG_TEMP_LOW, "BATT_CHG_TEMP_LOW"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_CHG_TEMP_LOW_END, "BATT_CHG_TEMP_LOW_END"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_ACT_TEMP_HIGH, "BATT_ACT_TEMP_HIGH"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_ACT_TEMP_HIGH_END, "BATT_ACT_TEMP_HIGH_END"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_ACT_TEMP_LOW, "BATT_ACT_TEMP_LOW"),
+	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_BATT_ACT_TEMP_LOW_END, "BATT_ACT_TEMP_LOW_END"),
+};
+
 static const struct resource axp803_pek_resources[] = {
 	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_PEK_RIS_EDGE, "PEK_DBR"),
 	DEFINE_RES_IRQ_NAMED(AXP803_IRQ_PEK_FAL_EDGE, "PEK_DBF"),
@@ -972,6 +998,8 @@ static const struct mfd_cell axp20x_cells[] = {
 	}, {
 		.name		= "axp20x-battery-power-supply",
 		.of_compatible	= "x-powers,axp209-battery-power-supply",
+		.num_resources	= ARRAY_SIZE(axp20x_battery_resources),
+		.resources	= axp20x_battery_resources,
 	}, {
 		.name		= "axp20x-ac-power-supply",
 		.of_compatible	= "x-powers,axp202-ac-power-supply",
@@ -1006,6 +1034,8 @@ static const struct mfd_cell axp221_cells[] = {
 	}, {
 		.name		= "axp20x-battery-power-supply",
 		.of_compatible	= "x-powers,axp221-battery-power-supply",
+		.num_resources	= ARRAY_SIZE(axp20x_battery_resources),
+		.resources	= axp20x_battery_resources,
 	}, {
 		.name		= "axp20x-usb-power-supply",
 		.of_compatible	= "x-powers,axp221-usb-power-supply",
@@ -1028,6 +1058,8 @@ static const struct mfd_cell axp223_cells[] = {
 	}, {
 		.name		= "axp20x-battery-power-supply",
 		.of_compatible	= "x-powers,axp221-battery-power-supply",
+		.num_resources	= ARRAY_SIZE(axp20x_battery_resources),
+		.resources	= axp20x_battery_resources,
 	}, {
 		.name		= "axp20x-regulator",
 	}, {
@@ -1144,6 +1176,8 @@ static const struct mfd_cell axp803_cells[] = {
 	}, {
 		.name		= "axp20x-battery-power-supply",
 		.of_compatible	= "x-powers,axp813-battery-power-supply",
+		.num_resources	= ARRAY_SIZE(axp803_battery_resources),
+		.resources	= axp803_battery_resources,
 	}, {
 		.name		= "axp20x-ac-power-supply",
 		.of_compatible	= "x-powers,axp813-ac-power-supply",
@@ -1204,6 +1238,8 @@ static const struct mfd_cell axp813_cells[] = {
 	}, {
 		.name		= "axp20x-battery-power-supply",
 		.of_compatible	= "x-powers,axp813-battery-power-supply",
+		.num_resources	= ARRAY_SIZE(axp803_battery_resources),
+		.resources	= axp803_battery_resources,
 	}, {
 		.name		= "axp20x-ac-power-supply",
 		.of_compatible	= "x-powers,axp813-ac-power-supply",
-- 
2.35.3

