From 7990afaf4d7e858e03de98b2024cc22c9127bd6a Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Mon, 24 Jan 2022 18:49:55 +0300
Subject: arm64:dts: Add sun50i-h5-nanopi-neo2-v1.1 device

---
 arch/arm64/boot/dts/allwinner/Makefile        |   1 +
 .../allwinner/sun50i-h5-nanopi-neo2-v1.1.dts  | 180 ++++++++++++++++++
 2 files changed, 181 insertions(+)
 create mode 100644 arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2-v1.1.dts

diff --git a/arch/arm64/boot/dts/allwinner/Makefile b/arch/arm64/boot/dts/allwinner/Makefile
index 5f535145f010..f7f9463d7cb0 100644
--- a/arch/arm64/boot/dts/allwinner/Makefile
+++ b/arch/arm64/boot/dts/allwinner/Makefile
@@ -26,6 +26,7 @@ dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-libretech-all-h3-cc.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-libretech-all-h3-it.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-libretech-all-h5-cc.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-nanopi-neo2.dtb
+dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-nanopi-neo2-v1.1.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-nanopi-neo-plus2.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-nanopi-neo-core2.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-nanopi-r1s-h5.dtb
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2-v1.1.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2-v1.1.dts
new file mode 100644
index 000000000000..06ffbbd29a93
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2-v1.1.dts
@@ -0,0 +1,180 @@
+/*
+ * Copyright (C) 2017 Icenowy Zheng <icenowy@aosc.io>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/dts-v1/;
+#include "sun50i-h5.dtsi"
+
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	model = "FriendlyARM NanoPi NEO 2";
+	compatible = "friendlyarm,nanopi-neo2", "allwinner,sun50i-h5";
+
+	aliases {
+		ethernet0 = &emac;
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		pwr {
+			label = "nanopi:red:pwr";
+			gpios = <&r_pio 0 10 GPIO_ACTIVE_HIGH>; /* PL10 */
+			linux,default-trigger = "default-on";
+		};
+
+		status {
+			label = "nanopi:green:status";
+			gpios = <&pio 0 10 GPIO_ACTIVE_HIGH>; /* PA10 */
+			linux,default-trigger = "heartbeat";
+		};
+	};
+
+	reg_gmac_3v3: gmac-3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "gmac-3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		startup-delay-us = <100000>;
+		enable-active-high;
+		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
+	};
+
+	reg_vcc3v3: vcc3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+	};
+
+	vdd_cpux: gpio-regulator {
+		compatible = "regulator-gpio";
+		pinctrl-names = "default";
+		regulator-name = "vdd-cpux";
+		regulator-type = "voltage";
+		regulator-boot-on;
+		regulator-always-on;
+		regulator-min-microvolt = <1100000>;
+		regulator-max-microvolt = <1300000>;
+		regulator-ramp-delay = <50>; /* 4ms */
+		gpios = <&r_pio 0 6 GPIO_ACTIVE_HIGH>; /* PL6 */
+		gpios-states = <0x1>;
+		states = <1100000 0x0
+			  1300000 0x1>;
+	};
+
+	reg_usb0_vbus: usb0-vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb0-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		enable-active-high;
+		gpio = <&r_pio 0 2 GPIO_ACTIVE_HIGH>; /* PL2 */
+		status = "okay";
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&vdd_cpux>;
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ehci3 {
+	status = "okay";
+};
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii-id";
+	status = "okay";
+};
+
+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@7 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <7>;
+	};
+};
+
+&mmc0 {
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <4>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>; /* PF6 */
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&ohci3 {
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pa_pins>;
+	status = "okay";
+};
+
+&usb_otg {
+	dr_mode = "otg";
+	status = "okay";
+};
+
+&usbphy {
+	/* USB Type-A port's VBUS is always on */
+	usb0_id_det-gpios = <&pio 6 12 GPIO_ACTIVE_HIGH>; /* PG12 */
+	usb0_vbus-supply = <&reg_usb0_vbus>;
+	status = "okay";
+};
-- 
2.35.3

