From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Jianfeng Liu <liujianfeng1994@gmail.com>
Date: Thu, 6 Jun 2024 23:28:01 +0800
Subject: arm64: dts: rockchip: Add HDMI support to ArmSoM Sige7

---
 arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts | 30 ++++++++++
 1 file changed, 30 insertions(+)

diff --git a/arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts b/arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts
+++ b/arch/arm64/boot/dts/rockchip/rk3588-armsom-sige7.dts
@@ -4,6 +4,7 @@
 
 #include <dt-bindings/gpio/gpio.h>
 #include <dt-bindings/leds/common.h>
+#include <dt-bindings/soc/rockchip,vop2.h>
 #include "rk3588.dtsi"
 
 / {
@@ -164,6 +165,20 @@ &gpu {
 	status = "okay";
 };
 
+&hdmi0 {
+	status = "okay";
+};
+
+&hdmi0_in {
+	hdmi0_in_vp0: endpoint {
+		remote-endpoint = <&vp0_out_hdmi0>;
+	};
+};
+
+&hdptxphy0 {
+	status = "okay";
+};
+
 &i2c0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&i2c0m2_xfer>;
@@ -723,3 +738,18 @@ &usb_host1_xhci {
 	dr_mode = "host";
 	status = "okay";
 };
+
+&vop {
+	status = "okay";
+};
+
+&vop_mmu {
+	status = "okay";
+};
+
+&vp0 {
+	vp0_out_hdmi0: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
+		reg = <ROCKCHIP_VOP2_EP_HDMI0>;
+		remote-endpoint = <&hdmi0_in_vp0>;
+	};
+};
-- 
Armbian

