From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: hehopmajieh <hehopmajieh@debian.bg>
Date: Wed, 20 May 2020 09:25:56 +0300
Subject: arm64:dts:sun50i-a64-olinuxino-1Ge16GW Disable clock phase and hs
 just for test

---
 arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino-1Ge16GW.dts | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino-1Ge16GW.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino-1Ge16GW.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino-1Ge16GW.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino-1Ge16GW.dts
@@ -15,8 +15,8 @@ / {
 
 &mmc2 {
 	vqmmc-supply = <&reg_eldo1>;
-	mmc-hs200-1_8v;
-	allwinner,drive-data-phase = <180>;
+/*	mmc-hs200-1_8v;
+	allwinner,drive-data-phase = <180>;*/
 };
 
 &pio {
-- 
Armbian

