From 60ededfd0381c8c76a587daff8ca5dfe47195149 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Wed, 5 Aug 2020 11:19:01 +0200
Subject: arm64: dts: sun50i-a64-pinephone: Fix BH modem manager behavior

PP 1.1 has STATUS line multiplexed with POWER KEY, but reading it doesn't
work reliably. Just treat 1.1 as if it was 1.0, and ignore the STATUS.
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts
index 93dc8512fe45..d67f31ef529e 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.1.dts
@@ -123,8 +123,8 @@ modem {
 
 		enable-gpios = <&pio 7 8 GPIO_ACTIVE_LOW>; /* PH8 */
 		reset-gpios = <&pio 2 4 GPIO_ACTIVE_HIGH>; /* PC4 */
-		status-gpios = <&pio 1 3 GPIO_ACTIVE_HIGH>; /* PB3 */
-		status-pwrkey-multiplexed; /* status acts as pwrkey */
+		pwrkey-gpios = <&pio 1 3 GPIO_ACTIVE_HIGH>; /* PB3 */
+		//status-pwrkey-multiplexed; /* status acts as pwrkey */
 
 		sleep-gpios = <&pio 7 7 GPIO_ACTIVE_HIGH>; /* PH7 */
 		wakeup-gpios = <&pio 1 2 GPIO_ACTIVE_HIGH>; /* PB2-RI */
-- 
2.35.3

