From 2c8fcfebe335951a63e1ecb3c8906c919f4ab94c Mon Sep 17 00:00:00 2001
From: Gunjan Gupta <viraniac@gmail.com>
Date: Fri, 29 Dec 2023 11:18:33 +0000
Subject: arm64: dts: h616: add hdmi support for zero2 and zero3

---
 .../allwinner/sun50i-h616-orangepi-zero.dtsi  |  25 ++
 .../allwinner/sun50i-h616-orangepi-zero2.dts  |   4 +
 .../arm64/boot/dts/allwinner/sun50i-h616.dtsi | 213 ++++++++++++++++++
 3 files changed, 242 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi
index 061848cf8b13..60f643abb3eb 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero.dtsi
@@ -23,6 +23,17 @@ chosen {
 		stdout-path = "serial0:115200n8";
 	};
 
+	connector {
+		compatible = "hdmi-connector";
+		type = "d";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
 	leds {
 		compatible = "gpio-leds";
 
@@ -95,6 +106,10 @@ &codec {
 	status = "okay";
 };
 
+&de {
+	status = "okay";
+};
+
 &ehci1 {
 	status = "okay";
 };
@@ -115,6 +130,16 @@ &emac0 {
 	status = "okay";
 };
 
+&hdmi {
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
 &mdio0 {
 	ext_rgmii_phy: ethernet-phy@1 {
 		compatible = "ethernet-phy-ieee802.3-c22";
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero2.dts
index 42c099483fdd..60dd0860f49f 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero2.dts
@@ -29,6 +29,10 @@ &gpu {
 	status = "okay";
 };
 
+&hdmi {
+	hvcc-supply = <&reg_bldo1>;
+};
+
 &mmc0 {
 	vmmc-supply = <&reg_dcdce>;
 };
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
index 5c1e2dc77268..564c5853af97 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
@@ -7,8 +7,11 @@
 #include <dt-bindings/clock/sun50i-h616-ccu.h>
 #include <dt-bindings/clock/sun50i-h6-r-ccu.h>
 #include <dt-bindings/clock/sun6i-rtc.h>
+#include <dt-bindings/clock/sun8i-de2.h>
+#include <dt-bindings/clock/sun8i-tcon-top.h>
 #include <dt-bindings/reset/sun50i-h616-ccu.h>
 #include <dt-bindings/reset/sun50i-h6-r-ccu.h>
+#include <dt-bindings/reset/sun8i-de2.h>
 #include <dt-bindings/thermal/thermal.h>
 
 / {
@@ -94,6 +97,12 @@ l2_cache: l2-cache {
 		};
 	};
 
+	de: display-engine {
+		compatible = "allwinner,sun50i-h6-display-engine";
+		allwinner,pipelines = <&mixer0>;
+		status = "disabled";
+	};
+
 	reserved-memory {
 		#address-cells = <2>;
 		#size-cells = <2>;
@@ -150,6 +159,50 @@ soc {
 		#size-cells = <1>;
 		ranges = <0x0 0x0 0x0 0x40000000>;
 
+		bus@1000000 {
+			compatible = "allwinner,sun50i-h616-de33",
+				     "allwinner,sun50i-a64-de2";
+			reg = <0x1000000 0x400000>;
+			allwinner,sram = <&de3_sram 1>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0 0x1000000 0x400000>;
+
+			display_clocks: clock@8000 {
+				compatible = "allwinner,sun50i-h616-de33-clk";
+				reg = <0x8000 0x100>;
+				clocks = <&ccu CLK_DE>, <&ccu CLK_BUS_DE>;
+				clock-names = "mod", "bus";
+				resets = <&ccu RST_BUS_DE>;
+				#clock-cells = <1>;
+				#reset-cells = <1>;
+			};
+
+			mixer0: mixer@100000 {
+				compatible = "allwinner,sun50i-h616-de33-mixer-0";
+				reg = <0x100000 0x100000>,
+				      <0x8100 0x40>,
+				      <0x280000 0x20000>;
+				clocks = <&display_clocks CLK_BUS_MIXER0>,
+					 <&display_clocks CLK_MIXER0>;
+				clock-names = "bus", "mod";
+				resets = <&display_clocks RST_MIXER0>;
+
+				ports {
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					mixer0_out: port@1 {
+						reg = <1>;
+
+						mixer0_out_tcon_top_mixer0: endpoint {
+							remote-endpoint = <&tcon_top_mixer0_in_mixer0>;
+						};
+					};
+				};
+			};
+		};
+
 		gpu: gpu@1800000 {
 			compatible = "allwinner,sun50i-h616-mali",
 				     "arm,mali-bifrost";
@@ -193,12 +246,31 @@ syscon: syscon@3000000 {
 			#size-cells = <1>;
 			ranges;
 
+			sram_a2: sram@100000 {
+				compatible = "mmio-sram";
+				reg = <0x00100000 0x18000>;
+				#address-cells = <1>;
+				#size-cells = <1>;
+				ranges = <0 0x00100000 0x18000>;
+
+				scpi_sram: scpi-sram@17c00 {
+					compatible = "arm,scp-shmem";
+					reg = <0x17c00 0x200>;
+				};
+			};
+
 			sram_c: sram@28000 {
 				compatible = "mmio-sram";
 				reg = <0x00028000 0x30000>;
 				#address-cells = <1>;
 				#size-cells = <1>;
 				ranges = <0 0x00028000 0x30000>;
+
+				de3_sram: sram-section@0 {
+					compatible = "allwinner,sun50i-h616-sram-c",
+						     "allwinner,sun50i-a64-sram-c";
+					reg = <0x0000 0x1e000>;
+				};
 			};
 
 			sram_c1: sram@1a00000 {
@@ -918,6 +990,147 @@ ohci3: usb@5311400 {
 			status = "disabled";
 		};
 
+		hdmi: hdmi@6000000 {
+			#sound-dai-cells = <0>;
+			compatible = "allwinner,sun50i-h616-dw-hdmi",
+				     "allwinner,sun50i-h6-dw-hdmi";
+			reg = <0x06000000 0x10000>;
+			reg-io-width = <1>;
+			interrupts = <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_HDMI>, <&ccu CLK_HDMI_SLOW>,
+				 <&ccu CLK_HDMI>, <&ccu CLK_HDMI_CEC>,
+				 <&ccu CLK_HDCP>, <&ccu CLK_BUS_HDCP>;
+			clock-names = "iahb", "isfr", "tmds", "cec", "hdcp",
+				      "hdcp-bus";
+			resets = <&ccu RST_BUS_HDMI>, <&ccu RST_BUS_HDCP>;
+			reset-names = "ctrl", "hdcp";
+			phys = <&hdmi_phy>;
+			phy-names = "phy";
+			status = "disabled";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				hdmi_in: port@0 {
+					reg = <0>;
+
+					hdmi_in_tcon_top: endpoint {
+						remote-endpoint = <&tcon_top_hdmi_out_hdmi>;
+					};
+				};
+
+				hdmi_out: port@1 {
+					reg = <1>;
+				};
+			};
+		};
+
+		hdmi_phy: hdmi-phy@6010000 {
+			compatible = "allwinner,sun50i-h616-hdmi-phy";
+			reg = <0x06010000 0x10000>;
+			clocks = <&ccu CLK_BUS_HDMI>, <&ccu CLK_HDMI_SLOW>;
+			clock-names = "bus", "mod";
+			resets = <&ccu RST_BUS_HDMI_SUB>;
+			reset-names = "phy";
+			#phy-cells = <0>;
+		};
+
+		tcon_top: tcon-top@6510000 {
+			compatible = "allwinner,sun50i-h6-tcon-top";
+			reg = <0x06510000 0x1000>;
+			clocks = <&ccu CLK_BUS_TCON_TOP>,
+				 <&ccu CLK_TCON_TV0>;
+			clock-names = "bus",
+				      "tcon-tv0";
+			clock-output-names = "tcon-top-tv0";
+			resets = <&ccu RST_BUS_TCON_TOP>;
+			#clock-cells = <1>;
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				tcon_top_mixer0_in: port@0 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <0>;
+
+					tcon_top_mixer0_in_mixer0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&mixer0_out_tcon_top_mixer0>;
+					};
+				};
+
+				tcon_top_mixer0_out: port@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+
+					tcon_top_mixer0_out_tcon_tv: endpoint@2 {
+						reg = <2>;
+						remote-endpoint = <&tcon_tv_in_tcon_top_mixer0>;
+					};
+				};
+
+				tcon_top_hdmi_in: port@4 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <4>;
+
+					tcon_top_hdmi_in_tcon_tv: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&tcon_tv_out_tcon_top>;
+					};
+				};
+
+				tcon_top_hdmi_out: port@5 {
+					reg = <5>;
+
+					tcon_top_hdmi_out_hdmi: endpoint {
+						remote-endpoint = <&hdmi_in_tcon_top>;
+					};
+				};
+			};
+		};
+
+		tcon_tv: lcd-controller@6515000 {
+			compatible = "allwinner,sun50i-h6-tcon-tv",
+				     "allwinner,sun8i-r40-tcon-tv";
+			reg = <0x06515000 0x1000>;
+			interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_TCON_TV0>,
+				 <&tcon_top CLK_TCON_TOP_TV0>;
+			clock-names = "ahb",
+				      "tcon-ch1";
+			resets = <&ccu RST_BUS_TCON_TV0>;
+			reset-names = "lcd";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				tcon_tv_in: port@0 {
+					reg = <0>;
+
+					tcon_tv_in_tcon_top_mixer0: endpoint {
+						remote-endpoint = <&tcon_top_mixer0_out_tcon_tv>;
+					};
+				};
+
+				tcon_tv_out: port@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+
+					tcon_tv_out_tcon_top: endpoint@1 {
+						reg = <1>;
+						remote-endpoint = <&tcon_top_hdmi_in_tcon_tv>;
+					};
+				};
+			};
+		};
+
 		rtc: rtc@7000000 {
 			compatible = "allwinner,sun50i-h616-rtc";
 			reg = <0x07000000 0x400>;
-- 
2.35.3

