From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Mon, 24 Jan 2022 13:26:03 +0300
Subject: drv:mmc:host:sunxi-mmc: add h5 emmc compatible

---
 drivers/mmc/host/sunxi-mmc.c | 8 ++++++++
 1 file changed, 8 insertions(+)

diff --git a/drivers/mmc/host/sunxi-mmc.c b/drivers/mmc/host/sunxi-mmc.c
index 111111111111..222222222222 100644
--- a/drivers/mmc/host/sunxi-mmc.c
+++ b/drivers/mmc/host/sunxi-mmc.c
@@ -1197,6 +1197,13 @@ static const struct sunxi_mmc_cfg sun50i_a64_emmc_cfg = {
 	.needs_new_timings = true,
 };
 
+static const struct sunxi_mmc_cfg sun50i_h5_emmc_cfg = {
+	.idma_des_size_bits = 13,
+	.clk_delays = NULL,
+	.can_calibrate = true,
+	.needs_new_timings = false,
+};
+
 static const struct sunxi_mmc_cfg sun50i_h616_cfg = {
 	.idma_des_size_bits = 16,
 	.idma_des_shift = 2,
@@ -1224,6 +1231,7 @@ static const struct of_device_id sunxi_mmc_of_match[] = {
 	{ .compatible = "allwinner,sun50i-a64-emmc", .data = &sun50i_a64_emmc_cfg },
 	{ .compatible = "allwinner,sun50i-a100-mmc", .data = &sun20i_d1_cfg },
 	{ .compatible = "allwinner,sun50i-a100-emmc", .data = &sun50i_a100_emmc_cfg },
+	{ .compatible = "allwinner,sun50i-h5-emmc", .data = &sun50i_h5_emmc_cfg },
 	{ .compatible = "allwinner,sun50i-h616-mmc", .data = &sun50i_h616_cfg },
 	{ /* sentinel */ }
 };
-- 
Armbian

