// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/*
 * Copyright (c) 2022 Rockchip Electronics Co., Ltd.
 * Copyright (c) 2024 Cyber RD Group
 *
 * Copyright (c) 2024 Tianling Shen <cnsztl@gmail.com>
 *
 * Copyright (c) 2024 chainsx <chainsx@outlook.com>
 */

/dts-v1/;
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/soc/rockchip,vop2.h>
#include <dt-bindings/usb/pd.h>
#include "rk3588.dtsi"

/ {
	model = "Cyber 3588 AIB";
	compatible = "cyber,cyber3588-aib", "rockchip,rk3588";

	aliases {
		mmc0 = &sdhci;
		mmc1 = &sdmmc;
	};

	chosen {
		stdout-path = "serial2:1500000n8";
	};

	gpio-leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&red_led_pin>, <&green_led_pin>, <&blue_led_pin>;

		status_led: led-0 {
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_STATUS;
			gpios = <&gpio1 RK_PA2 GPIO_ACTIVE_HIGH>;
		};

		led-1 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_STATUS;
			gpios = <&gpio1 RK_PA3 GPIO_ACTIVE_HIGH>;
		};

		led-2 {
			color = <LED_COLOR_ID_BLUE>;
			function = LED_FUNCTION_STATUS;
			gpios = <&gpio1 RK_PB2 GPIO_ACTIVE_HIGH>;
		};
	};

	fan: pwm-fan {
		compatible = "pwm-fan";
		cooling-levels = <0 50 80 120 160 220>;
		fan-supply = <&vcc5v0_sys>;
		pwms = <&pwm1 0 10000 0>;
		#cooling-cells = <2>;
	};

	rfkill-wlan {
		compatible = "rfkill-gpio";
		label = "rfkill-pcie-wlan";
		radio-type = "wlan";
		shutdown-gpios = <&gpio4 RK_PB5 GPIO_ACTIVE_HIGH>;
	};

	rfkill-wwan {
		compatible = "rfkill-gpio";
		label = "rfkill-wwan";
		radio-type = "wwan";
		pinctrl-names = "default";
		pinctrl-0 = <&wwan_disable_h>;
		reset-gpios = <&gpio4 RK_PA5 GPIO_ACTIVE_LOW>;
		shutdown-gpios = <&gpio4 RK_PB0 GPIO_ACTIVE_HIGH>;
	};

	vcc12v_dcin: vcc12v-dcin-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc12v_dcin";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
	};

	vcc5v0_sys: vcc5v0-sys-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc12v_dcin>;
	};

	/* pi6c pcie clock generator */
	vcc3v3_pi6c_03: vcc3v3-pi6c-03-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PC6 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&pcie_power_h>;
		regulator-name = "vcc3v3_pi6c_03";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vcc5v0_sys>;
        };

	/* actually fed by vcc5v0_sys, dependent on pi6c clock generator */
	vcc3v3_pcie2x1l0: vcc3v3-pcie2x1l0-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_pcie2x1l0";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
		regulator-always-on;
		vin-supply = <&vcc3v3_pi6c_03>;
	};

	vcc3v3_pcie2x1l2: vcc3v3-pcie2x1l2-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_pcie2x1l2";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
		regulator-always-on;
		vin-supply = <&vcc5v0_sys>;
	};

	/* actually fed by vcc5v0_sys, dependent on pi6c clock generator */
	vcc3v3_pcie30: vcc3v3-pcie30-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_pcie30";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
		regulator-always-on;
		vin-supply = <&vcc3v3_pi6c_03>;
	};

	vcc3v3_switch: vcc3v3-switch-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PB7 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&phy_pwr_en>;
		regulator-name = "vcc3v3_switch";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
		regulator-always-on;
		vin-supply = <&vcc12v_dcin>;
	};

	vcc3v3_wwan: vcc3v3-wwan-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PB0 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&wwan_power_h>;
		regulator-name = "vcc3v3_wwan";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-boot-on;
		regulator-always-on;
		vin-supply = <&vcc3v3_pcie30>;
	};

	vcc5v0_host: vcc5v0-host-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_host";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vcc5v0_sata: vcc5v0-sata-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio4 RK_PC2 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&sata_pwr_en>;
		regulator-name = "vcc5v0_sata";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc12v_dcin>;
	};

	vcc5v0_typec: vcc5v0-typec-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio4 RK_PB2 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_otg_en>;
		regulator-name = "vcc5v0_typec";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vcc_1v1_nldo_s3: vcc-1v1-nldo-s3 {
		compatible = "regulator-fixed";
		regulator-name = "vcc_1v1_nldo_s3";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1100000>;
		regulator-max-microvolt = <1100000>;
		vin-supply = <&vcc5v0_sys>;
	};
};

&combphy0_ps {
	status = "okay";
};

&combphy1_ps {
	status = "okay";
};

&combphy2_psu {
	status = "okay";
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu_big0_s0>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu_big0_s0>;
};

&cpu_b2 {
	cpu-supply = <&vdd_cpu_big1_s0>;
};

&cpu_b3 {
	cpu-supply = <&vdd_cpu_big1_s0>;
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&gmac1 {
	clock_in_out = "output";
	phy-mode = "rgmii-rxid";
	phy-supply = <&vcc3v3_switch>;
	pinctrl-names = "default";
	pinctrl-0 = <&gmac1_miim
		     &gmac1_tx_bus2
		     &gmac1_rx_bus2
		     &gmac1_rgmii_clk
		     &gmac1_rgmii_bus>;
	tx_delay = <0x42>;
	/* RK3588 GMAC is broken currently */
	status = "disabled";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&gpu {
	mali-supply = <&vdd_gpu_s0>;
	status = "okay";
};

&hdmi0 {
	status = "okay";
};

&hdmi0_in {
	hdmi0_in_vp0: endpoint {
		remote-endpoint = <&vp0_out_hdmi0>;
	};
};

&hdptxphy0 {
	status = "okay";
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0m2_xfer>;
	status = "okay";

	vdd_cpu_big0_s0: regulator@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu_big0_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_cpu_big1_s0: regulator@43 {
		compatible = "rockchip,rk8603", "rockchip,rk8602";
		reg = <0x43>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu_big1_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c1 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c1m2_xfer>;
	status = "okay";

	vdd_npu_s0: regulator@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_npu_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <950000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c2 {
	status = "okay";
};

&i2c6 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c6m0_xfer>;
	status = "okay";

	usbc0: usb-typec@22 {
		compatible = "fcs,fusb302";
		reg = <0x22>;
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PD3 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&usbc0_int>;
		vbus-supply = <&vcc5v0_typec>;
		status = "okay";

		usb_con: connector {
			compatible = "usb-c-connector";
			label = "USB-C";
			data-role = "dual";
			op-sink-microwatt = <1000000>;
			power-role = "dual";
			sink-pdos =
				<PDO_FIXED(5000, 1000, PDO_FIXED_USB_COMM)>;
			source-pdos =
				<PDO_FIXED(5000, 3000, PDO_FIXED_USB_COMM)>;
			try-power-role = "source";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;
					usbc0_orien_sw: endpoint {
						remote-endpoint = <&usbdp_phy0_orientation_switch>;
					};
				};

				port@1 {
					reg = <1>;
					usbc0_role_sw: endpoint {
						remote-endpoint = <&dwc3_0_role_switch>;
					};
				};

				port@2 {
					reg = <2>;
					dp_altmode_mux: endpoint {
						remote-endpoint = <&usbdp_phy0_dp_altmode_mux>;
					};
				};
			};
		};
	};
};

&i2c7 {
	status = "okay";
};

&mdio1 {
	switch@1d {
		compatible = "realtek,rtl8365mb";
		reg = <29>;
		reset-gpios = <&gpio0 RK_PC0 GPIO_ACTIVE_LOW>;

		ports {
			#address-cells = <1>;
			#size-cells = <0>;

			port@0 {
				reg = <0>;
				label = "lan2";
			};

			port@1 {
				reg = <1>;
				label = "lan3";
			};

			port@2 {
				reg = <2>;
				label = "lan4";
			};

			port@3 {
				reg = <3>;
				label = "lan5";
			};

			port@4 {
				reg = <4>;
				label = "lan6";
			};

			port@7 {
				reg = <7>;
				ethernet = <&gmac1>;
				phy-mode = "rgmii";

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};
		};
	};
};

/* M.2 M-Key */
&pcie2x1l0 {
	max-link-speed = <3>;
	phys = <&pcie30phy>;
	reset-gpios = <&gpio0 RK_PC4 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_pcie2x1l0>;
	status = "okay";
};

/* Right 2.5 GbE port */
&pcie2x1l1 {
	max-link-speed = <3>;
	phys = <&pcie30phy>;
	reset-gpios = <&gpio4 RK_PA2 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_pcie30>;
	status = "okay";

	pcie@0,0 {
		reg = <0x00300000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;

		rtl8125_0: pcie@30,0 {
			compatible = "pci10ec,8125";
			reg = <0x000000 0 0 0 0>;

			label = "lan1";
			realtek,led-data = <0x0 0x0 0x200 0x2b>;
		};
	};
};

/* Left 2.5 GbE port */
&pcie2x1l2 {
	reset-gpios = <&gpio4 RK_PB3 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_pcie2x1l2>;
	status = "okay";

	pcie@0,0 {
		reg = <0x00400000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;

		rtl8125_1: pcie@40,0 {
			compatible = "pci10ec,8125";
			reg = <0x000000 0 0 0 0>;

			label = "wan";
			realtek,led-data = <0x0 0x0 0x200 0x2b>;
		};
	};
};

&pcie30phy {
	data-lanes = <1 3 2 4>;
	status = "okay";
};

/* M.2 E-key */
&pcie3x4 {
	max-link-speed = <3>;
	num-lanes = <1>;
	reset-gpios = <&gpio4 RK_PB6 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_pcie30>;
	status = "okay";
};

/* M.2 B-key */
&pcie3x2 {
	max-link-speed = <3>;
	num-lanes = <1>;
	reset-gpios = <&gpio3 RK_PC6 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_wwan>;
	status = "okay";
};

&pinctrl {
	gpio-leds {
		red_led_pin: red-led-pin {
			rockchip,pins = <1 RK_PA2 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		green_led_pin: green-led-pin {
			rockchip,pins = <1 RK_PA3 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		blue_led_pin: blue-led-pin {
			rockchip,pins = <1 RK_PB2 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	gmac {
		phy_pwr_en: phy-pwr-en {
			rockchip,pins = <0 RK_PB7 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};

	pcie {
		pcie_power_h: pcie-power-h {
			rockchip,pins = <0 RK_PC6 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		wwan_power_h: wwan-power-h {
			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		wwan_disable_h: wwan-disable-h {
			rockchip,pins = <2 RK_PC5 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};

	sata {
		sata_pwr_en: sata-pwr-en {
			rockchip,pins = <4 RK_PC2 RK_FUNC_GPIO &pcfg_output_high>;
		};
	};

	usb {
		usbc0_int: usbc0-int {
			rockchip,pins = <0 RK_PD3 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		vcc5v0_otg_en: vcc5v0-otg-en {
			rockchip,pins = <4 RK_PB2 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};
};

&pwm1 {
	pinctrl-names = "active";
	pinctrl-0 = <&pwm1m1_pins>;
	status = "okay";
};

&saradc {
	vref-supply = <&avcc_1v8_s0>;
	status = "okay";
};

&sata1 {
	ahci-supply = <&vcc5v0_sata>;
	status = "okay";
};

&sdhci {
	bus-width = <8>;
	cap-mmc-highspeed;
	mmc-hs400-1_8v;
	mmc-hs400-enhanced-strobe;
	no-sdio;
	no-sd;
	non-removable;
	status = "okay";
};

&sdmmc {
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	disable-wp;
	no-sdio;
	no-mmc;
	sd-uhs-sdr50;
	vmmc-supply = <&vcc_3v3_s3>;
	vqmmc-supply = <&vccio_sd_s0>;
	status = "okay";
};

&spi2 {
	assigned-clocks = <&cru CLK_SPI2>;
	assigned-clock-rates = <200000000>;
	num-cs = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&spi2m2_cs0 &spi2m2_pins>;
	status = "okay";

	pmic@0 {
		compatible = "rockchip,rk806";
		spi-max-frequency = <1000000>;
		reg = <0x0>;

		interrupt-parent = <&gpio0>;
		interrupts = <7 IRQ_TYPE_LEVEL_LOW>;

		pinctrl-names = "default";
		pinctrl-0 = <&pmic_pins>, <&rk806_dvs1_null>,
			    <&rk806_dvs2_null>, <&rk806_dvs3_null>;

		system-power-controller;

		vcc1-supply = <&vcc5v0_sys>;
		vcc2-supply = <&vcc5v0_sys>;
		vcc3-supply = <&vcc5v0_sys>;
		vcc4-supply = <&vcc5v0_sys>;
		vcc5-supply = <&vcc5v0_sys>;
		vcc6-supply = <&vcc5v0_sys>;
		vcc7-supply = <&vcc5v0_sys>;
		vcc8-supply = <&vcc5v0_sys>;
		vcc9-supply = <&vcc5v0_sys>;
		vcc10-supply = <&vcc5v0_sys>;
		vcc11-supply = <&vcc_2v0_pldo_s3>;
		vcc12-supply = <&vcc5v0_sys>;
		vcc13-supply = <&vcc_1v1_nldo_s3>;
		vcc14-supply = <&vcc_1v1_nldo_s3>;
		vcca-supply = <&vcc5v0_sys>;

		gpio-controller;
		#gpio-cells = <2>;

		rk806_dvs1_null: dvs1-null-pins {
			pins = "gpio_pwrctrl1";
			function = "pin_fun0";
		};

		rk806_dvs2_null: dvs2-null-pins {
			pins = "gpio_pwrctrl2";
			function = "pin_fun0";
		};

		rk806_dvs3_null: dvs3-null-pins {
			pins = "gpio_pwrctrl3";
			function = "pin_fun0";
		};

		regulators {
			vdd_gpu_s0: dcdc-reg1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_gpu_s0";
				regulator-enable-ramp-delay = <400>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_cpu_lit_s0: dcdc-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_cpu_lit_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_log_s0: dcdc-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <675000>;
				regulator-max-microvolt = <750000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_log_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <750000>;
				};
			};

			vdd_vdenc_s0: dcdc-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_vdenc_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_ddr_s0: dcdc-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <675000>;
				regulator-max-microvolt = <900000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_ddr_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <850000>;
				};
			};

			vdd2_ddr_s3: dcdc-reg6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vdd2_ddr_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_2v0_pldo_s3: dcdc-reg7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <2000000>;
				regulator-max-microvolt = <2000000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_2v0_pldo_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <2000000>;
				};
			};

			vcc_3v3_s3: dcdc-reg8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_3v3_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vddq_ddr_s0: dcdc-reg9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vddq_ddr_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8_s3: dcdc-reg10 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			avcc_1v8_s0: pldo-reg1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "avcc_1v8_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8_s0: pldo-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			avdd_1v2_s0: pldo-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
				regulator-name = "avdd_1v2_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_3v3_s0: pldo-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vcc_3v3_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vccio_sd_s0: pldo-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vccio_sd_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			pldo6_s3: pldo-reg6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "pldo6_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd_0v75_s3: nldo-reg1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "vdd_0v75_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <750000>;
				};
			};

			vdd_ddr_pll_s0: nldo-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <850000>;
				regulator-name = "vdd_ddr_pll_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <850000>;
				};
			};

			avdd_0v75_s0: nldo-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "avdd_0v75_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_0v85_s0: nldo-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <850000>;
				regulator-name = "vdd_0v85_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_0v75_s0: nldo-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "vdd_0v75_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&tsadc {
	status = "okay";
};

&u2phy0 {
	status = "okay";
};

&u2phy0_otg {
	status = "okay";
};

&u2phy1 {
	status = "okay";
};

&u2phy1_otg {
	status = "okay";
};

&u2phy2 {
	status = "okay";
};

&u2phy2_host {
	status = "okay";
};

&u2phy3 {
	status = "okay";
};

&u2phy3_host {
	status = "okay";
};

&uart2 {
	pinctrl-0 = <&uart2m0_xfer>;
	status = "okay";
};

&usbdp_phy0 {
	mode-switch;
	orientation-switch;
	sbu1-dc-gpios = <&gpio4 RK_PA6 GPIO_ACTIVE_HIGH>;
	sbu2-dc-gpios = <&gpio4 RK_PA7 GPIO_ACTIVE_HIGH>;
	status = "okay";

	port {
		#address-cells = <1>;
		#size-cells = <0>;

		usbdp_phy0_orientation_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_orien_sw>;
		};

		usbdp_phy0_dp_altmode_mux: endpoint@1 {
			reg = <1>;
			remote-endpoint = <&dp_altmode_mux>;
		};
	};
};

&usbdp_phy1 {
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&usb_host0_xhci {
	usb-role-switch;
	status = "okay";

	port {
		#address-cells = <1>;
		#size-cells = <0>;

		dwc3_0_role_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_role_sw>;
		};
	};
};

&usb_host1_ehci {
	status = "okay";
};

&usb_host1_ohci {
	status = "okay";
};

&usb_host1_xhci {
	dr_mode = "host";
	status = "okay";
};

&usb_host2_xhci {
	status = "okay";
};

&vop_mmu {
	status = "okay";
};

&vop {
	status = "okay";
};

&vp0 {
	vp0_out_hdmi0: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
		reg = <ROCKCHIP_VOP2_EP_HDMI0>;
		remote-endpoint = <&hdmi0_in_vp0>;
	};
};
