From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Mon, 24 Jan 2022 14:46:11 +0300
Subject: arm:dts: a10-cubiebord a20-cubietruck green LED mmc0 default-trigger

---
 arch/arm/boot/dts/allwinner/sun4i-a10-cubieboard.dts | 2 +-
 arch/arm/boot/dts/allwinner/sun7i-a20-cubietruck.dts | 1 +
 2 files changed, 2 insertions(+), 1 deletion(-)

diff --git a/arch/arm/boot/dts/allwinner/sun4i-a10-cubieboard.dts b/arch/arm/boot/dts/allwinner/sun4i-a10-cubieboard.dts
index 111111111111..222222222222 100644
--- a/arch/arm/boot/dts/allwinner/sun4i-a10-cubieboard.dts
+++ b/arch/arm/boot/dts/allwinner/sun4i-a10-cubieboard.dts
@@ -83,7 +83,7 @@ led-0 {
 		led-1 {
 			label = "cubieboard:green:usr";
 			gpios = <&pio 7 20 GPIO_ACTIVE_HIGH>; /* LED2 */
-			linux,default-trigger = "heartbeat";
+			linux,default-trigger = "mmc0";
 		};
 	};
 };
diff --git a/arch/arm/boot/dts/allwinner/sun7i-a20-cubietruck.dts b/arch/arm/boot/dts/allwinner/sun7i-a20-cubietruck.dts
index 111111111111..222222222222 100644
--- a/arch/arm/boot/dts/allwinner/sun7i-a20-cubietruck.dts
+++ b/arch/arm/boot/dts/allwinner/sun7i-a20-cubietruck.dts
@@ -93,6 +93,7 @@ led-2 {
 		led-3 {
 			label = "cubietruck:green:usr";
 			gpios = <&pio 7 7 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "mmc0";
 		};
 	};
 
-- 
Armbian

