From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Valmantas Paliksa <walmis@gmail.com>
Date: Thu, 12 Dec 2024 12:24:33 +0200
Subject: Disable PHY_LANE_IDLE_OFF for each instance of
 rockchip_pcie_phy_power_one

Previously PHY_LANE_IDLE_OFF was only disabled for the first lane
---
 drivers/phy/rockchip/phy-rockchip-pcie.c | 12 +++++-----
 1 file changed, 6 insertions(+), 6 deletions(-)

diff --git a/drivers/phy/rockchip/phy-rockchip-pcie.c b/drivers/phy/rockchip/phy-rockchip-pcie.c
index 111111111111..222222222222 100644
--- a/drivers/phy/rockchip/phy-rockchip-pcie.c
+++ b/drivers/phy/rockchip/phy-rockchip-pcie.c
@@ -160,6 +160,12 @@ static int rockchip_pcie_phy_power_on(struct phy *phy)
 
 	guard(mutex)(&rk_phy->pcie_mutex);
 
+	regmap_write(rk_phy->reg_base,
+		     rk_phy->phy_data->pcie_laneoff,
+		     HIWORD_UPDATE(!PHY_LANE_IDLE_OFF,
+				   PHY_LANE_IDLE_MASK,
+				   PHY_LANE_IDLE_A_SHIFT + inst->index));
+
 	if (rk_phy->pwr_cnt++) {
 		return 0;
 	}
@@ -176,12 +182,6 @@ static int rockchip_pcie_phy_power_on(struct phy *phy)
 				   PHY_CFG_ADDR_MASK,
 				   PHY_CFG_ADDR_SHIFT));
 
-	regmap_write(rk_phy->reg_base,
-		     rk_phy->phy_data->pcie_laneoff,
-		     HIWORD_UPDATE(!PHY_LANE_IDLE_OFF,
-				   PHY_LANE_IDLE_MASK,
-				   PHY_LANE_IDLE_A_SHIFT + inst->index));
-
 	/*
 	 * No documented timeout value for phy operation below,
 	 * so we make it large enough here. And we use loop-break
-- 
Armbian

