From 150ddcb209012261b0a63d80ae9481134105e04a Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Sun, 1 Nov 2020 02:57:38 +0100
Subject: Revert "drm/sun4i: lvds: Invert the LVDS polarity"

This reverts commit 3bc46a083fa9f475dd2e0ab8717d9839b070b8d9.
---
 drivers/gpu/drm/sun4i/sun4i_tcon.c | 4 +++-
 1 file changed, 3 insertions(+), 1 deletion(-)

diff --git a/drivers/gpu/drm/sun4i/sun4i_tcon.c b/drivers/gpu/drm/sun4i/sun4i_tcon.c
index 960e83c8291d..fca95b76e258 100644
--- a/drivers/gpu/drm/sun4i/sun4i_tcon.c
+++ b/drivers/gpu/drm/sun4i/sun4i_tcon.c
@@ -476,7 +476,9 @@ static void sun4i_tcon0_mode_set_lvds(struct sun4i_tcon *tcon,
 		     SUN4I_TCON0_BASIC2_V_TOTAL(mode->crtc_vtotal * 2) |
 		     SUN4I_TCON0_BASIC2_V_BACKPORCH(bp));
 
-	reg = SUN4I_TCON0_LVDS_IF_CLK_SEL_TCON0;
+	reg = SUN4I_TCON0_LVDS_IF_CLK_SEL_TCON0 |
+		SUN4I_TCON0_LVDS_IF_DATA_POL_NORMAL |
+		SUN4I_TCON0_LVDS_IF_CLK_POL_NORMAL;
 	if (sun4i_tcon_get_pixel_depth(encoder) == 24)
 		reg |= SUN4I_TCON0_LVDS_IF_BITWIDTH_24BITS;
 	else
-- 
2.35.3

