From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Vasily Khoruzhick <anarsoul@gmail.com>
Date: Wed, 31 Oct 2018 20:50:09 -0700
Subject: arm64:dts: sun50i-a64-sopine-baseboard enable Bluetooth

SoPine has optional RTL8723BS WiFi + BT module, BT is connected to UART1
and uses PL4 as BT reset, PL5 as device wake GPIO, PL6 as host wake GPIO
the I2C controlling signals are connected to R_I2C bus.

Enable it in the device tree.

Signed-off-by: Vasily Khoruzhick <anarsoul@gmail.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts | 14 ++++++++++
 1 file changed, 14 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
@@ -197,6 +197,20 @@ &uart0 {
 	status = "okay";
 };
 
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>, <&uart1_rts_cts_pins>;
+	status = "okay";
+
+	bluetooth {
+		compatible = "realtek,rtl8723bs-bt";
+		reset-gpios = <&r_pio 0 4 GPIO_ACTIVE_LOW>; /* PL4 */
+		device-wake-gpios = <&r_pio 0 5 GPIO_ACTIVE_HIGH>; /* PL5 */
+		host-wake-gpios = <&r_pio 0 6 GPIO_ACTIVE_HIGH>; /* PL6 */
+		firmware-postfix = "pine64";
+	};
+};
+
 /* On Pi-2 connector */
 &uart2 {
 	pinctrl-names = "default";
-- 
Armbian

