From ef5deb15a48bd970f378ae63a058ecd70bf42834 Mon Sep 17 00:00:00 2001
From: AGM1968 <AGM1968@users.noreply.github.com>
Date: Mon, 26 Jun 2023 14:29:56 +0000
Subject: Temp_fix mailbox
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi

Signed-off-by: AGM1968 <AGM1968@users.noreply.github.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi | 7 ++++---
 1 file changed, 4 insertions(+), 3 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
index d502c1392b8e..5c986e66ab6d 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
@@ -42,7 +42,7 @@ bat: battery {
                 resistance-temp-table = <20 150>;
                 ocv-capacity-celsius = <20>;
                 ocv-capacity-table-0 =
-                	<4334000 100>,
+			<4334000 100>,
 			<4319700 99>,
 			<4304300 98>,
 			<4292200 97>,
@@ -144,7 +144,7 @@ bat: battery {
 			<3393500 1>,
 			<3256000 0>;
                 x-powers,ocv-capacity-table =
-                	<0xc0 0>,
+			<0xc0 0>,
 			<0xc1 1>,
 			<0xc2 1>,
 			<0xc3 2>,
@@ -191,7 +191,7 @@ ppkb_battery: keyboard-battery {
                 factory-internal-resistance-micro-ohms = <120000>;
                 ocv-capacity-celsius = <20>;
                 ocv-capacity-table-0 =
-                	<4147328 100>,
+			<4147328 100>,
 			<4132636 99>,
 			<4121720 98>,
 			<4110905 97>,
@@ -778,6 +778,7 @@ &mmc1 {
 	non-removable;
 	post-power-on-delay-ms = <1>; /* wifi power is always on */
 	status = "okay";
+	keep-power-in-suspend;
 
 	rtl8723cs: wifi@1 {
 		reg = <1>;
-- 
2.35.3

