From c2c2f67a5e65027ed1f142ad564fa0e170df47ca Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megi@xff.cz>
Date: Thu, 10 Nov 2022 20:11:10 +0100
Subject: arm64: dts: sun50i-a64-pinephone: Add support for Pinephone 1.2 beta

Beta versions uses a different magnetometer chip.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm64/boot/dts/allwinner/Makefile        |  1 +
 .../allwinner/sun50i-a64-pinephone-1.2b.dts   | 19 +++++++++++++++++++
 2 files changed, 20 insertions(+)
 create mode 100644 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.2b.dts

diff --git a/arch/arm64/boot/dts/allwinner/Makefile b/arch/arm64/boot/dts/allwinner/Makefile
index 00bed412ee31..9fd6b08ea528 100644
--- a/arch/arm64/boot/dts/allwinner/Makefile
+++ b/arch/arm64/boot/dts/allwinner/Makefile
@@ -12,6 +12,7 @@ dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-pinebook.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-pinephone-1.0.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-pinephone-1.1.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-pinephone-1.2.dtb
+dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-pinephone-1.2b.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-pinetab.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-pinetab-early-adopter.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-sopine-baseboard.dtb
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.2b.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.2b.dts
new file mode 100644
index 000000000000..f5ac2e9ca836
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone-1.2b.dts
@@ -0,0 +1,19 @@
+// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
+// Copyright (C) 2020 Ondrej Jirman <megous@megous.com>
+
+/dts-v1/;
+
+#include "sun50i-a64-pinephone-1.2.dts"
+
+/ {
+	model = "Pine64 PinePhone (1.2b)";
+	compatible = "pine64,pinephone-1.2b", "pine64,pinephone", "allwinner,sun50i-a64";
+};
+
+&lis3mdl {
+	status = "disabled";
+};
+
+&af8133j {
+	status = "okay";
+};
-- 
2.35.3

