From 7046bdcb478b36bc1886e3fca35a590e58c57201 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Wed, 2 Feb 2022 21:22:57 +0300
Subject: arm64:dts: sun50i-h6-orangepi enable higher clock
 regulator-max-microvolt

---
 arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi.dtsi
index ca57044cfe57..1c0e8288ebf6 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi.dtsi
@@ -218,7 +218,7 @@ reg_cldo3: cldo3 {
 			reg_dcdca: dcdca {
 				regulator-always-on;
 				regulator-min-microvolt = <810000>;
-				regulator-max-microvolt = <1080000>;
+				regulator-max-microvolt = <1160000>;
 				regulator-name = "vdd-cpu";
 			};
 
-- 
2.35.3

