From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Wed, 2 Feb 2022 20:40:02 +0300
Subject: arm64:dts:sun50i-h5 add cpu opp refs

---
 arch/arm64/boot/dts/allwinner/sun50i-h5-bananapi-m2-plus.dts | 1 +
 arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-k1-plus.dts   | 3 ++-
 arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-m1-plus2.dts  | 1 +
 arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-core2.dts | 1 +
 arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-plus2.dts | 1 +
 arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2-v1.1.dts | 1 +
 arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2.dts      | 1 +
 arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts   | 1 +
 8 files changed, 9 insertions(+), 1 deletion(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-bananapi-m2-plus.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-bananapi-m2-plus.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-bananapi-m2-plus.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-bananapi-m2-plus.dts
@@ -3,6 +3,7 @@
 
 /dts-v1/;
 #include "sun50i-h5.dtsi"
+#include "sun50i-h5-cpu-opp.dtsi"
 #include <arm/allwinner/sunxi-bananapi-m2-plus.dtsi>
 
 / {
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-k1-plus.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-k1-plus.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-k1-plus.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-k1-plus.dts
@@ -42,6 +42,7 @@
 
 /dts-v1/;
 #include "sun50i-h5.dtsi"
+#include "sun50i-h5-cpu-opp.dtsi"
 
 #include <dt-bindings/gpio/gpio.h>
 #include <dt-bindings/input/input.h>
@@ -393,4 +394,4 @@ &usbphy {
 &i2s0 {
 	sound-dai = <&pcm5102a>;
 	status = "disabled";
-};
\ No newline at end of file
+};
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-m1-plus2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-m1-plus2.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-m1-plus2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-m1-plus2.dts
@@ -43,6 +43,7 @@
 
 /dts-v1/;
 #include "sun50i-h5.dtsi"
+#include "sun50i-h5-cpu-opp.dtsi"
 
 #include <dt-bindings/gpio/gpio.h>
 
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-core2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-core2.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-core2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-core2.dts
@@ -43,6 +43,7 @@
 
 /dts-v1/;
 #include "sun50i-h5.dtsi"
+#include "sun50i-h5-cpu-opp.dtsi"
 
 #include <dt-bindings/gpio/gpio.h>
 #include <dt-bindings/input/input.h>
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-plus2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-plus2.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-plus2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-plus2.dts
@@ -4,6 +4,7 @@
 
 /dts-v1/;
 #include "sun50i-h5.dtsi"
+#include "sun50i-h5-cpu-opp.dtsi"
 
 #include <dt-bindings/gpio/gpio.h>
 #include <dt-bindings/input/input.h>
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2-v1.1.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2-v1.1.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2-v1.1.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2-v1.1.dts
@@ -42,6 +42,7 @@
 
 /dts-v1/;
 #include "sun50i-h5.dtsi"
+#include "sun50i-h5-cpu-opp.dtsi"
 
 #include <dt-bindings/gpio/gpio.h>
 
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2.dts
@@ -3,6 +3,7 @@
 
 /dts-v1/;
 #include "sun50i-h5.dtsi"
+#include "sun50i-h5-cpu-opp.dtsi"
 
 #include <dt-bindings/gpio/gpio.h>
 
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts
index 111111111111..222222222222 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts
@@ -5,6 +5,7 @@
 
 /dts-v1/;
 #include "sun50i-h5.dtsi"
+#include "sun50i-h5-cpu-opp.dtsi"
 
 #include <dt-bindings/gpio/gpio.h>
 #include <dt-bindings/input/input.h>
-- 
Armbian

