From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Koumes <koumes@centrum.cz>
Date: Sat, 1 Jun 2019 21:20:26 +0000
Subject: drv:media:dvb-frontends:si2168: fix cmd timeout

Some demuxer si2168 commands may take 130-140 ms.
(DVB-T/T2 tuner MyGica T230C v2).
Details: https://github.com/CoreELEC/CoreELEC/pull/208
---
 drivers/media/dvb-frontends/si2168.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/drivers/media/dvb-frontends/si2168.c b/drivers/media/dvb-frontends/si2168.c
index 111111111111..222222222222 100644
--- a/drivers/media/dvb-frontends/si2168.c
+++ b/drivers/media/dvb-frontends/si2168.c
@@ -40,7 +40,7 @@ static int si2168_cmd_execute(struct i2c_client *client, struct si2168_cmd *cmd)
 
 	if (cmd->rlen) {
 		/* wait cmd execution terminate */
-		#define TIMEOUT 70
+		#define TIMEOUT 200
 		timeout = jiffies + msecs_to_jiffies(TIMEOUT);
 		while (!time_after(jiffies, timeout)) {
 			ret = i2c_master_recv(client, cmd->args, cmd->rlen);
-- 
Armbian

