From c099653062731dfb0f13e60373a890b7ba88c149 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Sun, 23 Feb 2020 13:21:58 +0100
Subject: ARM: dts: sun8i-a83t-tbs-a711: Enable charging LED

The tablet has a LED connected to the PMIC. The LED is visible in the
top right corner of the tablet. Enable it.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
index 6a90763d8736..6edeaf8ed431 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
@@ -519,6 +519,10 @@ &battery_power_supply {
 	status = "okay";
 };
 
+&charger_led {
+	status = "okay";
+};
+
 &reg_aldo1 {
 	regulator-min-microvolt = <1800000>;
 	regulator-max-microvolt = <1800000>;
-- 
2.35.3

