// SPDX-License-Identifier: (GPL-2.0+ OR MIT)

/dts-v1/;

#include <dt-bindings/pinctrl/rockchip.h>
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/rockchip,vop2.h>
#include "rk3588s.dtsi"

/ {
	model = "Youyeetoo R1";
	compatible = "youyeetoo,r1", "rockchip,rk3588s";

	aliases {
		ethernet0 = &gmac1;
		mmc0 = &sdhci;
		mmc1 = &sdmmc;
		mmc2 = &sdio;
		serial2 = &uart2;
	};

	chosen {
		stdout-path = "serial2:1500000n8";
	};

	leds {
		compatible = "gpio-leds";

		sys_led: led-0 {
			label = "sys_led";
			gpios = <&gpio0 RK_PC5 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "heartbeat";
			pinctrl-names = "default";
			pinctrl-0 = <&sys_led_pin>;
		};
	};

	/* HDMI 0 CONNECTOR */

	hdmi0-con {
		compatible = "hdmi-connector";
		type = "a";

		port {
			hdmi0_con_in: endpoint {
				remote-endpoint = <&hdmi0_out_con>;
			};
		};
	};

	/* POWER REGULATOR 12V DC-IN */

	vcc12v_dcin: vcc12v-dcin-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc12v_dcin";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
	};

	/* POWER REGULATOR 5V SYS */

	vcc5v0_sys: vcc5v0-sys-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc12v_dcin>;
	};

	/* POWER REGULATOR CPU */

	vcc_1v1_nldo_s3: vcc-1v1-nldo-s3-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_1v1_nldo_s3";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1100000>;
		regulator-max-microvolt = <1100000>;
		vin-supply = <&vcc5v0_sys>;
	};

	/* POWER REGULATOR 3V (SD) */

	vcc_3v3_sd_s0: vcc-3v3-sd-s0-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_3v3_sd_s0";
		enable-active-high;
		regulator-boot-on;
		gpio = <&gpio4 RK_PB4 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&sd_s0_pwr>;
		regulator-max-microvolt = <3000000>;
		regulator-min-microvolt = <3000000>;
		vin-supply = <&vcc_3v3_s3>;
	};

	/* POWER REGULATOR 3.3V (PCIE)*/

	vcc_3v3_pcie20: vcc3v3-pcie20-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_3v3_pcie20";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		vin-supply = <&vcc_3v3_s3>;
	};

	/* POWER REGULATOR 5V (USB2 & USB3) */

	vcc5v0_usb: vcc5v0-usb-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_usb";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vcc5v0_host_20: vcc5v0-host-20 { // U13 (USB 2.0)
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio0 RK_PB0 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_host20_en>;
		regulator-name = "vcc5v0_host_20";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_usb>;
	};

	vcc5v0_host_30: vcc5v0-host-30 { // U12 (USB 3.0)
		compatible = "regulator-fixed";
		enable-active-high;
		gpio = <&gpio4 RK_PA6 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_host30_en>;
		regulator-name = "vcc5v0_host_30";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_usb>;
	};


	/* BLUETOOTH */
	wireless_bluetooth: wireless-bluetooth {
		compatible = "bluetooth-platdata";
		clocks = <&hym8563>;
		clock-names = "ext_clock";
		status = "okay";
	};

	/* WIFI */
	wireless_wlan: wireless-wlan {
		compatible = "wlan-platdata";
		wifi_chip_type = "rtl8852be";
		pinctrl-names = "default";
		pinctrl-0 = <&wifi_host_wake_irq>;
		WIFI,host_wake_irq = <&gpio0 RK_PA0 GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

    	/* FAN */
	fan0: pwm-fan {
		compatible = "pwm-fan";
		#cooling-cells = <2>;
		cooling-levels = <100 160 190 200 215 235 255>;
		pwms = <&pwm6 0 40000 0>;
        	fan-supply = <&vcc12v_dcin>;
	};
};

&combphy0_ps {
	status = "okay";
};

&combphy2_psu {
	status = "okay";
};

&gmac1 {
	clock_in_out = "output";
	phy-handle = <&rgmii_phy1>;
	phy-mode = "rgmii-rxid";
	pinctrl-0 = <&gmac1_miim
		     &gmac1_tx_bus2
		     &gmac1_rx_bus2
		     &gmac1_rgmii_clk
		     &gmac1_rgmii_bus>;
	pinctrl-names = "default";
	tx_delay = <0x42>;
	tx_delay = <0x43>;
	status = "okay";
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu_big0_s0>;
	mem-supply = <&vdd_cpu_big0_mem_s0>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu_big0_s0>;
	mem-supply = <&vdd_cpu_big0_mem_s0>;
};

&cpu_b2 {
	cpu-supply = <&vdd_cpu_big1_s0>;
	mem-supply = <&vdd_cpu_big1_mem_s0>;
};

&cpu_b3 {
	cpu-supply = <&vdd_cpu_big1_s0>;
	mem-supply = <&vdd_cpu_big1_mem_s0>;
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu_lit_s0>;
	mem-supply = <&vdd_cpu_lit_mem_s0>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu_lit_s0>;
	mem-supply = <&vdd_cpu_lit_mem_s0>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu_lit_s0>;
	mem-supply = <&vdd_cpu_lit_mem_s0>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu_lit_s0>;
	mem-supply = <&vdd_cpu_lit_mem_s0>;
};

&gpu {
	mali-supply = <&vdd_gpu_s0>;
	status = "okay";
};

&hdmi0 {
	enable-gpios = <&gpio4 RK_PB6 GPIO_ACTIVE_HIGH>;
	status = "okay";
};

&hdmi0_in {
	hdmi0_in_vp0: endpoint {
		remote-endpoint = <&vp0_out_hdmi0>;
	};
};

&hdmi0_out {
	hdmi0_out_con: endpoint {
		remote-endpoint = <&hdmi0_con_in>;
	};
};

&hdmi0_sound {
	status = "okay";
};

&hdptxphy0 {
	status = "okay";
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0m2_xfer>;
	status = "okay";

	vdd_cpu_big0_s0: vdd_cpu_big0_mem_s0: regulator@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu_big0_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_cpu_big1_s0: vdd_cpu_big1_mem_s0: regulator@43 {
		compatible = "rockchip,rk8603", "rockchip,rk8602";
		reg = <0x43>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu_big1_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c2 {
	status = "okay";

	vdd_npu_s0: vdd_npu_mem_s0: rk8602@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		fcs,suspend-voltage-selector = <1>;
		regulator-compatible = "rk860x-reg";
		regulator-name = "vdd_npu_s0";
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <950000>;
		regulator-ramp-delay = <2300>;
		regulator-boot-on;
		regulator-always-on;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c6 {
    status = "okay";
    pinctrl-names = "default";
    pinctrl-0 = <&i2c6m3_xfer>;

    /* RTC */
    hym8563: hym8563@51 {
        compatible = "haoyu,hym8563";
        reg = <0x51>;
        #clock-cells = <0>;
        clock-frequency = <32768>;
        clock-output-names = "hym8563";
        status = "okay";
    };
};

&i2s5_8ch {
	status = "okay";
};

&package_thermal {
	polling-delay = <1000>;

	trips {
		package_fan0: package-fan0 {
			temperature = <55000>;
			hysteresis = <2000>;
			type = "active";
		};
		package_fan1: package-fan1 {
			temperature = <65000>;
			hysteresis = <2000>;
			type = "active";
		};
	};

	cooling-maps {
		map1 {
			trip = <&package_fan0>;
			cooling-device = <&fan0 THERMAL_NO_LIMIT 1>;
		};
		map2 {
			trip = <&package_fan1>;
			cooling-device = <&fan0 2 THERMAL_NO_LIMIT>;
		};
	};
};


&mdio1 {
	rgmii_phy1: phy@1 {
		compatible = "ethernet-phy-ieee802.3-c22";
		reg = <0x1>;
	};
};

&pcie2x1l1 {
	reset-gpios = <&gpio1 RK_PA7 GPIO_ACTIVE_HIGH>;
	rockchip,init-delay-ms = <100>;
	vpcie3v3-supply = <&vcc_3v3_pcie20>;
	status = "okay";
};

&pcie2x1l2 {
	reset-gpios = <&gpio3 RK_PD1 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc_3v3_pcie20>;
	status = "okay";
};


&pinctrl {
	/* TODO: SOUND */
	sound {
		hp_detect: hp-detect {
            		rockchip,pins = <1 RK_PC0 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
	/* GPIO LEDS */
	gpio-leds {
		sys_led_pin: sys-led-pin {
			rockchip,pins = <0 RK_PC5 RK_FUNC_GPIO &pcfg_pull_none>;

		};
	};
	/* RTC */
	hym8563 {
		rtc_int: rtc-int {
			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};
	/* SD */
	sdmmc {
		sd_s0_pwr: sd-s0-pwr {
			rockchip,pins = <4 RK_PB4 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};
	/* USB */
	usb {
		vcc5v0_host20_en: vcc5v0-host20-en { // USB 2.0
		rockchip,pins = <0 RK_PC4 RK_FUNC_GPIO &pcfg_pull_up>;
		};
		vcc5v0_host30_en: vcc5v0-host30-en { // USB 3.0
		rockchip,pins = <4 RK_PA6 RK_FUNC_GPIO &pcfg_pull_up>;
		};
	};
	/* WIRELESS */
	wireless-wlan {
		wifi_host_wake_irq: wifi-host-wake-irq {
			rockchip,pins = <0 RK_PA0 RK_FUNC_GPIO &pcfg_pull_down>;
		};
	};
};

&saradc {
	vref-supply = <&avcc_1v8_s0>;
	status = "okay";
};

&sdhci {
	bus-width = <8>;
	no-sdio;
	no-sd;
	non-removable;
	/* HS400 doesn't work properly -> https://github.com/torvalds/linux/commit/cee572756aa2cb46e959e9797ad4b730b78a050b */
	mmc-hs200-1_8v;
	max-frequency = <200000000>;
	status = "okay";
};

&sdmmc {
	max-frequency = <200000000>;
	no-sdio;
	no-mmc;
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	disable-wp;
	sd-uhs-sdr104;
	vmmc-supply = <&vcc_3v3_sd_s0>;
	vqmmc-supply = <&vccio_sd_s0>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdmmc_bus4 &sdmmc_clk &sdmmc_cmd &sdmmc_det>;
	status = "okay";
};

&spi2 {
	status = "okay";
	assigned-clocks = <&cru CLK_SPI2>;
	assigned-clock-rates = <200000000>;
	pinctrl-names = "default";
	pinctrl-0 = <&spi2m2_cs0 &spi2m2_pins>;
	num-cs = <1>;

	pmic@0 {
		compatible = "rockchip,rk806";
		spi-max-frequency = <1000000>;
		reg = <0x0>;

		interrupt-parent = <&gpio0>;
		interrupts = <7 IRQ_TYPE_LEVEL_LOW>;

		pinctrl-names = "default";
		pinctrl-0 = <&pmic_pins>, <&rk806_dvs1_null>,
			    <&rk806_dvs2_null>, <&rk806_dvs3_null>;

		system-power-controller;

		vcc1-supply = <&vcc5v0_sys>;
		vcc2-supply = <&vcc5v0_sys>;
		vcc3-supply = <&vcc5v0_sys>;
		vcc4-supply = <&vcc5v0_sys>;
		vcc5-supply = <&vcc5v0_sys>;
		vcc6-supply = <&vcc5v0_sys>;
		vcc7-supply = <&vcc5v0_sys>;
		vcc8-supply = <&vcc5v0_sys>;
		vcc9-supply = <&vcc5v0_sys>;
		vcc10-supply = <&vcc5v0_sys>;
		vcc11-supply = <&vcc_2v0_pldo_s3>;
		vcc12-supply = <&vcc5v0_sys>;
		vcc13-supply = <&vcc_1v1_nldo_s3>;
		vcc14-supply = <&vcc_1v1_nldo_s3>;
		vcca-supply = <&vcc5v0_sys>;

		gpio-controller;
		#gpio-cells = <2>;

		rk806_dvs1_null: dvs1-null-pins {
			pins = "gpio_pwrctrl2";
			function = "pin_fun0";
		};

		rk806_dvs2_null: dvs2-null-pins {
			pins = "gpio_pwrctrl2";
			function = "pin_fudr_moden0";
		};

		rk806_dvs3_null: dvs3-null-pins {
			pins = "gpio_pwrctrl3";
			function = "pin_fun0";
		};

		regulators {
			vdd_gpu_s0: vdd_gpu_mem_s0: dcdc-reg1 {
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_gpu_s0";
				regulator-enable-ramp-delay = <400>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_cpu_lit_s0: vdd_cpu_lit_mem_s0: dcdc-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_cpu_lit_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_log_s0: dcdc-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <675000>;
				regulator-max-microvolt = <750000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_log_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <750000>;
				};
			};

			vdd_vdenc_s0: vdd_vdenc_mem_s0: dcdc-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-init-microvolt = <750000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_vdenc_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_ddr_s0: dcdc-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <675000>;
				regulator-max-microvolt = <900000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_ddr_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <850000>;
				};
			};

			vdd2_ddr_s3: dcdc-reg6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vdd2_ddr_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_2v0_pldo_s3: dcdc-reg7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <2000000>;
				regulator-max-microvolt = <2000000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_2v0_pldo_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <2000000>;
				};
			};

			vcc_3v3_s3: dcdc-reg8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_3v3_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vddq_ddr_s0: dcdc-reg9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vddq_ddr_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8_s3: dcdc-reg10 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			avcc_1v8_s0: pldo-reg1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "avcc_1v8_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vcc_1v8_s0: pldo-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			avdd_1v2_s0: pldo-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
				regulator-name = "avdd_1v2_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_3v3_s0: pldo-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vcc_3v3_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vccio_sd_s0: pldo-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vccio_sd_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			pldo6_s3: pldo-reg6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "pldo6_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd_0v75_s3: nldo-reg1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "vdd_0v75_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <750000>;
				};
			};

			vdd_ddr_pll_s0: nldo-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <850000>;
				regulator-name = "vdd_ddr_pll_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <850000>;
				};
			};

			avdd_0v75_s0: nldo-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "avdd_0v75_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_0v85_s0: nldo-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <850000>;
				regulator-name = "vdd_0v85_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_0v75_s0: nldo-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "vdd_0v75_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&uart2 {
	pinctrl-0 = <&uart2m0_xfer>;
	status = "okay";
};

&pwm6{
     status = "okay";
};

&tsadc {
	status = "okay";
};

/* USB */

&u2phy0 {
    status = "okay";
};

&u2phy2 {
    status = "okay";
};

&u2phy3 {
	status = "okay";
};

&u2phy0_otg {
	phy-supply = <&vcc5v0_host_30>;
	status = "okay";
};

&u2phy2_host {
	phy-supply = <&vcc5v0_host_20>;
	status = "okay";
};

&u2phy3_host {
	phy-supply = <&vcc5v0_host_20>;
    status = "okay";
};

&usb_host0_xhci {
	status = "okay";
	dr_mode = "host";
	extcon = <&u2phy0>;
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&usb_host1_ehci {
	status = "okay";
};

&usb_host1_ohci {
	status = "okay";
};

&usbdp_phy0 {
	status = "okay";
};

&vop_mmu {
	status = "okay";
};

&vop {
	status = "okay";
};

&vp0 {
	vp0_out_hdmi0: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
		reg = <ROCKCHIP_VOP2_EP_HDMI0>;
		remote-endpoint = <&hdmi0_in_vp0>;
	};
};
