From 074c33f4b2b60ea6d76968099f8210c61bbad7e1 Mon Sep 17 00:00:00 2001
From: Patrick Yavitz <pyavitz@armbian.com>
Date: Thu, 12 Dec 2024 06:49:59 -0500
Subject: Add BananaPi BPI-M4-Zero pinctrl

Signed-off-by: Patrick Yavitz <pyavitz@armbian.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi | 12 ++++++++++++
 1 file changed, 12 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
index 8de963bee2ac..2e418ffdfcdb 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
@@ -409,6 +409,12 @@ i2c0_pins: i2c0-pins {
 				function = "i2c0";
 			};
 
+			/omit-if-no-ref/
+			i2c1_pi_pins: i2c1-pi-pins {
+				pins = "PI7", "PI8";
+				function = "i2c1";
+			};
+
 			/omit-if-no-ref/
 			i2c2_ph_pins: i2c2-ph-pins {
 				pins = "PH2", "PH3";
@@ -571,6 +577,12 @@ spi1_cs0_pin: spi1-cs0-pin {
 				function = "spi1";
 			};
 
+			/omit-if-no-ref/
+			spi1_cs1_pin: spi1-cs1-pin {
+				pins = "PH9";
+				function = "spi1";
+			};
+
 			spdif_tx_pin: spdif-tx-pin {
 				pins = "PH4";
 				function = "spdif";
-- 
2.35.3

