From 3eaa6aabbb8758f9309a73287cfaaf9005a6979e Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megi@xff.cz>
Date: Fri, 23 Feb 2024 01:53:14 +0100
Subject: arm64: dts: sun50i-a64-pinephone: Use newer jack detection
 implementaion

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
index aeb282eba4b5..e7e90e5baff4 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinephone.dtsi
@@ -476,6 +476,7 @@ keyboard-power {
 &codec {
 	pinctrl-names = "default";
 	pinctrl-0 = <&aif2_pins>, <&aif3_pins>;
+	jack-type = "headset";
 	status = "okay";
 };
 
@@ -971,7 +972,7 @@ reboot_mode: reboot-mode@4 {
 &sound {
 	status = "okay";
 	simple-audio-card,name = "PinePhone";
-	simple-audio-card,aux-devs = <&codec_analog>, <&speaker_amp>;
+	simple-audio-card,aux-devs = <&codec_analog>, <&codec>, <&speaker_amp>;
 	simple-audio-card,widgets = "Microphone", "Headset Microphone",
 				    "Microphone", "Internal Microphone",
 				    "Headphone", "Headphone Jack",
-- 
2.35.3

