// SPDX-License-Identifier: (GPL-2.0+ OR MIT)

/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/soc/rockchip,vop2.h>
#include <dt-bindings/usb/pd.h>
#include "rk3588.dtsi"

/ {
	model = "Radxa ROCK 5B+";
	compatible = "radxa,rock-5b-plus", "rockchip,rk3588";

	aliases {
		mmc0 = &sdhci;
		mmc1 = &sdmmc;
		mmc2 = &sdio;
	};

	chosen {
		stdout-path = "serial2:1500000n8";
	};

	analog-sound {
		compatible = "audio-graph-card";
		label = "rk3588-es8316";

		widgets = "Microphone", "Mic Jack",
			  "Headphone", "Headphones";

		routing = "MIC2", "Mic Jack",
			  "Headphones", "HPOL",
			  "Headphones", "HPOR";

		dais = <&i2s0_8ch_p0>;
		hp-det-gpio = <&gpio1 RK_PD5 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&hp_detect>;
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&led_rgb_b>;

		led_rgb_b {
			function = LED_FUNCTION_STATUS;
			color = <LED_COLOR_ID_BLUE>;
			gpios = <&gpio0 RK_PB7 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "heartbeat";
		};
	};

	fan: pwm-fan {
		compatible = "pwm-fan";
		cooling-levels = <0 120 150 180 210 240 255>;
		fan-supply = <&vcc5v0_sys>;
		pwms = <&pwm1 0 50000 0>;
		#cooling-cells = <2>;
	};

	rfkill {
		compatible = "rfkill-gpio";
		label = "rfkill-pcie-wlan";
		radio-type = "wlan";
		shutdown-gpios = <&gpio4 RK_PA2 GPIO_ACTIVE_HIGH>;
	};

	rfkill-bt {
		compatible = "rfkill-gpio";
		label = "rfkill-m2-bt";
		radio-type = "bluetooth";
		shutdown-gpios = <&gpio3 RK_PD5 GPIO_ACTIVE_HIGH>;
	};

	vcc3v3_pcie2x1l0: vcc3v3-pcie2x1l0-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpios = <&gpio1 RK_PD2 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&pcie2_0_vcc3v3_en>;
		regulator-name = "vcc3v3_pcie2x1l0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		startup-delay-us = <50000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vcc3v3_pcie2x1l2: vcc3v3-pcie2x1l2-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3_pcie2x1l2";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		startup-delay-us = <5000>;
		vin-supply = <&vcc_3v3_s3>;
	};

	vcc3v3_pcie30: vcc3v3-pcie30-regulator {
		compatible = "regulator-fixed";
		enable-active-high;
		gpios = <&gpio1 RK_PA4 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&pcie3_vcc3v3_en>;
		regulator-name = "vcc3v3_pcie30";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		startup-delay-us = <5000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vbus5v0_typec: vbus5v0-typec-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vbus5v0_typec";
		gpio = <&gpio2 RK_PB6 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vbus5v0_typec_en>;
		enable-active-high;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		vin-supply = <&vcc5v0_sys>;
	};

	vcc5v0_host: vcc5v0-host-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_host";
		regulator-boot-on;
		regulator-always-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		enable-active-high;
		gpio = <&gpio4 RK_PA1 GPIO_ACTIVE_HIGH>;
		pinctrl-names = "default";
		pinctrl-0 = <&vcc5v0_host_en>;
		vin-supply = <&vcc5v0_sys>;
	};

	vcc5v0_sys: vcc5v0-sys-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc5v0_sys";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
	};

	vcc_1v1_nldo_s3: vcc-1v1-nldo-s3-regulator {
		compatible = "regulator-fixed";
		regulator-name = "vcc_1v1_nldo_s3";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <1100000>;
		regulator-max-microvolt = <1100000>;
		vin-supply = <&vcc5v0_sys>;
	};
};

&combphy0_ps {
	status = "okay";
};

&combphy1_ps {
	status = "okay";
};

&combphy2_psu {
	status = "okay";
};

&cpu_b0 {
	cpu-supply = <&vdd_cpu_big0_s0>;
};

&cpu_b1 {
	cpu-supply = <&vdd_cpu_big0_s0>;
};

&cpu_b2 {
	cpu-supply = <&vdd_cpu_big1_s0>;
};

&cpu_b3 {
	cpu-supply = <&vdd_cpu_big1_s0>;
};

&cpu_l0 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&cpu_l1 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&cpu_l2 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&cpu_l3 {
	cpu-supply = <&vdd_cpu_lit_s0>;
};

&gpu {
	mali-supply = <&vdd_gpu_s0>;
	status = "okay";
};

&hdmi0 {
	status = "okay";
};

&hdmi0_in {
	hdmi0_in_vp0: endpoint {
		remote-endpoint = <&vp0_out_hdmi0>;
	};
};

&hdptxphy0 {
	status = "okay";
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0m2_xfer>;
	status = "okay";

	vdd_cpu_big0_s0: regulator@42 {
		compatible = "rockchip,rk8602";
		reg = <0x42>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu_big0_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};

	vdd_cpu_big1_s0: regulator@43 {
		compatible = "rockchip,rk8603", "rockchip,rk8602";
		reg = <0x43>;
		fcs,suspend-voltage-selector = <1>;
		regulator-name = "vdd_cpu_big1_s0";
		regulator-always-on;
		regulator-boot-on;
		regulator-min-microvolt = <550000>;
		regulator-max-microvolt = <1050000>;
		regulator-ramp-delay = <2300>;
		vin-supply = <&vcc5v0_sys>;

		regulator-state-mem {
			regulator-off-in-suspend;
		};
	};
};

&i2c4 {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&i2c4m1_xfer>;

	usbc0: fusb302@22 {
		compatible = "fcs,fusb302";
		reg = <0x22>;
		interrupt-parent = <&gpio3>;
		interrupts = <RK_PB4 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		pinctrl-0 = <&usbc0_int>;
		vbus-supply = <&vbus5v0_typec>;
		status = "okay";

		usb_con: connector {
			compatible = "usb-c-connector";
			label = "USB-C";
			data-role = "dual";
			power-role = "dual";
			try-power-role = "sink";
			op-sink-microwatt = <1000000>;
			sink-pdos =
				<PDO_FIXED(5000, 3000, PDO_FIXED_USB_COMM)
				 PDO_FIXED(9000, 3000, PDO_FIXED_USB_COMM)
				 PDO_FIXED(12000, 3000, PDO_FIXED_USB_COMM)>;

			source-pdos =
				<PDO_FIXED(5000, 3000, PDO_FIXED_USB_COMM)>;

			altmodes {
				displayport {
					svid = /bits/ 16 <0xff01>;
					vdo = <0xffffffff>;
				};
			};

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				// TODO this still does not work right. kind of poking in the dark right now though..
				port@0 {
					reg = <0>;

					usbc0_orien_sw: endpoint {
						remote-endpoint = <&usbdp_phy0_orientation_switch>;
					};
				};

				port@1 {
					reg = <0>;

					usbc0_role_sw: endpoint {
						remote-endpoint = <&dwc3_0_role_switch>;
					};
				};

				port@2 {
					reg = <1>;

					dp_altmode_mux: endpoint {
						remote-endpoint = <&usbdp_phy0_dp_altmode_mux>;
					};
				};
			};
		};
	};
};

&i2c6 {
	status = "okay";

	hym8563: rtc@51 {
		compatible = "haoyu,hym8563";
		reg = <0x51>;
		#clock-cells = <0>;
		clock-output-names = "hym8563";
		pinctrl-names = "default";
		pinctrl-0 = <&hym8563_int>;
		interrupt-parent = <&gpio0>;
		interrupts = <RK_PB0 IRQ_TYPE_LEVEL_LOW>;
		wakeup-source;
	};
};

&i2c7 {
	status = "okay";

	es8316: audio-codec@11 {
		compatible = "everest,es8316";
		reg = <0x11>;
		clocks = <&cru I2S0_8CH_MCLKOUT>;
		clock-names = "mclk";
		assigned-clocks = <&cru I2S0_8CH_MCLKOUT>;
		assigned-clock-rates = <12288000>;
		#sound-dai-cells = <0>;

		port {
			es8316_p0_0: endpoint {
				remote-endpoint = <&i2s0_8ch_p0_0>;
			};
		};
	};
};

&i2s0_8ch {
	pinctrl-names = "default";
	pinctrl-0 = <&i2s0_lrck
		     &i2s0_mclk
		     &i2s0_sclk
		     &i2s0_sdi0
		     &i2s0_sdo0>;
	status = "okay";

	i2s0_8ch_p0: port {
		i2s0_8ch_p0_0: endpoint {
			dai-format = "i2s";
			mclk-fs = <256>;
			remote-endpoint = <&es8316_p0_0>;
		};
	};
};

&package_thermal {
	polling-delay = <1000>;

	trips {
		package_fan0: package-fan0 {
			temperature = <55000>;
			hysteresis = <2000>;
			type = "active";
		};

		package_fan1: package-fan1 {
			temperature = <65000>;
			hysteresis = <2000>;
			type = "active";
		};
	};

	cooling-maps {
		map0 {
			trip = <&package_fan0>;
			cooling-device = <&fan THERMAL_NO_LIMIT 1>;
		};

		map1 {
			trip = <&package_fan1>;
			cooling-device = <&fan 2 THERMAL_NO_LIMIT>;
		};
	};
};

&pcie2x1l0 {
	pinctrl-names = "default";
	pinctrl-0 = <&pcie2_0_rst>;
	reset-gpios = <&gpio4 RK_PA5 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_pcie2x1l0>;
	status = "okay";
};

&pcie2x1l2 {
	pinctrl-names = "default";
	pinctrl-0 = <&pcie2_2_rst>;
	reset-gpios = <&gpio3 RK_PB0 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_pcie2x1l2>;
	status = "okay";
};

&pcie30phy {
	status = "okay";
};

&pcie3x4 {
	pinctrl-names = "default";
	pinctrl-0 = <&pcie3_rst>;
	reset-gpios = <&gpio4 RK_PB6 GPIO_ACTIVE_HIGH>;
	vpcie3v3-supply = <&vcc3v3_pcie30>;
	status = "okay";
};

&pinctrl {
	hym8563 {
		hym8563_int: hym8563-int {
			rockchip,pins = <0 RK_PB0 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	leds {
		led_rgb_b: led-rgb-b {
			rockchip,pins = <0 RK_PB7 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	sound {
		hp_detect: hp-detect {
			rockchip,pins = <1 RK_PD5 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	pcie2 {
		pcie2_0_rst: pcie2-0-rst {
			rockchip,pins = <4 RK_PA5 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		pcie2_0_vcc3v3_en: pcie2-0-vcc-en {
			rockchip,pins = <1 RK_PD2 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		pcie2_2_rst: pcie2-2-rst {
			rockchip,pins = <3 RK_PB0 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	pcie3 {
		pcie3_rst: pcie3-rst {
			rockchip,pins = <4 RK_PB6 RK_FUNC_GPIO &pcfg_pull_none>;
		};

		pcie3_vcc3v3_en: pcie3-vcc3v3-en {
			rockchip,pins = <1 RK_PA4 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb {
		vcc5v0_host_en: vcc5v0-host-en {
			rockchip,pins = <4 RK_PA1 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};

	usb-typec {
		usbc0_int: usbc0-int {
			rockchip,pins = <3 RK_PB4 RK_FUNC_GPIO &pcfg_pull_up>;
		};

		vbus5v0_typec_en: vbus5v0-typec-en {
			rockchip,pins = <2 RK_PB6 RK_FUNC_GPIO &pcfg_pull_none>;
		};
	};
};

&pwm1 {
	status = "okay";
};

&saradc {
	vref-supply = <&avcc_1v8_s0>;
	status = "okay";
};

&sdhci {
	bus-width = <8>;
	no-sdio;
	no-sd;
	non-removable;
	// CHANGED: manually applied rock5b hs200 patch
	mmc-hs200-1_8v;
	status = "okay";
};

&sdmmc {
	max-frequency = <200000000>;
	no-sdio;
	no-mmc;
	bus-width = <4>;
	cap-mmc-highspeed;
	cap-sd-highspeed;
	cd-gpios = <&gpio0 RK_PA4 GPIO_ACTIVE_LOW>;
	disable-wp;
	sd-uhs-sdr104;
	vmmc-supply = <&vcc_3v3_s3>;
	vqmmc-supply = <&vccio_sd_s0>;
	status = "okay";
};

// removed from -plus vs 5b in vendor DT
// TODO find out why?
/*
&sdio {
	max-frequency = <200000000>;
	no-sd;
	no-mmc;
	non-removable;
	bus-width = <4>;
	cap-sdio-irq;
	disable-wp;
	keep-power-in-suspend;
	wakeup-source;
	sd-uhs-sdr12;
	sd-uhs-sdr25;
	sd-uhs-sdr50;
	sd-uhs-sdr104;
	vmmc-supply = <&vcc3v3_pcie2x1l0>;
	vqmmc-supply = <&vcc_1v8_s3>;
	pinctrl-names = "default";
	pinctrl-0 = <&sdiom0_pins>;
	status = "okay";
};
*/

&sfc {
	pinctrl-names = "default";
	pinctrl-0 = <&fspim2_pins>;
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <104000000>;
		spi-rx-bus-width = <4>;
		spi-tx-bus-width = <1>;
	};
};

&tsadc {
	status = "okay";
};

&uart6 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart6m1_xfer &uart6m1_ctsn &uart6m1_rtsn>;
	status = "okay";
};

&spi2 {
	status = "okay";
	assigned-clocks = <&cru CLK_SPI2>;
	assigned-clock-rates = <200000000>;
	pinctrl-names = "default";
	pinctrl-0 = <&spi2m2_cs0 &spi2m2_pins>;
	num-cs = <1>;

	pmic@0 {
		compatible = "rockchip,rk806";
		spi-max-frequency = <1000000>;
		reg = <0x0>;

		interrupt-parent = <&gpio0>;
		interrupts = <7 IRQ_TYPE_LEVEL_LOW>;

		pinctrl-names = "default";
		pinctrl-0 = <&pmic_pins>, <&rk806_dvs1_null>,
			    <&rk806_dvs2_null>, <&rk806_dvs3_null>;

		system-power-controller;

		vcc1-supply = <&vcc5v0_sys>;
		vcc2-supply = <&vcc5v0_sys>;
		vcc3-supply = <&vcc5v0_sys>;
		vcc4-supply = <&vcc5v0_sys>;
		vcc5-supply = <&vcc5v0_sys>;
		vcc6-supply = <&vcc5v0_sys>;
		vcc7-supply = <&vcc5v0_sys>;
		vcc8-supply = <&vcc5v0_sys>;
		vcc9-supply = <&vcc5v0_sys>;
		vcc10-supply = <&vcc5v0_sys>;
		vcc11-supply = <&vcc_2v0_pldo_s3>;
		vcc12-supply = <&vcc5v0_sys>;
		vcc13-supply = <&vcc_1v1_nldo_s3>;
		vcc14-supply = <&vcc_1v1_nldo_s3>;
		vcca-supply = <&vcc5v0_sys>;

		gpio-controller;
		#gpio-cells = <2>;

		rk806_dvs1_null: dvs1-null-pins {
			pins = "gpio_pwrctrl1";
			function = "pin_fun0";
		};

		rk806_dvs2_null: dvs2-null-pins {
			pins = "gpio_pwrctrl2";
			function = "pin_fun0";
		};

		rk806_dvs3_null: dvs3-null-pins {
			pins = "gpio_pwrctrl3";
			function = "pin_fun0";
		};

		regulators {
			vdd_gpu_s0: vdd_gpu_mem_s0: dcdc-reg1 {
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_gpu_s0";
				regulator-enable-ramp-delay = <400>;

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_cpu_lit_s0: vdd_cpu_lit_mem_s0: dcdc-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_cpu_lit_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_log_s0: dcdc-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <675000>;
				regulator-max-microvolt = <750000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_log_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <750000>;
				};
			};

			vdd_vdenc_s0: vdd_vdenc_mem_s0: dcdc-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <550000>;
				regulator-max-microvolt = <950000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_vdenc_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_ddr_s0: dcdc-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <675000>;
				regulator-max-microvolt = <900000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_ddr_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <850000>;
				};
			};

			vdd2_ddr_s3: dcdc-reg6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vdd2_ddr_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
				};
			};

			vcc_2v0_pldo_s3: dcdc-reg7 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <2000000>;
				regulator-max-microvolt = <2000000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vdd_2v0_pldo_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <2000000>;
				};
			};

			vcc_3v3_s3: dcdc-reg8 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-name = "vcc_3v3_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <3300000>;
				};
			};

			vddq_ddr_s0: dcdc-reg9 {
				regulator-always-on;
				regulator-boot-on;
				regulator-name = "vddq_ddr_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8_s3: dcdc-reg10 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			avcc_1v8_s0: pldo-reg1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "avcc_1v8_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_1v8_s0: pldo-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "vcc_1v8_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			avdd_1v2_s0: pldo-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
				regulator-name = "avdd_1v2_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vcc_3v3_s0: pldo-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <3300000>;
				regulator-max-microvolt = <3300000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vcc_3v3_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vccio_sd_s0: pldo-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <3300000>;
				regulator-ramp-delay = <12500>;
				regulator-name = "vccio_sd_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			pldo6_s3: pldo-reg6 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-name = "pldo6_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <1800000>;
				};
			};

			vdd_0v75_s3: nldo-reg1 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "vdd_0v75_s3";

				regulator-state-mem {
					regulator-on-in-suspend;
					regulator-suspend-microvolt = <750000>;
				};
			};

			vdd_ddr_pll_s0: nldo-reg2 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <850000>;
				regulator-name = "vdd_ddr_pll_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
					regulator-suspend-microvolt = <850000>;
				};
			};

			avdd_0v75_s0: nldo-reg3 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "avdd_0v75_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_0v85_s0: nldo-reg4 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <850000>;
				regulator-name = "vdd_0v85_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};

			vdd_0v75_s0: nldo-reg5 {
				regulator-always-on;
				regulator-boot-on;
				regulator-min-microvolt = <750000>;
				regulator-max-microvolt = <750000>;
				regulator-name = "vdd_0v75_s0";

				regulator-state-mem {
					regulator-off-in-suspend;
				};
			};
		};
	};
};

&tsadc {
	status = "okay";
};

&uart2 {
	pinctrl-0 = <&uart2m0_xfer>;
	status = "okay";
};

&u2phy0 {
	status = "okay";
};

&u2phy0_otg {
	status = "okay";
};

&u2phy1 {
	status = "okay";
};

&u2phy1_otg {
	status = "okay";
};

&u2phy2 {
	status = "okay";
};

&u2phy2_host {
	/* connected to USB hub, which is powered by vcc5v0_sys */
	phy-supply = <&vcc5v0_sys>;
	status = "okay";
};

&u2phy3 {
	status = "okay";
};

&u2phy3_host {
	phy-supply = <&vcc5v0_host>;
	status = "okay";
};

&usbdp_phy0 {
	status = "okay";

	mode-switch;
	orientation-switch;
	sbu1-dc-gpios = <&gpio0 RK_PC4 GPIO_ACTIVE_HIGH>;
	sbu2-dc-gpios = <&gpio0 RK_PC5 GPIO_ACTIVE_HIGH>;

	port {
		#address-cells = <1>;
		#size-cells = <0>;

		usbdp_phy0_orientation_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_orien_sw>;
		};

		usbdp_phy0_dp_altmode_mux: endpoint@1 {
			reg = <1>;
			remote-endpoint = <&dp_altmode_mux>;
		};
	};
};

&usbdp_phy1 {
	status = "okay";
};

&usb_host0_ehci {
	status = "okay";
};

&usb_host0_ohci {
	status = "okay";
};

&usb_host0_xhci {
	usb-role-switch;
	status = "okay";

	port {
		#address-cells = <1>;
		#size-cells = <0>;

		dwc3_0_role_switch: endpoint@0 {
			reg = <0>;
			remote-endpoint = <&usbc0_role_sw>;
		};
	};
};

&usb_host1_ehci {
	status = "okay";
};

&usb_host1_ohci {
	status = "okay";
};

&usb_host1_xhci {
	dr_mode = "host";
	status = "okay";
};

&usb_host2_xhci {
	status = "okay";
};

&vop_mmu {
	status = "okay";
};

&vop {
	status = "okay";
};

&vp0 {
	vp0_out_hdmi0: endpoint@ROCKCHIP_VOP2_EP_HDMI0 {
		reg = <ROCKCHIP_VOP2_EP_HDMI0>;
		remote-endpoint = <&hdmi0_in_vp0>;
	};
};
