From ab05f16488960a29e368534057af5aabea7cca78 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Wed, 2 Feb 2022 12:54:05 +0300
Subject: arm:dts:overlay Add Overlays for sunxi

---
 arch/arm/boot/dts/allwinner/Makefile          |   2 +
 arch/arm/boot/dts/allwinner/overlay/Makefile  |  97 +++++
 .../overlay/README.sun4i-a10-overlays         | 278 ++++++++++++++
 .../overlay/README.sun5i-a13-overlays         | 172 +++++++++
 .../overlay/README.sun7i-a20-overlays         | 348 ++++++++++++++++++
 .../overlay/README.sun8i-h3-overlays          | 250 +++++++++++++
 .../overlay/sun4i-a10-analog-codec.dtso       |  13 +
 .../dts/allwinner/overlay/sun4i-a10-can.dtso  |  15 +
 .../allwinner/overlay/sun4i-a10-fixup.scr-cmd | 124 +++++++
 .../dts/allwinner/overlay/sun4i-a10-i2c1.dtso |  22 ++
 .../dts/allwinner/overlay/sun4i-a10-i2c2.dtso |  22 ++
 .../dts/allwinner/overlay/sun4i-a10-nand.dtso | 103 ++++++
 .../allwinner/overlay/sun4i-a10-pps-gpio.dtso |  29 ++
 .../dts/allwinner/overlay/sun4i-a10-pwm.dtso  |  15 +
 .../overlay/sun4i-a10-spdif-out.dtso          |  38 ++
 .../overlay/sun4i-a10-spi-jedec-nor.dtso      |  57 +++
 .../overlay/sun4i-a10-spi-spidev.dtso         |  57 +++
 .../dts/allwinner/overlay/sun4i-a10-spi0.dtso |  23 ++
 .../dts/allwinner/overlay/sun4i-a10-spi1.dtso |  22 ++
 .../dts/allwinner/overlay/sun4i-a10-spi2.dtso |  23 ++
 .../allwinner/overlay/sun4i-a10-uart2.dtso    |  37 ++
 .../allwinner/overlay/sun4i-a10-uart3.dtso    |  47 +++
 .../allwinner/overlay/sun4i-a10-uart4.dtso    |  37 ++
 .../allwinner/overlay/sun4i-a10-uart5.dtso    |  32 ++
 .../allwinner/overlay/sun4i-a10-uart6.dtso    |  32 ++
 .../allwinner/overlay/sun4i-a10-uart7.dtso    |  32 ++
 .../allwinner/overlay/sun4i-a10-w1-gpio.dtso  |  29 ++
 .../overlay/sun5i-a13-analog-codec.dtso       |  13 +
 .../allwinner/overlay/sun5i-a13-fixup.scr-cmd |  48 +++
 .../dts/allwinner/overlay/sun5i-a13-i2c1.dtso |  22 ++
 .../dts/allwinner/overlay/sun5i-a13-i2c2.dtso |  22 ++
 .../dts/allwinner/overlay/sun5i-a13-nand.dtso |  60 +++
 .../dts/allwinner/overlay/sun5i-a13-pwm.dtso  |  15 +
 .../overlay/sun5i-a13-spi-jedec-nor.dtso      |  57 +++
 .../overlay/sun5i-a13-spi-spidev.dtso         |  57 +++
 .../dts/allwinner/overlay/sun5i-a13-spi0.dtso |  38 ++
 .../dts/allwinner/overlay/sun5i-a13-spi1.dtso |  39 ++
 .../dts/allwinner/overlay/sun5i-a13-spi2.dtso |  22 ++
 .../allwinner/overlay/sun5i-a13-uart0.dtso    |  32 ++
 .../allwinner/overlay/sun5i-a13-uart1.dtso    |  22 ++
 .../allwinner/overlay/sun5i-a13-uart2.dtso    |  22 ++
 .../allwinner/overlay/sun5i-a13-uart3.dtso    |  22 ++
 .../overlay/sun7i-a20-analog-codec.dtso       |  13 +
 .../dts/allwinner/overlay/sun7i-a20-can.dtso  |  15 +
 .../allwinner/overlay/sun7i-a20-fixup.scr-cmd | 143 +++++++
 .../dts/allwinner/overlay/sun7i-a20-i2c1.dtso |  22 ++
 .../dts/allwinner/overlay/sun7i-a20-i2c2.dtso |  22 ++
 .../dts/allwinner/overlay/sun7i-a20-i2c3.dtso |  22 ++
 .../dts/allwinner/overlay/sun7i-a20-i2c4.dtso |  32 ++
 .../dts/allwinner/overlay/sun7i-a20-i2s0.dtso |  25 ++
 .../dts/allwinner/overlay/sun7i-a20-i2s1.dtso |  25 ++
 .../dts/allwinner/overlay/sun7i-a20-mmc2.dtso |  18 +
 .../dts/allwinner/overlay/sun7i-a20-nand.dtso | 103 ++++++
 .../allwinner/overlay/sun7i-a20-pps-gpio.dtso |  29 ++
 .../dts/allwinner/overlay/sun7i-a20-pwm.dtso  |  15 +
 .../overlay/sun7i-a20-spdif-out.dtso          |  38 ++
 .../overlay/sun7i-a20-spi-add-cs1.dtso        |  16 +
 .../overlay/sun7i-a20-spi-jedec-nor.dtso      |  57 +++
 .../overlay/sun7i-a20-spi-spidev.dtso         |  57 +++
 .../dts/allwinner/overlay/sun7i-a20-spi0.dtso |  23 ++
 .../dts/allwinner/overlay/sun7i-a20-spi1.dtso |  22 ++
 .../dts/allwinner/overlay/sun7i-a20-spi2.dtso |  23 ++
 .../allwinner/overlay/sun7i-a20-uart2.dtso    |  32 ++
 .../allwinner/overlay/sun7i-a20-uart3.dtso    |  42 +++
 .../allwinner/overlay/sun7i-a20-uart4.dtso    |  22 ++
 .../allwinner/overlay/sun7i-a20-uart5.dtso    |  22 ++
 .../allwinner/overlay/sun7i-a20-uart6.dtso    |  22 ++
 .../allwinner/overlay/sun7i-a20-uart7.dtso    |  22 ++
 .../allwinner/overlay/sun7i-a20-w1-gpio.dtso  |  29 ++
 .../overlay/sun8i-h3-analog-codec.dtso        |  17 +
 .../dts/allwinner/overlay/sun8i-h3-cir.dtso   |  15 +
 .../allwinner/overlay/sun8i-h3-fixup.scr-cmd  | 110 ++++++
 .../dts/allwinner/overlay/sun8i-h3-i2c0.dtso  |  20 +
 .../dts/allwinner/overlay/sun8i-h3-i2c1.dtso  |  20 +
 .../dts/allwinner/overlay/sun8i-h3-i2c2.dtso  |  20 +
 .../allwinner/overlay/sun8i-h3-pps-gpio.dtso  |  29 ++
 .../dts/allwinner/overlay/sun8i-h3-pwm.dtso   |  39 ++
 .../allwinner/overlay/sun8i-h3-spdif-out.dtso |  38 ++
 .../overlay/sun8i-h3-spi-add-cs1.dtso         |  41 +++
 .../overlay/sun8i-h3-spi-jedec-nor.dtso       |  42 +++
 .../overlay/sun8i-h3-spi-spidev.dtso          |  42 +++
 .../dts/allwinner/overlay/sun8i-h3-uart1.dtso |  22 ++
 .../dts/allwinner/overlay/sun8i-h3-uart2.dtso |  22 ++
 .../dts/allwinner/overlay/sun8i-h3-uart3.dtso |  22 ++
 .../allwinner/overlay/sun8i-h3-usbhost0.dtso  |  27 ++
 .../allwinner/overlay/sun8i-h3-usbhost1.dtso  |  27 ++
 .../allwinner/overlay/sun8i-h3-usbhost2.dtso  |  27 ++
 .../allwinner/overlay/sun8i-h3-usbhost3.dtso  |  27 ++
 .../allwinner/overlay/sun8i-h3-w1-gpio.dtso   |  29 ++
 .../dts/allwinner/overlay/sun8i-r40-i2c2.dtso |  20 +
 .../dts/allwinner/overlay/sun8i-r40-i2c3.dtso |  20 +
 .../overlay/sun8i-r40-spi-spidev0.dtso        |  27 ++
 .../overlay/sun8i-r40-spi-spidev1.dtso        |  27 ++
 .../allwinner/overlay/sun8i-r40-uart2.dtso    |  22 ++
 .../allwinner/overlay/sun8i-r40-uart4.dtso    |  22 ++
 .../allwinner/overlay/sun8i-r40-uart5.dtso    |  22 ++
 .../allwinner/overlay/sun8i-r40-uart7.dtso    |  22 ++
 97 files changed, 4176 insertions(+)
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/Makefile
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/README.sun4i-a10-overlays
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/README.sun5i-a13-overlays
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/README.sun7i-a20-overlays
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/README.sun8i-h3-overlays
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-analog-codec.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-can.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-fixup.scr-cmd
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-i2c1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-i2c2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-nand.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-pps-gpio.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-pwm.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spdif-out.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi-jedec-nor.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi-spidev.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi0.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart3.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart4.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart5.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart6.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart7.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun4i-a10-w1-gpio.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-analog-codec.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-fixup.scr-cmd
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-i2c1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-i2c2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-nand.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-pwm.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi-jedec-nor.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi-spidev.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi0.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart0.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart3.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-analog-codec.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-can.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-fixup.scr-cmd
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c3.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c4.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2s0.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2s1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-mmc2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-nand.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-pps-gpio.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-pwm.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spdif-out.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-add-cs1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-jedec-nor.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-spidev.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi0.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart3.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart4.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart5.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart6.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart7.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun7i-a20-w1-gpio.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-analog-codec.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-cir.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-fixup.scr-cmd
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c0.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-pps-gpio.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-pwm.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spdif-out.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-add-cs1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-jedec-nor.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-spidev.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart3.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost0.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost3.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-h3-w1-gpio.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-r40-i2c2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-r40-i2c3.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-r40-spi-spidev0.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-r40-spi-spidev1.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart2.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart4.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart5.dtso
 create mode 100644 arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart7.dtso

diff --git a/arch/arm/boot/dts/allwinner/Makefile b/arch/arm/boot/dts/allwinner/Makefile
index 2e8615538458..ff32410674de 100644
--- a/arch/arm/boot/dts/allwinner/Makefile
+++ b/arch/arm/boot/dts/allwinner/Makefile
@@ -272,3 +272,5 @@ dtb-$(CONFIG_MACH_SUNIV) += \
 	suniv-f1c100s-licheepi-nano.dtb \
 	suniv-f1c200s-lctech-pi.dtb \
 	suniv-f1c200s-popstick-v1.1.dtb
+
+subdir-y	:= overlay
diff --git a/arch/arm/boot/dts/allwinner/overlay/Makefile b/arch/arm/boot/dts/allwinner/overlay/Makefile
new file mode 100644
index 000000000000..0c47e8fda8fc
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/Makefile
@@ -0,0 +1,97 @@
+# SPDX-License-Identifier: GPL-2.0
+dtb-$(CONFIG_MACH_SUN4I) += \
+	sun4i-a10-analog-codec.dtbo \
+	sun4i-a10-can.dtbo \
+	sun4i-a10-i2c1.dtbo \
+	sun4i-a10-i2c2.dtbo \
+	sun4i-a10-nand.dtbo \
+	sun4i-a10-pps-gpio.dtbo \
+	sun4i-a10-pwm.dtbo \
+	sun4i-a10-spdif-out.dtbo \
+	sun4i-a10-spi-jedec-nor.dtbo \
+	sun4i-a10-spi-spidev.dtbo \
+	sun4i-a10-uart2.dtbo \
+	sun4i-a10-uart3.dtbo \
+	sun4i-a10-uart4.dtbo \
+	sun4i-a10-uart5.dtbo \
+	sun4i-a10-uart6.dtbo \
+	sun4i-a10-uart7.dtbo \
+	sun4i-a10-w1-gpio.dtbo
+
+dtb-$(CONFIG_MACH_SUN5I) += \
+	sun5i-a13-analog-codec.dtbo \
+	sun5i-a13-i2c1.dtbo \
+	sun5i-a13-i2c2.dtbo \
+	sun5i-a13-nand.dtbo \
+	sun5i-a13-pwm.dtbo \
+	sun5i-a13-spi0.dtbo \
+	sun5i-a13-spi1.dtbo \
+	sun5i-a13-spi2.dtbo \
+	sun5i-a13-spi-jedec-nor.dtbo \
+	sun5i-a13-spi-spidev.dtbo \
+	sun5i-a13-uart0.dtbo \
+	sun5i-a13-uart1.dtbo \
+	sun5i-a13-uart2.dtbo \
+	sun5i-a13-uart3.dtbo
+
+dtb-$(CONFIG_MACH_SUN7I) += \
+	sun7i-a20-analog-codec.dtbo \
+	sun7i-a20-can.dtbo \
+	sun7i-a20-i2c1.dtbo \
+	sun7i-a20-i2c2.dtbo \
+	sun7i-a20-i2c3.dtbo \
+	sun7i-a20-i2c4.dtbo \
+	sun7i-a20-mmc2.dtbo \
+	sun7i-a20-nand.dtbo \
+	sun7i-a20-pps-gpio.dtbo \
+	sun7i-a20-pwm.dtbo \
+	sun7i-a20-spdif-out.dtbo \
+	sun7i-a20-spi-add-cs1.dtbo \
+	sun7i-a20-spi-jedec-nor.dtbo \
+	sun7i-a20-spi-spidev.dtbo \
+	sun7i-a20-uart2.dtbo \
+	sun7i-a20-uart3.dtbo \
+	sun7i-a20-uart4.dtbo \
+	sun7i-a20-uart5.dtbo \
+	sun7i-a20-uart6.dtbo \
+	sun7i-a20-uart7.dtbo \
+	sun7i-a20-w1-gpio.dtbo
+
+dtb-$(CONFIG_MACH_SUN8I) += \
+	sun8i-h3-analog-codec.dtbo \
+	sun8i-h3-cir.dtbo \
+	sun8i-h3-i2c0.dtbo \
+	sun8i-h3-i2c1.dtbo \
+	sun8i-h3-i2c2.dtbo \
+	sun8i-h3-pps-gpio.dtbo \
+	sun8i-h3-pwm.dtbo \
+	sun8i-h3-spdif-out.dtbo \
+	sun8i-h3-spi-add-cs1.dtbo \
+	sun8i-h3-spi-jedec-nor.dtbo \
+	sun8i-h3-spi-spidev.dtbo \
+	sun8i-h3-uart1.dtbo \
+	sun8i-h3-uart2.dtbo \
+	sun8i-h3-uart3.dtbo \
+	sun8i-h3-usbhost0.dtbo \
+	sun8i-h3-usbhost1.dtbo \
+	sun8i-h3-usbhost2.dtbo \
+	sun8i-h3-usbhost3.dtbo \
+	sun8i-h3-w1-gpio.dtbo \
+	sun8i-r40-i2c2.dtbo \
+	sun8i-r40-i2c3.dtbo \
+	sun8i-r40-spi-spidev0.dtbo \
+	sun8i-r40-spi-spidev1.dtbo \
+	sun8i-r40-uart2.dtbo \
+	sun8i-r40-uart4.dtbo \
+	sun8i-r40-uart5.dtbo \
+	sun8i-r40-uart7.dtbo
+
+scr-$(CONFIG_MACH_SUN4I) += sun4i-a10-fixup.scr
+scr-$(CONFIG_MACH_SUN5I) += sun5i-a13-fixup.scr
+scr-$(CONFIG_MACH_SUN7I) += sun7i-a20-fixup.scr
+scr-$(CONFIG_MACH_SUN8I) += sun8i-h3-fixup.scr
+
+dtbotxt-$(CONFIG_MACH_SUN4I) += README.sun4i-a10-overlays
+dtbotxt-$(CONFIG_MACH_SUN5I) += README.sun5i-a13-overlays
+dtbotxt-$(CONFIG_MACH_SUN7I) += README.sun7i-a20-overlays
+dtbotxt-$(CONFIG_MACH_SUN8I) += README.sun8i-h3-overlays
diff --git a/arch/arm/boot/dts/allwinner/overlay/README.sun4i-a10-overlays b/arch/arm/boot/dts/allwinner/overlay/README.sun4i-a10-overlays
new file mode 100644
index 000000000000..e0795f13ddf1
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/README.sun4i-a10-overlays
@@ -0,0 +1,278 @@
+This document describes overlays provided in the kernel packages
+For generic Armbian overlays documentation please see
+https://docs.armbian.com/User-Guide_Allwinner_overlays/
+
+### Platform:
+
+sun4i-a10 (Allwinner A10)
+
+### Platform details:
+
+Supported pin banks: PB, PC, PD, PE, PG, PH, PI
+
+SPI controller 0 have 2 exposed hardware CS,
+other SPI controllers have only one hardware CS
+Reference: A10 User manual section 17.4.13, A10 datasheet section 5.2
+
+I2C bus 0 is used for the AXP209 PMIC
+
+### Provided overlays:
+
+- analog-codec
+- can
+- i2c1
+- i2c2
+- nand
+- pps-gpio
+- pwm
+- spdif-out
+- spi0
+- spi1
+- spi2
+- spi-jedec-nor
+- spi-spidev
+- uart1
+- uart2
+- uart3
+- uart4
+- uart5
+- uart6
+- uart7
+- w1-gpio
+
+### Overlay details:
+
+### analog-codec
+
+Activates SoC analog codec driver that provides Line Out and Mic In
+functionality
+
+## can
+
+Activates SoC CAN controller
+
+CAN pins (TX, RX): PH20, PH21
+
+### i2c1
+
+Activates TWI/I2C bus 1
+
+I2C1 pins (SCL, SDA): PB18, PB19
+
+### i2c2
+
+Activates TWI/I2C bus 2
+
+I2C2 pins (SCL, SDA): PB20, PB21
+
+### nand
+
+Activates NAND controller
+
+This overlay should not be used until mainline MLC NAND support
+allows using NAND storage reliably
+
+### pps-gpio
+
+Activates pulse-per-second GPIO client
+
+Parameters:
+
+param_pps_pin (pin)
+	Pin PPS source is connected to
+	Optional
+	Default: PI15
+
+param_pps_falling_edge (bool)
+	Assert by falling edge
+	Optional
+	Default: 0
+	When set (to 1), assert is indicated by a falling edge
+		(instead of by a rising edge)
+
+### pwm
+
+Activates hardware PWM controller
+
+PWM pins (PWM0, PWM1): PB2, PI3
+
+Parameters:
+
+param_pwm_pins (string)
+	PWM pins activated with this overlay
+	Optional
+	Default: both
+	Supported values: 0, 1, both
+	If set to 0 only PWM0 can be used,
+		if set to 1 then only PWM1 can be used,
+		if set to both (default), both PWM0 and PWM1 can be used
+
+### spdif-out
+
+Activates SPDIF/Toslink audio output
+
+SPDIF pin: PB13
+
+### spi0
+
+Activates SPI controller 0 to use it with other overlays and sets up the pin multiplexing for it
+
+SPI 0 pins (MOSI, MISO, SCK, CS0, CS1): PI12, PI13, PI11, PI10, PI14
+
+### spi1
+
+Activates SPI controller 1 to use it with other overlays and sets up the pin multiplexing for it
+
+SPI 1 pins (MOSI, MISO, SCK, CS0): PI18, PI19, PI17, PI16
+
+### spi2
+
+Activates SPI controller 2 to use it with other overlays and sets up the pin multiplexing for it
+
+SPI 2 pins a (MOSI, MISO, SCK, CS0): PC21, PC22, PC20, PC19
+SPI 2 pins b (MOSI, MISO, SCK, CS0): PB16, PB17, PB15, PB14
+
+Parameters:
+
+param_spi2_bus_pins (char)
+	SPI bus 2 pinmux variant
+	Optional
+	Default: a
+	Supported values: a, b
+	Determines what pins SPI bus 2 is exposed on if SPI 2 is used
+
+
+### spi-jedec-nor
+
+Activates MTD support for JEDEC compatible SPI NOR flash chips on SPI bus
+supported by the kernel SPI NOR driver
+
+SPI 0 pins (MOSI, MISO, SCK, CS0, CS1): PI12, PI13, PI11, PI10, PI14
+SPI 1 pins (MOSI, MISO, SCK, CS0): PI18, PI19, PI17, PI16
+SPI 2 pins a (MOSI, MISO, SCK, CS0): PC21, PC22, PC20, PC19
+SPI 2 pins b (MOSI, MISO, SCK, CS0): PB16, PB17, PB15, PB14
+
+Parameters:
+
+param_spinor_spi_bus (int)
+	SPI bus to activate SPI NOR flash support on
+	Required
+	Supported values: 0, 1, 2
+
+param_spinor_max_freq (int)
+	Maximum SPI frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### spi-spidev
+
+Activates SPIdev device node (/dev/spidevX.Y) for userspace SPI access,
+where X is the bus number and Y is the CS number
+
+SPI 0 pins (MOSI, MISO, SCK, CS0, CS1): PI12, PI13, PI11, PI10, PI14
+SPI 1 pins (MOSI, MISO, SCK, CS0): PI18, PI19, PI17, PI16
+SPI 2 pins a (MOSI, MISO, SCK, CS0): PC21, PC22, PC20, PC19
+SPI 2 pins b (MOSI, MISO, SCK, CS0): PB16, PB17, PB15, PB14
+
+Parameters:
+
+param_spidev_spi_bus (int)
+	SPI bus to activate mcp2515 support on
+	Required
+	Supported values: 0, 1, 2
+
+param_spidev_max_freq (int)
+	Maximum SPIdev frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### uart2
+
+Activates serial port 2 (/dev/ttyS2)
+
+UART 2 pins (TX, RX, RTS, CTS): PI18, PI19, PI16, PI17
+
+Parameters:
+
+param_uart2_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
+
+### uart3
+
+Activates serial port 3 (/dev/ttyS3)
+
+UART 3 pins a (TX, RX, RTS, CTS): PG6, PG7, PG8, PG9
+UART 3 pins b (TX, RX, RTS, CTS): PH0, PH1, PH2, PH3
+
+Parameters:
+
+param_uart3_pins (char)
+	Determines what pins UART 3 is exposed on
+	Optional
+	Default: a
+	Supported values: a, b
+
+param_uart3_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
+
+### uart4
+
+Activates serial port 4 (/dev/ttyS4)
+
+UART 4 pins a (TX, RX): PG10, PG11
+UART 4 pins b (TX, RX): PH4, PH5
+
+Parameters:
+
+param_uart4_pins (char)
+	Determines what pins UART 4 is exposed on
+	Optional
+	Default: a
+	Supported values: a, b
+
+### uart 5
+
+Activates serial port 5 (/dev/ttyS5)
+
+UART 5 pins (TX, RX): PH6, PH7
+
+### uart 6
+
+Activates serial port 6 (/dev/ttyS6)
+
+UART 6 pins (TX, RX): PI12, PI13
+
+### uart 7
+
+Activates serial port 7 (/dev/ttyS7)
+
+UART 7 pins (TX, RX): PI20, PI21
+
+### w1-gpio
+
+Activates 1-Wire GPIO master
+Requires an external pull-up resistor on the data pin
+or enabling the internal pull-up
+
+Parameters:
+
+param_w1_pin (pin)
+	Data pin for 1-Wire master
+	Optional
+	Default: PI15
+
+param_w1_pin_int_pullup (bool)
+	Enable internal pull-up for the data pin
+	Optional
+	Default: 0
+	Set to 1 to enable the pull-up
+	This option should not be used with multiple sensors or long wires -
+		please use external pull-up resistor instead
diff --git a/arch/arm/boot/dts/allwinner/overlay/README.sun5i-a13-overlays b/arch/arm/boot/dts/allwinner/overlay/README.sun5i-a13-overlays
new file mode 100644
index 000000000000..9f9653f09573
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/README.sun5i-a13-overlays
@@ -0,0 +1,172 @@
+This document describes overlays provided in the kernel packages
+For generic Armbian overlays documentation please see
+https://docs.armbian.com/User-Guide_Allwinner_overlays/
+
+### Platform:
+
+sun5i-a13 (Allwinner A13)
+
+### Platform details:
+
+I2C bus 0 is used for the AXP209 PMIC
+
+### Provided overlays:
+
+- analog-codec
+- i2c1
+- i2c2
+- nand
+- pwm
+- spi0
+- spi1
+- spi2
+- spi-jedec-nor
+- spi-spidev
+- uart0
+- uart1
+- uart2
+- uart3
+
+### Overlay details:
+
+### analog-codec
+
+Activates SoC analog codec driver that provides HP Out and Mic In
+functionality
+
+### i2c1
+
+Activates TWI/I2C bus 1
+
+I2C1 pins (SCL, SDA): PB15, PB16
+
+### i2c2
+
+Activates TWI/I2C bus 2
+
+I2C2 pins (SCL, SDA): PB17, PB18
+
+### nand
+
+Activates NAND controller
+
+This overlay should not be used until mainline MLC NAND support
+allows using NAND storage reliably
+
+### pwm
+
+Activates hardware PWM controller
+
+PWM pins (PWM0): PB2
+
+### spi0
+
+Activates SPI controller 0 to use it with other overlays and sets up the pin multiplexing for it
+
+SPI 0 pins (MOSI, MISO, SCK, CS0): PC0, PC1, PC2, PC3
+
+### spi1
+
+Activates SPI controller 1 to use it with other overlays and sets up the pin multiplexing for it
+
+SPI 1 pins (MOSI, MISO, SCK, CS0): PG11, PG12, PG10, PG9
+
+### spi2
+
+Activates SPI controller 2 to use it with other overlays and sets up the pin multiplexing for it
+
+SPI 2 pins (MOSI, MISO, SCK, CS0): PE2, PE3, PE1, PE0
+
+### spi-jedec-nor
+
+Activates MTD support for JEDEC compatible SPI NOR flash chips on SPI bus
+supported by the kernel SPI NOR driver
+
+SPI 0 pins (MOSI, MISO, SCK, CS0): PC0, PC1, PC2, PC3
+SPI 1 pins (MOSI, MISO, SCK, CS0): PG11, PG12, PG10, PG9
+SPI 2 pins (MOSI, MISO, SCK, CS0): PE2, PE3, PE1, PE0
+
+Parameters:
+
+param_spinor_spi_bus (int)
+	SPI bus to activate SPI NOR flash support on
+	Required
+	Supported values: 0, 1, 2
+
+param_spinor_max_freq (int)
+	Maximum SPI frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### spi-spidev
+
+Activates SPIdev device node (/dev/spidevX.Y) for userspace SPI access,
+where X is the bus number and Y is the CS number
+
+SPI 0 pins (MOSI, MISO, SCK, CS0): PC0, PC1, PC2, PC3
+SPI 1 pins (MOSI, MISO, SCK, CS0): PG11, PG12, PG10, PG9
+SPI 2 pins (MOSI, MISO, SCK, CS0): PE2, PE3, PE1, PE0
+
+Parameters:
+
+param_spidev_spi_bus (int)
+	SPI bus to activate mcp2515 support on
+	Required
+	Supported values: 0, 1, 2
+
+param_spidev_max_freq (int)
+	Maximum SPIdev frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### uart 0
+
+Activates serial port 0 (/dev/ttyS0)
+
+UART 0 pins (TX, RX): PF2, PF4
+
+### uart 1
+
+Activates serial port 1 (/dev/ttyS1)
+
+UART 1 pins a (TX, RX): PE10, PE11
+UART 1 pins b (TX, RX): PG3, PG4
+
+Parameters:
+
+param_uart1_pins (char)
+	UART 1 pinmux variant
+	Optional
+	Default: a
+	Supported values: a, b
+	Determines what pins UART 1 is exposed on if UART 1 is used
+
+### uart2
+
+Activates serial port 2 (/dev/ttyS2)
+
+UART 2 pins (TX, RX, RTS, CTS): PD2, PD3, PD4, PD5
+
+Parameters:
+
+param_uart2_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
+
+### uart3
+
+Activates serial port 3 (/dev/ttyS3)
+
+UART 3 pins (TX, RX, RTS, CTS): PG9, PG10, PG12, PG11
+
+Parameters:
+
+param_uart3_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
diff --git a/arch/arm/boot/dts/allwinner/overlay/README.sun7i-a20-overlays b/arch/arm/boot/dts/allwinner/overlay/README.sun7i-a20-overlays
new file mode 100644
index 000000000000..362f87961135
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/README.sun7i-a20-overlays
@@ -0,0 +1,348 @@
+This document describes overlays provided in the kernel packages
+For generic Armbian overlays documentation please see
+https://docs.armbian.com/User-Guide_Allwinner_overlays/
+
+### Platform:
+
+sun7i-a20 (Allwinner A20)
+
+### Platform details:
+
+Supported pin banks: PB, PC, PD, PE, PG, PH, PI
+
+SPI controller 0 have 2 exposed hardware CS,
+other SPI controllers have only one hardware CS
+Reference: A20 Datasheet sections 6.3.5.1, 1.19.2
+
+I2C bus 0 is used for the AXP209 PMIC
+
+### Provided overlays:
+
+- analog-codec
+- can
+- i2c1
+- i2c2
+- i2c3
+- i2c4
+- i2s0
+- i2s1
+- mmc2
+- nand
+- pps-gpio
+- pwm
+- spdif-out
+- spi0
+- spi1
+- spi2
+- spi-add-cs1
+- spi-jedec-nor
+- spi-spidev
+- uart1
+- uart2
+- uart3
+- uart4
+- uart5
+- uart6
+- uart7
+- w1-gpio
+
+### Overlay details:
+
+### analog-codec
+
+Activates SoC analog codec driver that provides Line Out and Mic In
+functionality
+
+## can
+
+Activates SoC CAN controller
+
+CAN pins (TX, RX): PH20, PH21
+
+### i2c1
+
+Activates TWI/I2C bus 1
+
+I2C1 pins (SCL, SDA): PB18, PB19
+
+### i2c2
+
+Activates TWI/I2C bus 2
+
+I2C2 pins (SCL, SDA): PB20, PB21
+
+### i2c3
+
+Activates TWI/I2C bus 3
+
+I2C3 pins (SCL, SDA): PI0, PI1
+
+### i2c4
+
+Activates TWI/I2C bus 4
+
+I2C4 pins (SCL, SDA): PI2, PI3
+
+### i2s0
+
+Activates SoC I2S controller 0
+
+I2S0 pins (MCLK, BCLK, LRCK, DO0, DO1, DO2, DO3, DI): PB5, PB6, PB7, PB8, PB9, PB10, PB11, PB12
+
+### i2s1
+
+Activates SoC I2S controller 1
+
+I2S1 pins (MCLK, BCLK, LRCK, DO, DI): PA9, PA14, PA15, PA16, PA17
+
+### mmc2
+
+Activates SD/MMC controller 2. To be used on boards with second SD slot, eMMC
+or tSD instead of NAND storage.
+
+MMC2 pins: PC6, PC7, PC8, PC9, PC10, PC11
+
+Parameters:
+
+param_mmc2_cd_pin (pin)
+	SD/MMC 2 card detect pin
+	Optional
+	Default: PH0
+
+param_mmc2_non_removable (bool)
+	Option for non-removable storage options on MMC 2 controller (eMMC or tSD)
+	Optional
+	Default: 0
+	Set to 1 to use this option
+
+### nand
+
+Activates NAND controller
+
+This overlay should not be used until mainline MLC NAND support
+allows using NAND storage reliably
+
+### pps-gpio
+
+Activates pulse-per-second GPIO client
+
+Parameters:
+
+param_pps_pin (pin)
+	Pin PPS source is connected to
+	Optional
+	Default: PI15
+
+param_pps_falling_edge (bool)
+	Assert by falling edge
+	Optional
+	Default: 0
+	When set (to 1), assert is indicated by a falling edge
+		(instead of by a rising edge)
+
+### pwm
+
+Activates hardware PWM controller
+
+PWM pins (PWM0, PWM1): PB2, PI3
+
+Parameters:
+
+param_pwm_pins (string)
+	PWM pins activated with this overlay
+	Optional
+	Default: both
+	Supported values: 0, 1, both
+	If set to 0 only PWM0 can be used,
+		if set to 1 then only PWM1 can be used,
+		if set to both (default), both PWM0 and PWM1 can be used
+
+### spdif-out
+
+Activates SPDIF/Toslink audio output
+
+SPDIF pin: PB13
+
+### spi0
+
+Activates SPI controller 0 to use it with other overlays and sets up the pin multiplexing for it
+
+SPI 0 pins (MOSI, MISO, SCK, CS0, CS1): PI12, PI13, PI11, PI10, PI14
+
+### spi1
+
+Activates SPI controller 1 to use it with other overlays and sets up the pin multiplexing for it
+
+SPI 1 pins (MOSI, MISO, SCK, CS0): PI18, PI19, PI17, PI16
+
+### spi2
+
+Activates SPI controller 2 to use it with other overlays and sets up the pin multiplexing for it
+
+SPI 2 pins a (MOSI, MISO, SCK, CS0): PC21, PC22, PC20, PC19
+SPI 2 pins b (MOSI, MISO, SCK, CS0): PB16, PB17, PB15, PB14
+
+Parameters:
+
+param_spi2_bus_pins (char)
+	SPI bus 2 pinmux variant
+	Optional
+	Default: a
+	Supported values: a, b
+	Determines what pins SPI bus 2 is exposed on if SPI 2 is used
+
+### spi-add-cs1
+
+Activates SPI chip select 1 on SPI controller 0
+This overlay is required for using chip select 1 with other SPI overlays
+
+SPI 0 CS1 pin: PI14
+
+### spi-jedec-nor
+
+Activates MTD support for JEDEC compatible SPI NOR flash chips on SPI bus
+supported by the kernel SPI NOR driver
+
+SPI 0 pins (MOSI, MISO, SCK, CS0, CS1): PI12, PI13, PI11, PI10, PI14
+SPI 1 pins (MOSI, MISO, SCK, CS0): PI18, PI19, PI17, PI16
+SPI 2 pins a (MOSI, MISO, SCK, CS0): PC21, PC22, PC20, PC19
+SPI 2 pins b (MOSI, MISO, SCK, CS0): PB16, PB17, PB15, PB14
+
+Parameters:
+
+param_spinor_spi_bus (int)
+	SPI bus to activate SPI NOR flash support on
+	Required
+	Supported values: 0, 1, 2
+
+param_spinor_spi_cs (int)
+	SPI chip select number for SPI NOR connected to SPI bus 0
+	Optional
+	Default: 0
+	Supported values: 0, 1
+	Using chip select 1 on SPI 0 requires using "spi-add-cs1" overlay
+
+param_spinor_max_freq (int)
+	Maximum SPI frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### spi-spidev
+
+Activates SPIdev device node (/dev/spidevX.Y) for userspace SPI access,
+where X is the bus number and Y is the CS number
+
+SPI 0 pins (MOSI, MISO, SCK, CS0, CS1): PI12, PI13, PI11, PI10, PI14
+SPI 1 pins (MOSI, MISO, SCK, CS0): PI18, PI19, PI17, PI16
+SPI 2 pins a (MOSI, MISO, SCK, CS0): PC21, PC22, PC20, PC19
+SPI 2 pins b (MOSI, MISO, SCK, CS0): PB16, PB17, PB15, PB14
+
+Parameters:
+
+param_spidev_spi_bus (int)
+	SPI bus to activate mcp2515 support on
+	Required
+	Supported values: 0, 1, 2
+
+param_spidev_spi_cs (int)
+	SPI chip select number for SPIdev on SPI bus 0
+	Optional
+	Default: 0
+	Supported values: 0, 1
+	Using chip select 1 on SPI 0 requires using "spi-add-cs1" overlay
+
+param_spidev_max_freq (int)
+	Maximum SPIdev frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### uart2
+
+Activates serial port 2 (/dev/ttyS2)
+
+UART 2 pins (TX, RX, RTS, CTS): PI18, PI19, PI16, PI17
+
+Parameters:
+
+param_uart2_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
+
+### uart3
+
+Activates serial port 3 (/dev/ttyS3)
+
+UART 3 pins a (TX, RX, RTS, CTS): PG6, PG7, PG8, PG9
+UART 3 pins b (TX, RX, RTS, CTS): PH0, PH1, PH2, PH3
+
+Parameters:
+
+param_uart3_pins (char)
+	Determines what pins UART 3 is exposed on
+	Optional
+	Default: a
+	Supported values: a, b
+
+param_uart3_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
+
+### uart4
+
+Activates serial port 4 (/dev/ttyS4)
+
+UART 4 pins a (TX, RX): PG10, PG11
+UART 4 pins b (TX, RX): PH4, PH5
+
+Parameters:
+
+param_uart4_pins (char)
+	Determines what pins UART 4 is exposed on
+	Optional
+	Default: a
+	Supported values: a, b
+
+### uart 5
+
+Activates serial port 5 (/dev/ttyS5)
+
+UART 5 pins (TX, RX): PH6, PH7
+
+### uart 6
+
+Activates serial port 6 (/dev/ttyS6)
+
+UART 6 pins (TX, RX): PI12, PI13
+
+### uart 7
+
+Activates serial port 7 (/dev/ttyS7)
+
+UART 7 pins (TX, RX): PI20, PI21
+
+### w1-gpio
+
+Activates 1-Wire GPIO master
+Requires an external pull-up resistor on the data pin
+or enabling the internal pull-up
+
+Parameters:
+
+param_w1_pin (pin)
+	Data pin for 1-Wire master
+	Optional
+	Default: PI15
+
+param_w1_pin_int_pullup (bool)
+	Enable internal pull-up for the data pin
+	Optional
+	Default: 0
+	Set to 1 to enable the pull-up
+	This option should not be used with multiple sensors or long wires -
+		please use external pull-up resistor instead
diff --git a/arch/arm/boot/dts/allwinner/overlay/README.sun8i-h3-overlays b/arch/arm/boot/dts/allwinner/overlay/README.sun8i-h3-overlays
new file mode 100644
index 000000000000..302973491051
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/README.sun8i-h3-overlays
@@ -0,0 +1,250 @@
+This document describes overlays provided in the kernel packages
+For generic Armbian overlays documentation please see
+https://docs.armbian.com/User-Guide_Allwinner_overlays/
+
+### Platform:
+
+sun8i-h3 (Allwinner H3)
+
+### Platform details:
+
+Supported pin banks: PA, PC, PD, PG
+
+Both SPI controllers have only one hardware CS pin exposed,
+adding fixed software (GPIO) chip selects is possible with a separate overlay
+
+### Provided overlays:
+
+- analog-codec
+- cir
+- i2c0
+- i2c1
+- i2c2
+- pps-gpio
+- pwm
+- spdif-out
+- spi-add-cs1
+- spi-jedec-nor
+- spi-spidev
+- uart1
+- uart2
+- uart3
+- usbhost0
+- usbhost1
+- usbhost2
+- usbhost3
+- w1-gpio
+
+### Overlay details:
+
+### analog-codec
+
+Activates SoC analog codec driver that provides Line Out and Mic In
+functionality
+
+### cir
+
+Activates CIR (Infrared remote) receiver
+
+CIR pin: PL11
+
+### i2c0
+
+Activates TWI/I2C bus 0
+
+I2C0 pins (SCL, SDA): PA11, PA12
+
+### i2c1
+
+Activates TWI/I2C bus 1
+
+I2C1 pins (SCL, SDA): PA18, PA19
+
+### i2c2
+
+Activates TWI/I2C bus 2
+
+I2C2 pins (SCL, SDA): PE12, PE13
+
+On most board this bus is wired to Camera (CSI) socket
+
+### pps-gpio
+
+Activates pulse-per-second GPIO client
+
+Parameters:
+
+param_pps_pin (pin)
+	Pin PPS source is connected to
+	Optional
+	Default: PD14
+
+param_pps_falling_edge (bool)
+	Assert by falling edge
+	Optional
+	Default: 0
+	When set (to 1), assert is indicated by a falling edge
+		(instead of by a rising edge)
+
+### pwm
+
+Activates hardware PWM controller
+
+PWM pin: PA5
+
+Pin PA5 is used as UART0 RX by default, so if this overlay is activated,
+UART0 and kernel console on ttyS0 will be disabled
+
+### spdif-out
+
+Activates SPDIF/Toslink audio output
+
+SPDIF pin: PA17
+
+### spi-add-cs1
+
+Adds support for using SPI chip select 1 with GPIO for both SPI controllers
+Respective GPIO will be claimed only if controller is enabled by another
+overlay
+This overlay is required for using chip select 1 with other SPI overlays
+Due to the u-boot limitations CS1 pin can't be customized by a parameter, but
+it can be changed by using an edited copy of this overlay
+A total of 4 chip selects can be used with custom overlays (1 HW + 3 GPIO)
+
+SPI 0 pins (CS1): PA21
+SPI 1 pins (CS1): PA10
+
+### spi-jedec-nor
+
+Activates MTD support for JEDEC compatible SPI NOR flash chips on SPI bus
+supported by the kernel SPI NOR driver
+
+SPI 0 pins (MOSI, MISO, SCK, CS): PC0, PC1, PC2, PC3
+SPI 1 pins (MOSI, MISO, SCK, CS): PA15, PA16, PA14, PA13
+
+Parameters:
+
+param_spinor_spi_bus (int)
+	SPI bus to activate SPI NOR flash support on
+	Required
+	Supported values: 0, 1
+
+param_spinor_spi_cs (int)
+	SPI chip select number
+	Optional
+	Default: 0
+	Supported values: 0, 1
+	Using chip select 1 requires using "spi-add-cs1" overlay
+
+param_spinor_max_freq (int)
+	Maximum SPI frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### spi-spidev
+
+Activates SPIdev device node (/dev/spidevX.Y) for userspace SPI access,
+where X is the bus number and Y is the CS number
+
+SPI 0 pins (MOSI, MISO, SCK, CS): PC0, PC1, PC2, PC3
+SPI 1 pins (MOSI, MISO, SCK, CS): PA15, PA16, PA14, PA13
+
+Parameters:
+
+param_spidev_spi_bus (int)
+	SPI bus to activate SPIdev support on
+	Required
+	Supported values: 0, 1
+
+param_spidev_spi_cs (int)
+	SPI chip select number
+	Optional
+	Default: 0
+	Supported values: 0, 1
+	Using chip select 1 requires using "spi-add-cs1" overlay
+
+param_spidev_max_freq (int)
+	Maximum SPIdev frequency
+	Optional
+	Default: 1000000
+	Range: 3000 - 100000000
+
+### uart1
+
+Activates serial port 1 (/dev/ttyS1)
+
+UART 1 pins (TX, RX, RTS, CTS): PG6, PG7, PG8, PG9
+
+Parameters:
+
+param_uart1_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable
+
+### uart2
+
+Activates serial port 2 (/dev/ttyS2)
+
+UART 2 pins (TX, RX, RTS, CTS): PA0, PA1, PA2, PA3
+
+Parameters:
+
+param_uart2_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
+
+### uart3
+
+Activates serial port 3 (/dev/ttyS3)
+
+UART 3 pins (TX, RX, RTS, CTS): PA13, PA14, PA15, PA16
+
+Parameters:
+
+param_uart3_rtscts (bool)
+	Enable RTS and CTS pins
+	Optional
+	Default: 0
+	Set to 1 to enable CTS and RTS pins
+
+### usbhost0
+
+Activates USB host controller 0
+
+### usbhost1
+
+Activates USB host controller 1
+
+### usbhost2
+
+Activates USB host controller 2
+
+### usbhost3
+
+Activates USB host controller 3
+
+### w1-gpio
+
+Activates 1-Wire GPIO master
+Requires an external pull-up resistor on the data pin
+or enabling the internal pull-up
+
+Parameters:
+
+param_w1_pin (pin)
+	Data pin for 1-Wire master
+	Optional
+	Default: PD14
+
+param_w1_pin_int_pullup (bool)
+	Enable internal pull-up for the data pin
+	Optional
+	Default: 0
+	Set to 1 to enable the pull-up
+	This option should not be used with multiple devices, parasite power setup
+		or long wires -	please use external pull-up resistor instead
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-analog-codec.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-analog-codec.dtso
new file mode 100644
index 000000000000..9254e22e0eea
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-analog-codec.dtso
@@ -0,0 +1,13 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target = <&codec>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-can.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-can.dtso
new file mode 100644
index 000000000000..1a9511d1956b
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-can.dtso
@@ -0,0 +1,15 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target = <&can0>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&can0_ph_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-fixup.scr-cmd b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-fixup.scr-cmd
new file mode 100644
index 000000000000..c5614cb95124
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-fixup.scr-cmd
@@ -0,0 +1,124 @@
+# overlays fixup script
+# implements (or rather substitutes) overlay arguments functionality
+# using u-boot scripting, environment variables and "fdt" command
+
+# setexpr test_var ${tmp_bank} - A
+# works only for hex numbers (A-F)
+
+setenv decompose_pin 'setexpr tmp_bank sub "P(B|C|D|E|G|H|I)\\d+" "\\1";
+setexpr tmp_pin sub "P\\S(\\d+)" "\\1";
+test "${tmp_bank}" = "B" && setenv tmp_bank 1;
+test "${tmp_bank}" = "C" && setenv tmp_bank 2;
+test "${tmp_bank}" = "D" && setenv tmp_bank 3;
+test "${tmp_bank}" = "E" && setenv tmp_bank 4;
+test "${tmp_bank}" = "G" && setenv tmp_bank 6;
+test "${tmp_bank}" = "H" && setenv tmp_bank 7;
+test "${tmp_bank}" = "I" && setenv tmp_bank 8'
+
+if test -n "${param_spinor_spi_bus}"; then
+	test "${param_spinor_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c05000"
+	test "${param_spinor_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c06000"
+	test "${param_spinor_spi_bus}" = "2" && setenv tmp_spi_path "spi@1c17000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spiflash status "okay"
+	if test -n "${param_spinor_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spiflash spi-max-frequency "<${param_spinor_max_freq}>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test -n "${param_spidev_spi_bus}"; then
+	test "${param_spidev_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c05000"
+	test "${param_spidev_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c06000"
+	test "${param_spidev_spi_bus}" = "2" && setenv tmp_spi_path "spi@1c17000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spidev status "okay"
+	if test -n "${param_spidev_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spidev spi-max-frequency "<${param_spidev_max_freq}>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test "${param_spi2_bus_pins}" = "b"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/spi2@1 phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/spi2_cs0@1 phandle
+	fdt set /soc/spi@1c17000 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/spi@1c17000 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
+
+if test -n "${param_pps_pin}"; then
+	setenv tmp_bank "${param_pps_pin}"
+	setenv tmp_pin "${param_pps_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@1c20800/pps_pins pins "${param_pps_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@1c20800 phandle
+	fdt set /pps@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test "${param_pps_falling_edge}" = "1"; then
+	fdt set /pps@0 assert-falling-edge
+fi
+
+if test "${param_pwm_pins}" = "0"; then
+	fdt get value tmp_phandle /soc/pinctrl@1c20800/pwm0@0
+	fdt set /soc/pwm@1c20e00 pinctrl-0 "<${tmp_phandle}>"
+	env delete tmp_phandle
+fi
+
+if test "${param_pwm_pins}" = "1"; then
+	fdt get value tmp_phandle /soc/pinctrl@1c20800/pwm1@0
+	fdt set /soc/pwm@1c20e00 pinctrl-0 "<${tmp_phandle}>"
+	env delete tmp_phandle
+fi
+
+if test -n "${param_w1_pin}"; then
+	setenv tmp_bank "${param_w1_pin}"
+	setenv tmp_pin "${param_w1_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@1c20800/w1_pins pins "${param_w1_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@1c20800 phandle
+	fdt set /onewire@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test "${param_w1_pin_int_pullup}" = "1"; then
+	fdt set /soc/pinctrl@1c20800/w1_pins bias-pull-up
+fi
+
+if test "${param_uart2_rtscts}" = "1"; then
+	fdt get value tmp_phandle /soc/pinctrl@1c20800/uart2@0 phandle
+	fdt set /soc/serial@1c28800 pinctrl-0 "<${tmp_phandle}>"
+	env delete tmp_phandle
+fi
+
+if test "${param_uart3_pins}" = "b"; then
+	if test "${param_uart3_rtscts}" = "1"; then
+		fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart3_pins_b phandle
+		fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart3_pins_b_rts_cts phandle
+		fdt set /soc/serial@1c28c00 pinctrl-names "default" "default"
+		fdt set /soc/serial@1c28c00 pinctrl-0 "<${tmp_phandle1}>"
+		fdt set /soc/serial@1c28c00 pinctrl-1 "<${tmp_phandle2}>"
+		env delete tmp_phandle1 tmp_phandle2
+	else
+		fdt get value tmp_phandle /soc/pinctrl@1c20800/uart3_pins_b phandle
+		fdt set /soc/serial@1c28c00 pinctrl-0 "<${tmp_phandle}>"
+		env delete tmp_phandle
+	fi
+else
+	if test "${param_uart3_rtscts}" = "1"; then
+		fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart3_pins_a phandle
+		fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart3_pins_a_rts_cts phandle
+		fdt set /soc/serial@1c28c00 pinctrl-names "default" "default"
+		fdt set /soc/serial@1c28c00 pinctrl-0 "<${tmp_phandle1}>"
+		fdt set /soc/serial@1c28c00 pinctrl-1 "<${tmp_phandle2}>"
+		env delete tmp_phandle1 tmp_phandle2
+	fi
+fi
+
+if test "${param_uart4_pins}" = "b"; then
+	fdt get value tmp_phandle /soc/pinctrl@1c20800/uart4@1 phandle
+	fdt set /soc/serial@1c29000 pinctrl-0 "<${tmp_phandle}>"
+	env delete tmp_phandle
+fi
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-i2c1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-i2c1.dtso
new file mode 100644
index 000000000000..4c104bf4a5f0
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-i2c1.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c1 = "/soc@1c00000/i2c@1c2b000";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c1_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-i2c2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-i2c2.dtso
new file mode 100644
index 000000000000..1c2c3e9aca81
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-i2c2.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c2 = "/soc@1c00000/i2c@1c2b400";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c2>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c2_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-nand.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-nand.dtso
new file mode 100644
index 000000000000..f0d4c2f34859
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-nand.dtso
@@ -0,0 +1,103 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			nand_pins_a: nand_pins@0 {
+				pins = "PC0", "PC1", "PC2",
+						"PC5", "PC8", "PC9", "PC10",
+						"PC11", "PC12", "PC13", "PC14",
+						"PC15", "PC16";
+				function = "nand0";
+			};
+
+			nand_cs0_pins_a: nand_cs@0 {
+				pins = "PC4";
+				function = "nand0";
+			};
+
+			nand_cs1_pins_a: nand_cs@1 {
+				pins = "PC3";
+				function = "nand0";
+			};
+
+			nand_cs2_pins_a: nand_cs@2 {
+				pins = "PC17";
+				function = "nand0";
+			};
+
+			nand_cs3_pins_a: nand_cs@3 {
+				pins = "PC18";
+				function = "nand0";
+			};
+
+			nand_rb0_pins_a: nand_rb@0 {
+				pins = "PC6";
+				function = "nand0";
+			};
+
+			nand_rb1_pins_a: nand_rb@1 {
+				pins = "PC7";
+				function = "nand0";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&nfc>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&nand_pins_a>, <&nand_cs0_pins_a>, <&nand_rb0_pins_a>;
+			status = "okay";
+
+			nand@0 {
+				reg = <0>;
+				allwinner,rb = <0>;
+				nand-ecc-mode = "hw";
+				nand-on-flash-bbt;
+
+				partitions {
+					compatible = "fixed-partitions";
+					#address-cells = <2>;
+					#size-cells = <2>;
+
+					partition@0 {
+						label = "SPL";
+						reg = <0x0 0x0 0x0 0x400000>;
+					};
+
+					partition@400000 {
+						label = "SPL.backup";
+						reg = <0x0 0x400000 0x0 0x400000>;
+					};
+
+					partition@800000 {
+						label = "U-Boot";
+						reg = <0x0 0x800000 0x0 0x400000>;
+					};
+
+					partition@c00000 {
+						label = "U-Boot.backup";
+						reg = <0x0 0xc00000 0x0 0x400000>;
+					};
+
+					partition@1000000 {
+						label = "env";
+						reg = <0x0 0x1000000 0x0 0x400000>;
+					};
+
+					partition@1400000 {
+						label = "rootfs";
+						reg = <0x0 0xa00000 0x01 0xff000000>;
+					};
+				};
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-pps-gpio.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-pps-gpio.dtso
new file mode 100644
index 000000000000..6031fc53e548
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-pps-gpio.dtso
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			pps_pins: pps_pins {
+				pins = "PI15";
+				function = "gpio_in";
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			pps@0 {
+				compatible = "pps-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&pps_pins>;
+				gpios = <&pio 8 15 0>;  /* PI15 */
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-pwm.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-pwm.dtso
new file mode 100644
index 000000000000..ba885004fe4f
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-pwm.dtso
@@ -0,0 +1,15 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target = <&pwm>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&pwm0_pin>, <&pwm1_pin>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spdif-out.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spdif-out.dtso
new file mode 100644
index 000000000000..234dfc880f1f
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spdif-out.dtso
@@ -0,0 +1,38 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target = <&spdif>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&spdif_tx_pin>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			sound {
+				compatible = "simple-audio-card";
+				simple-audio-card,name = "On-board SPDIF";
+
+				simple-audio-card,cpu {
+					sound-dai = <&spdif>;
+				};
+
+				simple-audio-card,codec {
+					sound-dai = <&spdif_out>;
+				};
+			};
+
+			spdif_out: spdif-out {
+				#sound-dai-cells = <0>;
+				compatible = "linux,spdif-dit";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi-jedec-nor.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi-jedec-nor.dtso
new file mode 100644
index 000000000000..ee4ff6f453d1
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi-jedec-nor.dtso
@@ -0,0 +1,57 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc@1c00000/spi@1c05000";
+			spi1 = "/soc@1c00000/spi@1c06000";
+			spi2 = "/soc@1c00000/spi@1c17000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&spi2>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi-spidev.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi-spidev.dtso
new file mode 100644
index 000000000000..eac4f1e2d244
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi-spidev.dtso
@@ -0,0 +1,57 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc@1c00000/spi@1c05000";
+			spi1 = "/soc@1c00000/spi@1c06000";
+			spi2 = "/soc@1c00000/spi@1c17000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&spi2>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi0.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi0.dtso
new file mode 100644
index 000000000000..cad50d8a29a7
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi0.dtso
@@ -0,0 +1,23 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc@1c00000/spi@1c05000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&spi0_pi_pins>;
+			pinctrl-1 = <&spi0_cs0_pi_pin>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi1.dtso
new file mode 100644
index 000000000000..8c606d6b06a1
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi1.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi1 = "/soc@1c00000/spi@1c06000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi1>;
+		__overlay__ {
+			status = "okay";
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi1_pins>, <&spi1_cs0_pin>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi2.dtso
new file mode 100644
index 000000000000..145f285588f8
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-spi2.dtso
@@ -0,0 +1,23 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi2 = "/soc@1c00000/spi@1c17000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi2>;
+		__overlay__ {
+			status = "okay";
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&spi2_pins_a>;
+			pinctrl-1 = <&spi2_cs0_pins_a>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart2.dtso
new file mode 100644
index 000000000000..89bb44d5aee0
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart2.dtso
@@ -0,0 +1,37 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial2 = "/soc@1c00000/serial@1c28800";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart2_pins_a: uart2@0 {
+				pins = "PI16", "PI17", "PI18", "PI19";
+				function = "uart2";
+			};
+
+			uart2_pins_a_2: uart2@1 {
+				pins = "PI18", "PI19";
+				function = "uart2";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart2>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart2_pins_a_2>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart3.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart3.dtso
new file mode 100644
index 000000000000..f599d92082e4
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart3.dtso
@@ -0,0 +1,47 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial3 = "/soc@1c00000/serial@1c28c00";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart3_pins_a: uart3@0 {
+				pins = "PG6", "PG7";
+				function = "uart3";
+			};
+
+			uart3_pins_a_rts_cts: uart3@1 {
+				pins = "PG8", "PG9";
+				function = "uart3";
+			};
+
+			uart3_pins_b: uart3@2 {
+				pins = "PH0", "PH1";
+				function = "uart3";
+			};
+
+			uart3_pins_b_rts_cts: uart3@3 {
+				pins = "PH2", "PH3";
+				function = "uart3";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart3>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart3_pins_a>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart4.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart4.dtso
new file mode 100644
index 000000000000..b5e562a6477b
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart4.dtso
@@ -0,0 +1,37 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial4 = "/soc@1c00000/serial@1c29000";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart4_pins_a: uart4@0 {
+				pins = "PG10", "PG11";
+				function = "uart4";
+			};
+
+			uart4_pins_b: uart4@1 {
+				pins = "PH4", "PH5";
+				function = "uart4";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart4>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart4_pins_a>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart5.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart5.dtso
new file mode 100644
index 000000000000..12c3f9699b23
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart5.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial5 = "/soc@1c00000/serial@1c29400";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart5_pins_a: uart5@0 {
+				pins = "PH6", "PH7";
+				function = "uart5";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart5>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart5_pins_a>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart6.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart6.dtso
new file mode 100644
index 000000000000..6be41d505509
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart6.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial6 = "/soc@1c00000/serial@1c29800";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart6_pins_a: uart6@0 {
+				pins = "PI12", "PI13";
+				function = "uart6";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart6>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart6_pins_a>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart7.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart7.dtso
new file mode 100644
index 000000000000..967f6afbe7d3
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-uart7.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial7 = "/soc@1c00000/serial@1c29c00";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart7_pins_a: uart7@0 {
+				pins = "PI20", "PI21";
+				function = "uart7";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart7>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart7_pins_a>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-w1-gpio.dtso b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-w1-gpio.dtso
new file mode 100644
index 000000000000..41da08c60aa7
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun4i-a10-w1-gpio.dtso
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a10";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			w1_pins: w1_pins {
+				pins = "PI15";
+				function = "gpio_in";
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			onewire@0 {
+				compatible = "w1-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&w1_pins>;
+				gpios = <&pio 8 15 0>; /* PI15 */
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-analog-codec.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-analog-codec.dtso
new file mode 100644
index 000000000000..60e2717fc582
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-analog-codec.dtso
@@ -0,0 +1,13 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun4i-a13";
+
+	fragment@0 {
+		target = <&codec>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-fixup.scr-cmd b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-fixup.scr-cmd
new file mode 100644
index 000000000000..c82590c1ac18
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-fixup.scr-cmd
@@ -0,0 +1,48 @@
+# overlays fixup script
+# implements (or rather substitutes) overlay arguments functionality
+# using u-boot scripting, environment variables and "fdt" command
+
+if test -n "${param_spinor_spi_bus}"; then
+	test "${param_spinor_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c05000"
+	test "${param_spinor_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c06000"
+	test "${param_spinor_spi_bus}" = "2" && setenv tmp_spi_path "spi@1c17000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spiflash status "okay"
+	if test -n "${param_spinor_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spiflash spi-max-frequency "<${param_spinor_max_freq}>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test -n "${param_spidev_spi_bus}"; then
+	test "${param_spidev_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c05000"
+	test "${param_spidev_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c06000"
+	test "${param_spidev_spi_bus}" = "2" && setenv tmp_spi_path "spi@1c17000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spidev status "okay"
+	if test -n "${param_spidev_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spidev spi-max-frequency "<${param_spidev_max_freq}>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test "${param_uart1_pins}" = "b"; then
+	fdt get value tmp_phandle /soc/pinctrl@1c28400/uart1@1 phandle
+	fdt set /soc/serial@1c28400 pinctrl-0 "<${tmp_phandle}>"
+	env delete tmp_phandle
+fi
+
+if test "${param_uart2_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart2@0 phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart2-cts-rts@0 phandle
+	fdt set /soc/serial@1c28800 pinctrl-0 "<${tmp_phandle1}>, <${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
+
+if test "${param_uart3_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart3@0 phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart3-cts-rts@0 phandle
+	fdt set /soc/serial@1c28c00 pinctrl-names "default" "default"
+	fdt set /soc/serial@1c28c00 pinctrl-0 "<${tmp_phandle1}>, <${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-i2c1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-i2c1.dtso
new file mode 100644
index 000000000000..444c32ca01d5
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-i2c1.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c1 = "/soc@1c00000/i2c@1c2b000";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c1_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-i2c2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-i2c2.dtso
new file mode 100644
index 000000000000..7a30681ca287
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-i2c2.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c2 = "/soc@1c00000/i2c@1c2b400";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c2>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c2_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-nand.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-nand.dtso
new file mode 100644
index 000000000000..0c5fc89a1058
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-nand.dtso
@@ -0,0 +1,60 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target = <&nfc>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&nand_pins>, <&nand_cs0_pin>, <&nand_rb0_pin>;
+			status = "okay";
+
+			nand@0 {
+				reg = <0>;
+				allwinner,rb = <0>;
+				nand-ecc-mode = "hw";
+				nand-on-flash-bbt;
+
+				partitions {
+					compatible = "fixed-partitions";
+					#address-cells = <2>;
+					#size-cells = <2>;
+
+					partition@0 {
+						label = "SPL";
+						reg = <0x0 0x0 0x0 0x400000>;
+					};
+
+					partition@400000 {
+						label = "SPL.backup";
+						reg = <0x0 0x400000 0x0 0x400000>;
+					};
+
+					partition@800000 {
+						label = "U-Boot";
+						reg = <0x0 0x800000 0x0 0x400000>;
+					};
+
+					partition@c00000 {
+						label = "U-Boot.backup";
+						reg = <0x0 0xc00000 0x0 0x400000>;
+					};
+
+					partition@1000000 {
+						label = "env";
+						reg = <0x0 0x1000000 0x0 0x400000>;
+					};
+
+					partition@1400000 {
+						label = "rootfs";
+						reg = <0x0 0xa00000 0x01 0xff000000>;
+					};
+				};
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-pwm.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-pwm.dtso
new file mode 100644
index 000000000000..54f5d5123eb1
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-pwm.dtso
@@ -0,0 +1,15 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target = <&pwm>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&pwm0_pin>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi-jedec-nor.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi-jedec-nor.dtso
new file mode 100644
index 000000000000..8cebb0b988de
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi-jedec-nor.dtso
@@ -0,0 +1,57 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc/spi@1c05000";
+			spi1 = "/soc/spi@1c06000";
+			spi2 = "/soc/spi@1c17000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&spi2>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi-spidev.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi-spidev.dtso
new file mode 100644
index 000000000000..ad0685f8af18
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi-spidev.dtso
@@ -0,0 +1,57 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a10";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc/spi@1c05000";
+			spi1 = "/soc/spi@1c06000";
+			spi2 = "/soc/spi@1c17000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&spi2>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi0.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi0.dtso
new file mode 100644
index 000000000000..b23a754c0006
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi0.dtso
@@ -0,0 +1,38 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc/spi@1c05000";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			spi0_pins_a: spi0@0 {
+				pins = "PC0", "PC1", "PC2";
+				function = "spi0";
+			};
+
+			spi0_cs0_pins_a: spi0-cs0@0 {
+				pins = "PC3";
+				function = "spi0";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi0>;
+		__overlay__ {
+				status = "okay";
+				pinctrl-names = "default", "default";
+				pinctrl-0 = <&spi0_pins_a>;
+				pinctrl-1 = <&spi0_cs0_pins_a>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi1.dtso
new file mode 100644
index 000000000000..cc0af5db3fd0
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi1.dtso
@@ -0,0 +1,39 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi1 = "/soc/spi@1c06000";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			spi1_pins_a: spi1@0 {
+				pins = "PG10", "PG11", "PG12";
+				function = "spi1";
+			};
+
+			spi1_cs0_pins_a: spi1-cs0@0 {
+				pins = "PG9";
+				function = "spi1";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			status = "okay";
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi1_pins_a>, <&spi1_cs0_pins_a>;
+		};
+	};
+
+
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi2.dtso
new file mode 100644
index 000000000000..6cf5c41a9eca
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-spi2.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi2 = "/soc/spi@1c17000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi2>;
+		__overlay__ {
+			status = "okay";
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi2_pe_pins>, <&spi2_cs0_pe_pin>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart0.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart0.dtso
new file mode 100644
index 000000000000..6edad42bfcd7
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart0.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			uart0 = "/soc@1c00000/serial@1c28000";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart0_pa_pins: uart0@0 {
+				pins = "PF2", "PF4";
+				function = "uart0";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart0>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart0_pa_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart1.dtso
new file mode 100644
index 000000000000..675b701ed535
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart1.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			uart1 = "/soc@1c00000/serial@1c28400";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart1>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart1_pe_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart2.dtso
new file mode 100644
index 000000000000..b3c4e3d7a0e2
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart2.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			uart2 = "/soc@1c00000/serial@1c28800";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart2>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart2_pd_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart3.dtso b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart3.dtso
new file mode 100644
index 000000000000..15c25d0c5992
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun5i-a13-uart3.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun5i-a13";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			uart3 = "/soc@1c00000/serial@1c28c00";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart3>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart3_pg_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-analog-codec.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-analog-codec.dtso
new file mode 100644
index 000000000000..e1a70c5102bc
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-analog-codec.dtso
@@ -0,0 +1,13 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target = <&codec>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-can.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-can.dtso
new file mode 100644
index 000000000000..65aebcd4144c
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-can.dtso
@@ -0,0 +1,15 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target = <&can0>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&can0_pins_a>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-fixup.scr-cmd b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-fixup.scr-cmd
new file mode 100644
index 000000000000..b97042a720a7
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-fixup.scr-cmd
@@ -0,0 +1,143 @@
+# overlays fixup script
+# implements (or rather substitutes) overlay arguments functionality
+# using u-boot scripting, environment variables and "fdt" command
+
+# setexpr test_var ${tmp_bank} - A
+# works only for hex numbers (A-F)
+
+setenv decompose_pin 'setexpr tmp_bank sub "P(B|C|D|E|G|H|I)\\d+" "\\1";
+setexpr tmp_pin sub "P\\S(\\d+)" "\\1";
+test "${tmp_bank}" = "B" && setenv tmp_bank 1;
+test "${tmp_bank}" = "C" && setenv tmp_bank 2;
+test "${tmp_bank}" = "D" && setenv tmp_bank 3;
+test "${tmp_bank}" = "E" && setenv tmp_bank 4;
+test "${tmp_bank}" = "G" && setenv tmp_bank 6;
+test "${tmp_bank}" = "H" && setenv tmp_bank 7;
+test "${tmp_bank}" = "I" && setenv tmp_bank 8'
+
+if test -n "${param_spinor_spi_bus}"; then
+	test "${param_spinor_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c05000"
+	test "${param_spinor_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c06000"
+	test "${param_spinor_spi_bus}" = "2" && setenv tmp_spi_path "spi@1c17000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spiflash status "okay"
+	if test -n "${param_spinor_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spiflash spi-max-frequency "<${param_spinor_max_freq}>"
+	fi
+	if test "${param_spinor_spi_bus}" = "0" && test "${param_spinor_spi_cs}" = "1"; then
+		fdt set /soc/${tmp_spi_path}/spiflash reg "<1>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test -n "${param_spidev_spi_bus}"; then
+	test "${param_spidev_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c05000"
+	test "${param_spidev_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c06000"
+	test "${param_spidev_spi_bus}" = "2" && setenv tmp_spi_path "spi@1c17000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spidev status "okay"
+	if test -n "${param_spidev_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spidev spi-max-frequency "<${param_spidev_max_freq}>"
+	fi
+	if test "${param_spidev_spi_bus}" = "0" && test "${param_spidev_spi_cs}" = "1"; then
+		fdt set /soc/${tmp_spi_path}/spidev reg "<1>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test "${param_spi2_bus_pins}" = "b"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/spi2@1 phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/spi2_cs0@1 phandle
+	fdt set /soc/spi@1c17000 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/spi@1c17000 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
+
+if test -n "${param_pps_pin}"; then
+	setenv tmp_bank "${param_pps_pin}"
+	setenv tmp_pin "${param_pps_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@1c20800/pps_pins pins "${param_pps_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@1c20800 phandle
+	fdt set /pps@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test "${param_pps_falling_edge}" = "1"; then
+	fdt set /pps@0 assert-falling-edge
+fi
+
+if test "${param_pwm_pins}" = "0"; then
+	fdt get value tmp_phandle /soc/pinctrl@1c20800/pwm0@0
+	fdt set /soc/pwm@1c20e00 pinctrl-0 "<${tmp_phandle}>"
+	env delete tmp_phandle
+fi
+
+if test "${param_pwm_pins}" = "1"; then
+	fdt get value tmp_phandle /soc/pinctrl@1c20800/pwm1@0
+	fdt set /soc/pwm@1c20e00 pinctrl-0 "<${tmp_phandle}>"
+	env delete tmp_phandle
+fi
+
+if test -n "${param_w1_pin}"; then
+	setenv tmp_bank "${param_w1_pin}"
+	setenv tmp_pin "${param_w1_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@1c20800/w1_pins pins "${param_w1_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@1c20800 phandle
+	fdt set /onewire@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test -n "${param_mmc2_cd_pin}"; then
+	setenv tmp_bank "${param_mmc2_cd_pin}"
+	setenv tmp_pin "${param_mmc2_cd_pin}"
+	run decompose_pin
+	fdt get value tmp_phandle /soc/pinctrl@1c20800 phandle
+	fdt set /soc/mmc@1c11000 cd-gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 1>"
+fi
+
+if test "${param_mmc2_non_removable}" = "1"; then
+	fdt rm /soc/mmc@1c11000 cd-gpios
+	fdt set /soc/mmc@1c11000 non-removable
+fi
+
+if test "${param_w1_pin_int_pullup}" = "1"; then
+	fdt set /soc/pinctrl@1c20800/w1_pins bias-pull-up
+fi
+
+if test "${param_uart2_rtscts}" = "1"; then
+	fdt get value tmp_phandle /soc/pinctrl@1c20800/uart2-pi-pins phandle
+	fdt set /soc/serial@1c28800 pinctrl-0 "<${tmp_phandle}>"
+	env delete tmp_phandle
+fi
+
+if test "${param_uart3_pins}" = "b"; then
+	if test "${param_uart3_rtscts}" = "1"; then
+		fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart3-ph-pins phandle
+		fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart3-cts-rts-ph-pins phandle
+		fdt set /soc/serial@1c28c00 pinctrl-names "default" "default"
+		fdt set /soc/serial@1c28c00 pinctrl-0 "<${tmp_phandle1}>"
+		fdt set /soc/serial@1c28c00 pinctrl-1 "<${tmp_phandle2}>"
+		env delete tmp_phandle1 tmp_phandle2
+	else
+		fdt get value tmp_phandle /soc/pinctrl@1c20800/uart3-ph-pins phandle
+		fdt set /soc/serial@1c28c00 pinctrl-0 "<${tmp_phandle}>"
+		env delete tmp_phandle
+	fi
+else
+	if test "${param_uart3_rtscts}" = "1"; then
+		fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart3-pg-pins phandle
+		fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart3-cts-rts-pg-pins phandle
+		fdt set /soc/serial@1c28c00 pinctrl-names "default" "default"
+		fdt set /soc/serial@1c28c00 pinctrl-0 "<${tmp_phandle1}>"
+		fdt set /soc/serial@1c28c00 pinctrl-1 "<${tmp_phandle2}>"
+		env delete tmp_phandle1 tmp_phandle2
+	fi
+fi
+
+if test "${param_uart4_pins}" = "b"; then
+	fdt get value tmp_phandle /soc/pinctrl@1c20800/uart4-pg-pins phandle
+	fdt set /soc/serial@1c29000 pinctrl-0 "<${tmp_phandle}>"
+	env delete tmp_phandle
+fi
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c1.dtso
new file mode 100644
index 000000000000..c5f6e9732d3a
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c1.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c1 = "/soc@1c00000/i2c@1c2b000";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c1_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c2.dtso
new file mode 100644
index 000000000000..fa93d1ed9b72
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c2.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c2 = "/soc@1c00000/i2c@1c2b400";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c2>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c2_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c3.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c3.dtso
new file mode 100644
index 000000000000..945795c338e8
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c3.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c3 = "/soc@1c00000/i2c@1c2b800";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c3>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c3_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c4.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c4.dtso
new file mode 100644
index 000000000000..4fcf08c2469b
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2c4.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c4 = "/soc@1c00000/i2c@1c2c000";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			i2c4_pins_a: i2c4@0 {
+				pins = "PI2", "PI3";
+				function = "i2c4";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&i2c4>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c4_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2s0.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2s0.dtso
new file mode 100644
index 000000000000..1a19a2417d3b
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2s0.dtso
@@ -0,0 +1,25 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			i2s0_pins: i2s0 {
+				pins = "PB5", "PB6", "PB7", "PB8", "PB9", "PB10", "PB11", "PB12";
+				function = "i2s0";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s0>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2s0_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2s1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2s1.dtso
new file mode 100644
index 000000000000..e6f0a22b7991
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-i2s1.dtso
@@ -0,0 +1,25 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			i2s1_pins: i2s1 {
+				pins = "PA9", "PA14", "PA15", "PA16", "PA17";
+				function = "i2s1";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&i2s1>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2s1_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-mmc2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-mmc2.dtso
new file mode 100644
index 000000000000..ede92f243a1d
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-mmc2.dtso
@@ -0,0 +1,18 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target = <&mmc2>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&mmc2_pins>;
+			vmmc-supply = <&reg_vcc3v3>;
+			bus-width = <4>;
+			cd-gpios = <&pio 7 0 1>; /* PH0, active low */
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-nand.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-nand.dtso
new file mode 100644
index 000000000000..ffa49cc69473
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-nand.dtso
@@ -0,0 +1,103 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			nand_pins_a: nand_pins@0 {
+				pins = "PC0", "PC1", "PC2",
+						"PC5", "PC8", "PC9", "PC10",
+						"PC11", "PC12", "PC13", "PC14",
+						"PC15", "PC16";
+				function = "nand0";
+			};
+
+			nand_cs0_pins_a: nand_cs@0 {
+				pins = "PC4";
+				function = "nand0";
+			};
+
+			nand_cs1_pins_a: nand_cs@1 {
+				pins = "PC3";
+				function = "nand0";
+			};
+
+			nand_cs2_pins_a: nand_cs@2 {
+				pins = "PC17";
+				function = "nand0";
+			};
+
+			nand_cs3_pins_a: nand_cs@3 {
+				pins = "PC18";
+				function = "nand0";
+			};
+
+			nand_rb0_pins_a: nand_rb@0 {
+				pins = "PC6";
+				function = "nand0";
+			};
+
+			nand_rb1_pins_a: nand_rb@1 {
+				pins = "PC7";
+				function = "nand0";
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&nfc>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&nand_pins_a>, <&nand_cs0_pins_a>, <&nand_rb0_pins_a>;
+			status = "okay";
+
+			nand@0 {
+				reg = <0>;
+				allwinner,rb = <0>;
+				nand-ecc-mode = "hw";
+				nand-on-flash-bbt;
+
+				partitions {
+					compatible = "fixed-partitions";
+					#address-cells = <2>;
+					#size-cells = <2>;
+
+					partition@0 {
+						label = "SPL";
+						reg = <0x0 0x0 0x0 0x400000>;
+					};
+
+					partition@400000 {
+						label = "SPL.backup";
+						reg = <0x0 0x400000 0x0 0x400000>;
+					};
+
+					partition@800000 {
+						label = "U-Boot";
+						reg = <0x0 0x800000 0x0 0x400000>;
+					};
+
+					partition@c00000 {
+						label = "U-Boot.backup";
+						reg = <0x0 0xc00000 0x0 0x400000>;
+					};
+
+					partition@1000000 {
+						label = "env";
+						reg = <0x0 0x1000000 0x0 0x400000>;
+					};
+
+					partition@1400000 {
+						label = "rootfs";
+						reg = <0x0 0xa00000 0x01 0xff000000>;
+					};
+				};
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-pps-gpio.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-pps-gpio.dtso
new file mode 100644
index 000000000000..fe3e2bd96467
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-pps-gpio.dtso
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			pps_pins: pps_pins {
+				pins = "PI15";
+				function = "gpio_in";
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			pps@0 {
+				compatible = "pps-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&pps_pins>;
+				gpios = <&pio 8 15 0>;  /* PI15 */
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-pwm.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-pwm.dtso
new file mode 100644
index 000000000000..b0cfe4deae76
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-pwm.dtso
@@ -0,0 +1,15 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target = <&pwm>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&pwm0_pin>, <&pwm1_pin>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spdif-out.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spdif-out.dtso
new file mode 100644
index 000000000000..11a09396bd35
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spdif-out.dtso
@@ -0,0 +1,38 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target = <&spdif>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&spdif_tx_pin>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			sound {
+				compatible = "simple-audio-card";
+				simple-audio-card,name = "On-board SPDIF";
+
+				simple-audio-card,cpu {
+					sound-dai = <&spdif>;
+				};
+
+				simple-audio-card,codec {
+					sound-dai = <&spdif_out>;
+				};
+			};
+
+			spdif_out: spdif-out {
+				#sound-dai-cells = <0>;
+				compatible = "linux,spdif-dit";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-add-cs1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-add-cs1.dtso
new file mode 100644
index 000000000000..c0a4ba2b3d4e
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-add-cs1.dtso
@@ -0,0 +1,16 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target = <&spi0>;
+		__overlay__ {
+			pinctrl-names = "default", "default", "default";
+			pinctrl-0 = <&spi0_pi_pins>;
+			pinctrl-1 = <&spi0_cs0_pi_pin>;
+			pinctrl-2 = <&spi0_cs1_pi_pin>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-jedec-nor.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-jedec-nor.dtso
new file mode 100644
index 000000000000..b91097eca5b6
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-jedec-nor.dtso
@@ -0,0 +1,57 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc@1c00000/spi@1c05000";
+			spi1 = "/soc@1c00000/spi@1c06000";
+			spi2 = "/soc@1c00000/spi@1c17000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&spi2>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-spidev.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-spidev.dtso
new file mode 100644
index 000000000000..341fe3229ffc
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi-spidev.dtso
@@ -0,0 +1,57 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc@1c00000/spi@1c05000";
+			spi1 = "/soc@1c00000/spi@1c06000";
+			spi2 = "/soc@1c00000/spi@1c17000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&spi2>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi0.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi0.dtso
new file mode 100644
index 000000000000..cad50d8a29a7
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi0.dtso
@@ -0,0 +1,23 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc@1c00000/spi@1c05000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			status = "okay";
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&spi0_pi_pins>;
+			pinctrl-1 = <&spi0_cs0_pi_pin>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi1.dtso
new file mode 100644
index 000000000000..f0218eb9f76b
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi1.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi1 = "/soc@1c00000/spi@1c06000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi1>;
+		__overlay__ {
+			status = "okay";
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi1_pi_pins>, <&spi1_cs0_pi_pin>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi2.dtso
new file mode 100644
index 000000000000..effba42b48bd
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-spi2.dtso
@@ -0,0 +1,23 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi2 = "/soc@1c00000/spi@1c17000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi2>;
+		__overlay__ {
+			status = "okay";
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&spi2_pb_pins>;
+			pinctrl-1 = <&spi2_pb_cs0_pin>;
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart2.dtso
new file mode 100644
index 000000000000..79d1dca7a311
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart2.dtso
@@ -0,0 +1,32 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial2 = "/soc@1c00000/serial@1c28800";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart2_pins_a_2: uart2@1 {
+				pins = "PI18", "PI19";
+				function = "uart2";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart2>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart2_pins_a_2>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart3.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart3.dtso
new file mode 100644
index 000000000000..703acbcf377b
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart3.dtso
@@ -0,0 +1,42 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial3 = "/soc@1c00000/serial@1c28c00";
+		};
+	};
+
+	fragment@1 {
+		target = <&pio>;
+		__overlay__ {
+			uart3_pins_a_2: uart3@2 {
+				pins = "PG6", "PG7";
+				function = "uart3";
+			};
+
+			uart3_pins_a_rts_cts: uart3@1 {
+				pins = "PG8", "PG9";
+				function = "uart3";
+			};
+
+			uart3_pins_b_rts_cts: uart3@3 {
+				pins = "PH2", "PH3";
+				function = "uart3";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&uart3>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart3_pins_a_2>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart4.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart4.dtso
new file mode 100644
index 000000000000..19180341a67f
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart4.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial4 = "/soc@1c00000/serial@1c29000";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart4>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart4_pg_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart5.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart5.dtso
new file mode 100644
index 000000000000..a1369eee2917
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart5.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial5 = "/soc@1c00000/serial@1c29400";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart5>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart5_pi_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart6.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart6.dtso
new file mode 100644
index 000000000000..fb9efe2a9475
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart6.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial6 = "/soc@1c00000/serial@1c29800";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart6>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart6_pi_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart7.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart7.dtso
new file mode 100644
index 000000000000..bbdca3ec67ed
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-uart7.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial7 = "/soc@1c00000/serial@1c29c00";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart7>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart7_pi_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-w1-gpio.dtso b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-w1-gpio.dtso
new file mode 100644
index 000000000000..7d77606a1604
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun7i-a20-w1-gpio.dtso
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun7i-a20";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			w1_pins: w1_pins {
+				pins = "PI15";
+				function = "gpio_in";
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			onewire@0 {
+				compatible = "w1-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&w1_pins>;
+				gpios = <&pio 8 15 0>; /* PI15 */
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-analog-codec.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-analog-codec.dtso
new file mode 100644
index 000000000000..36dbc31ae2a2
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-analog-codec.dtso
@@ -0,0 +1,17 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target = <&codec>;
+		__overlay__ {
+			allwinner,audio-routing =
+				"Line Out", "LINEOUT",
+				"MIC1", "Mic",
+				"Mic",  "MBIAS";
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-cir.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-cir.dtso
new file mode 100644
index 000000000000..bf4a0eafa133
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-cir.dtso
@@ -0,0 +1,15 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target = <&ir>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&r_ir_rx_pin>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-fixup.scr-cmd b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-fixup.scr-cmd
new file mode 100644
index 000000000000..604fe8bb78c1
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-fixup.scr-cmd
@@ -0,0 +1,110 @@
+# overlays fixup script
+# implements (or rather substitutes) overlay arguments functionality
+# using u-boot scripting, environment variables and "fdt" command
+
+# setexpr test_var ${tmp_bank} - A
+# works only for hex numbers (A-F)
+
+setenv decompose_pin 'setexpr tmp_bank sub "P(A|C|D|G)\\d+" "\\1";
+setexpr tmp_pin sub "P\\S(\\d+)" "\\1";
+test "${tmp_bank}" = "A" && setenv tmp_bank 0;
+test "${tmp_bank}" = "C" && setenv tmp_bank 2;
+test "${tmp_bank}" = "D" && setenv tmp_bank 3;
+test "${tmp_bank}" = "G" && setenv tmp_bank 6'
+
+if test -n "${param_spinor_spi_bus}"; then
+	test "${param_spinor_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c68000"
+	test "${param_spinor_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c69000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spiflash status "okay"
+	if test -n "${param_spinor_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spiflash spi-max-frequency "<${param_spinor_max_freq}>"
+	fi
+	if test "${param_spinor_spi_cs}" = "1"; then
+		fdt set /soc/${tmp_spi_path}/spiflash reg "<1>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test -n "${param_spidev_spi_bus}"; then
+	test "${param_spidev_spi_bus}" = "0" && setenv tmp_spi_path "spi@1c68000"
+	test "${param_spidev_spi_bus}" = "1" && setenv tmp_spi_path "spi@1c69000"
+	fdt set /soc/${tmp_spi_path} status "okay"
+	fdt set /soc/${tmp_spi_path}/spidev status "okay"
+	if test -n "${param_spidev_max_freq}"; then
+		fdt set /soc/${tmp_spi_path}/spidev spi-max-frequency "<${param_spidev_max_freq}>"
+	fi
+	if test "${param_spidev_spi_cs}" = "1"; then
+		fdt set /soc/${tmp_spi_path}/spidev reg "<1>"
+	fi
+	env delete tmp_spi_path
+fi
+
+if test -n "${param_pps_pin}"; then
+	setenv tmp_bank "${param_pps_pin}"
+	setenv tmp_pin "${param_pps_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@1c20800/pps_pins pins "${param_pps_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@1c20800 phandle
+	fdt set /pps@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test "${param_pps_falling_edge}" = "1"; then
+	fdt set /pps@0 assert-falling-edge
+fi
+
+for f in ${overlays}; do
+	if test "${f}" = "pwm"; then
+		setenv bootargs_new ""
+		for arg in ${bootargs}; do
+			if test "${arg}" = "console=ttyS0,115200"; then
+				echo "Warning: Disabling ttyS0 console due to enabled PWM overlay"
+			else
+				setenv bootargs_new "${bootargs_new} ${arg}"
+			fi
+		done
+		setenv bootargs "${bootargs_new}"
+	fi
+done
+
+if test -n "${param_w1_pin}"; then
+	setenv tmp_bank "${param_w1_pin}"
+	setenv tmp_pin "${param_w1_pin}"
+	run decompose_pin
+	fdt set /soc/pinctrl@1c20800/w1_pins pins "${param_w1_pin}"
+	fdt get value tmp_phandle /soc/pinctrl@1c20800 phandle
+	fdt set /onewire@0 gpios "<${tmp_phandle} ${tmp_bank} ${tmp_pin} 0>"
+	env delete tmp_pin tmp_bank tmp_phandle
+fi
+
+if test "${param_w1_pin_int_pullup}" = "1"; then
+	fdt set /soc/pinctrl@1c20800/w1_pins bias-pull-up
+fi
+
+if test "${param_uart1_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart1-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart1-rts-cts-pins phandle
+	fdt set /soc/serial@1c28400 pinctrl-names "default" "default"
+	fdt set /soc/serial@1c28400 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@1c28400 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
+
+if test "${param_uart2_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart2-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart2-rts-cts-pins phandle
+	fdt set /soc/serial@1c28800 pinctrl-names "default" "default"
+	fdt set /soc/serial@1c28800 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@1c28800 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
+
+if test "${param_uart3_rtscts}" = "1"; then
+	fdt get value tmp_phandle1 /soc/pinctrl@1c20800/uart3-pins phandle
+	fdt get value tmp_phandle2 /soc/pinctrl@1c20800/uart3-rts-cts-pins phandle
+	fdt set /soc/serial@1c28c00 pinctrl-names "default" "default"
+	fdt set /soc/serial@1c28c00 pinctrl-0 "<${tmp_phandle1}>"
+	fdt set /soc/serial@1c28c00 pinctrl-1 "<${tmp_phandle2}>"
+	env delete tmp_phandle1 tmp_phandle2
+fi
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c0.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c0.dtso
new file mode 100644
index 000000000000..a36ac8667674
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c0.dtso
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c0 = "/soc/i2c@1c2ac00";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c1.dtso
new file mode 100644
index 000000000000..258c86de07cc
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c1.dtso
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c1 = "/soc/i2c@1c2b000";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c2.dtso
new file mode 100644
index 000000000000..a1e3284984df
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-i2c2.dtso
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c2 = "/soc/i2c@1c2b400";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c2>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-pps-gpio.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-pps-gpio.dtso
new file mode 100644
index 000000000000..16a737b02935
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-pps-gpio.dtso
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			pps_pins: pps_pins {
+				pins = "PD14";
+				function = "gpio_in";
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			pps@0 {
+				compatible = "pps-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&pps_pins>;
+				gpios = <&pio 3 14 0>; /* PD14 */
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-pwm.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-pwm.dtso
new file mode 100644
index 000000000000..ed3b8e606249
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-pwm.dtso
@@ -0,0 +1,39 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target-path = "/chosen";
+		__overlay__ {
+			/delete-property/ stdout-path;
+		};
+	};
+
+	fragment@1 {
+		target = <&uart0>;
+		__overlay__ {
+			status = "disabled";
+		};
+	};
+
+	fragment@2 {
+		target = <&pio>;
+		__overlay__ {
+			pwm0_pin: pwm0 {
+				pins = "PA5";
+				function = "pwm0";
+			};
+		};
+	};
+
+	fragment@3 {
+		target = <&pwm>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&pwm0_pin>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spdif-out.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spdif-out.dtso
new file mode 100644
index 000000000000..35b2d567704c
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spdif-out.dtso
@@ -0,0 +1,38 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target = <&spdif>;
+		__overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&spdif_tx_pin>;
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			sound {
+				compatible = "simple-audio-card";
+				simple-audio-card,name = "On-board SPDIF";
+
+				simple-audio-card,cpu {
+					sound-dai = <&spdif>;
+				};
+
+				simple-audio-card,codec {
+					sound-dai = <&spdif_out>;
+				};
+			};
+
+			spdif_out: spdif-out {
+				#sound-dai-cells = <0>;
+				compatible = "linux,spdif-dit";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-add-cs1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-add-cs1.dtso
new file mode 100644
index 000000000000..bd8e2561729d
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-add-cs1.dtso
@@ -0,0 +1,41 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			spi0_cs1: spi0_cs1 {
+				pins = "PA21";
+				function = "gpio_out";
+				output-high;
+			};
+
+			spi1_cs1: spi1_cs1 {
+				pins = "PA10";
+				function = "gpio_out";
+				output-high;
+			};
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			pinctrl-names = "default", "default";
+			pinctrl-1 = <&spi0_cs1>;
+			cs-gpios = <0>, <&pio 0 21 0>; /* PA21 */
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			pinctrl-names = "default", "default";
+			pinctrl-1 = <&spi1_cs1>;
+			cs-gpios = <0>, <&pio 0 10 0>; /* PA10 */
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-jedec-nor.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-jedec-nor.dtso
new file mode 100644
index 000000000000..95fa5f2ca1ef
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-jedec-nor.dtso
@@ -0,0 +1,42 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc/spi@1c68000";
+			spi1 = "/soc/spi@1c69000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+				status = "disabled";
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spiflash@0 {
+				compatible = "jedec,spi-nor";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+				status = "disabled";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-spidev.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-spidev.dtso
new file mode 100644
index 000000000000..c79beb95ecfa
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-spi-spidev.dtso
@@ -0,0 +1,42 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			spi0 = "/soc/spi@1c68000";
+			spi1 = "/soc/spi@1c69000";
+		};
+	};
+
+	fragment@1 {
+		target = <&spi0>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+
+	fragment@2 {
+		target = <&spi1>;
+		__overlay__ {
+			#address-cells = <1>;
+			#size-cells = <0>;
+			spidev@0 {
+				compatible = "armbian,spi-dev";
+				status = "disabled";
+				reg = <0>;
+				spi-max-frequency = <1000000>;
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart1.dtso
new file mode 100644
index 000000000000..3c10d4db420b
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart1.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial1 = "/soc/serial@1c28400";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart1>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart1_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart2.dtso
new file mode 100644
index 000000000000..f16e61862913
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart2.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial2 = "/soc/serial@1c28800";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart2>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart2_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart3.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart3.dtso
new file mode 100644
index 000000000000..b1aef575e0f0
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-uart3.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			serial3 = "/soc/serial@1c28c00";
+		};
+	};
+
+	fragment@1 {
+		target = <&uart3>;
+		 __overlay__ {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart3_pins>;
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost0.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost0.dtso
new file mode 100644
index 000000000000..6bd8aedbee20
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost0.dtso
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target = <&ehci0>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&ohci0>;
+		 __overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&usbphy>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost1.dtso
new file mode 100644
index 000000000000..4c7222b10beb
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost1.dtso
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target = <&ehci1>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&ohci1>;
+		 __overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&usbphy>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost2.dtso
new file mode 100644
index 000000000000..2b83ec933a9d
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost2.dtso
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target = <&ehci2>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&ohci2>;
+		 __overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&usbphy>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost3.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost3.dtso
new file mode 100644
index 000000000000..e2f28ab1ae64
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-usbhost3.dtso
@@ -0,0 +1,27 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target = <&ehci3>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@1 {
+		target = <&ohci3>;
+		 __overlay__ {
+			status = "okay";
+		};
+	};
+
+	fragment@2 {
+		target = <&usbphy>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-w1-gpio.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-w1-gpio.dtso
new file mode 100644
index 000000000000..f4ccb7fba9ad
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-h3-w1-gpio.dtso
@@ -0,0 +1,29 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target = <&pio>;
+		__overlay__ {
+			w1_pins: w1_pins {
+				pins = "PD14";
+				function = "gpio_in";
+			};
+		};
+	};
+
+	fragment@1 {
+		target-path = "/";
+		__overlay__ {
+			onewire@0 {
+				compatible = "w1-gpio";
+				pinctrl-names = "default";
+				pinctrl-0 = <&w1_pins>;
+				gpios = <&pio 3 14 0>; /* PD14 */
+				status = "okay";
+			};
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-i2c2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-i2c2.dtso
new file mode 100644
index 000000000000..a1e3284984df
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-i2c2.dtso
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c2 = "/soc/i2c@1c2b400";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c2>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-i2c3.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-i2c3.dtso
new file mode 100644
index 000000000000..949a98234551
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-i2c3.dtso
@@ -0,0 +1,20 @@
+/dts-v1/;
+/plugin/;
+
+/ {
+	compatible = "allwinner,sun8i-h3";
+
+	fragment@0 {
+		target-path = "/aliases";
+		__overlay__ {
+			i2c3 = "/soc/i2c@1c2b800";
+		};
+	};
+
+	fragment@1 {
+		target = <&i2c3>;
+		__overlay__ {
+			status = "okay";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-spi-spidev0.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-spi-spidev0.dtso
new file mode 100644
index 000000000000..fae9c3f75bb7
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-spi-spidev0.dtso
@@ -0,0 +1,27 @@
+/dts-v1/;
+/ {
+    compatible = "allwinner,sun8i-r40";
+    fragment@0 {
+        target-path = "/aliases";
+        __overlay__ {
+            spi0 = "/soc/spi@1c05000";
+        };
+    };
+    fragment@1 {
+        target = <0xffffffff>;
+        __overlay__ {
+            #address-cells = <0x00000001>;
+            #size-cells = <0x00000000>;
+            status = "okay";
+            spidev@0 {
+                compatible = "armbian,spi-dev";
+                status = "okay";
+                reg = <0x00000000>;
+                spi-max-frequency = <0x000f4240>;
+            };
+        };
+    };
+    __fixups__ {
+        spi0 = "/fragment@1:target:0";
+    };
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-spi-spidev1.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-spi-spidev1.dtso
new file mode 100644
index 000000000000..cb98ddf6bbd8
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-spi-spidev1.dtso
@@ -0,0 +1,27 @@
+/dts-v1/;
+/ {
+    compatible = "allwinner,sun8i-r40";
+    fragment@0 {
+        target-path = "/aliases";
+        __overlay__ {
+            spi1 = "/soc/spi@1c06000";
+        };
+    };
+    fragment@1 {
+        target = <0xffffffff>;
+        __overlay__ {
+            #address-cells = <0x00000001>;
+            #size-cells = <0x00000000>;
+            status = "okay";
+            spidev@0 {
+                compatible = "armbian,spi-dev";
+                status = "okay";
+                reg = <0x00000000>;
+                spi-max-frequency = <0x000f4240>;
+            };
+        };
+    };
+    __fixups__ {
+        spi1 = "/fragment@1:target:0";
+    };
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart2.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart2.dtso
new file mode 100644
index 000000000000..2030d6777fa9
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart2.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/ {
+    compatible = "allwinner,sun8i-r40";
+    fragment@0 {
+        target-path = "/aliases";
+        __overlay__ {
+            serial2 = "/soc/serial@1c28800";
+        };
+    };
+    fragment@1 {
+        target = <0xffffffff>;
+        __overlay__ {
+            pinctrl-names = "default";
+            pinctrl-0 = <0xffffffff>;
+            status = "okay";
+        };
+    };
+    __fixups__ {
+        uart2 = "/fragment@1:target:0";
+        uart2_pi_pins = "/fragment@1/__overlay__:pinctrl-0:0";
+    };
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart4.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart4.dtso
new file mode 100644
index 000000000000..0d7f934f6828
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart4.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/ {
+    compatible = "allwinner,sun8i-r40";
+    fragment@0 {
+        target-path = "/aliases";
+        __overlay__ {
+            serial4 = "/soc/serial@1c29000";
+        };
+    };
+    fragment@1 {
+        target = <0xffffffff>;
+        __overlay__ {
+            pinctrl-names = "default";
+            pinctrl-0 = <0xffffffff>;
+            status = "okay";
+        };
+    };
+    __fixups__ {
+        uart4 = "/fragment@1:target:0";
+        uart4_ph_pins = "/fragment@1/__overlay__:pinctrl-0:0";
+    };
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart5.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart5.dtso
new file mode 100644
index 000000000000..e695535afc7e
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart5.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/ {
+    compatible = "allwinner,sun8i-r40";
+    fragment@0 {
+        target-path = "/aliases";
+        __overlay__ {
+            serial5 = "/soc/serial@1c29400";
+        };
+    };
+    fragment@1 {
+        target = <0xffffffff>;
+        __overlay__ {
+            pinctrl-names = "default";
+            pinctrl-0 = <0xffffffff>;
+            status = "okay";
+        };
+    };
+    __fixups__ {
+        uart5 = "/fragment@1:target:0";
+        uart5_ph_pins = "/fragment@1/__overlay__:pinctrl-0:0";
+    };
+};
diff --git a/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart7.dtso b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart7.dtso
new file mode 100644
index 000000000000..e572598339a6
--- /dev/null
+++ b/arch/arm/boot/dts/allwinner/overlay/sun8i-r40-uart7.dtso
@@ -0,0 +1,22 @@
+/dts-v1/;
+/ {
+    compatible = "allwinner,sun8i-r40";
+    fragment@0 {
+        target-path = "/aliases";
+        __overlay__ {
+            serial7 = "/soc/serial@1c29c00";
+        };
+    };
+    fragment@1 {
+        target = <0xffffffff>;
+        __overlay__ {
+            pinctrl-names = "default";
+            pinctrl-0 = <0xffffffff>;
+            status = "okay";
+        };
+    };
+    __fixups__ {
+        uart7 = "/fragment@1:target:0";
+        uart7_pi_pins = "/fragment@1/__overlay__:pinctrl-0:0";
+    };
+};
-- 
2.35.3

