From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Mon, 7 Feb 2022 19:15:17 +0300
Subject: arm:dts: sun8i-h2-plus-orangepi-zero fix xradio interrupt

---
 arch/arm/boot/dts/allwinner/sun8i-h2-plus-orangepi-zero.dts | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-h2-plus-orangepi-zero.dts b/arch/arm/boot/dts/allwinner/sun8i-h2-plus-orangepi-zero.dts
index 111111111111..222222222222 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-h2-plus-orangepi-zero.dts
+++ b/arch/arm/boot/dts/allwinner/sun8i-h2-plus-orangepi-zero.dts
@@ -49,6 +49,7 @@
 
 #include <dt-bindings/gpio/gpio.h>
 #include <dt-bindings/input/input.h>
+#include <dt-bindings/pinctrl/sun4i-a10.h>
 
 / {
 	model = "Xunlong Orange Pi Zero";
@@ -151,6 +152,10 @@ &mmc1 {
 	 */
 	xr819: wifi@1 {
 		reg = <1>;
+		compatible = "xradio,xr819";
+		interrupt-parent = <&pio>;
+		interrupts = <6 10 IRQ_TYPE_EDGE_RISING>;
+		interrupt-names = "host-wake";
 	};
 };
 
-- 
Armbian

