From 881c70e2d4624f2af93a7464c0b7471896b2cb9a Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Sun, 23 Feb 2020 13:40:15 +0100
Subject: dt-bindings: leds: Add a binding for AXP813 charger led

The AXP813 PMIC can control one LED. Add binding to represent the LED.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 .../devicetree/bindings/leds/leds-axp20x.yaml | 24 +++++++++++++++++++
 1 file changed, 24 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/leds/leds-axp20x.yaml

diff --git a/Documentation/devicetree/bindings/leds/leds-axp20x.yaml b/Documentation/devicetree/bindings/leds/leds-axp20x.yaml
new file mode 100644
index 000000000000..110edae82204
--- /dev/null
+++ b/Documentation/devicetree/bindings/leds/leds-axp20x.yaml
@@ -0,0 +1,24 @@
+# SPDX-License-Identifier: GPL-2.0
+%YAML 1.2
+---
+$id: http://devicetree.org/schemas/leds/leds-axp20x.yaml#
+$schema: http://devicetree.org/meta-schemas/core.yaml#
+
+title: LED driver for AXP813 PMIC from X-Powers.
+
+maintainers:
+  - Ondrej Jirman <megi@xff.cz>
+
+description: |
+  This module is part of the AXP20x MFD device. For more details
+  see Documentation/devicetree/bindings/mfd/axp20x.txt.
+
+  The LED controller is represented as a sub-node of the PMIC node on
+  the device tree.
+
+properties:
+  compatible:
+    const: x-powers,axp813-charger-led
+
+required:
+  - compatible
-- 
2.35.3

