From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Paolo Sabatino <paolo.sabatino@gmail.com>
Date: Sun, 12 Jan 2025 12:39:03 +0100
Subject: rockchip: increase SPDIF max burst value to maximum

---
 sound/soc/rockchip/rockchip_spdif.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/sound/soc/rockchip/rockchip_spdif.c b/sound/soc/rockchip/rockchip_spdif.c
index 111111111111..222222222222 100644
--- a/sound/soc/rockchip/rockchip_spdif.c
+++ b/sound/soc/rockchip/rockchip_spdif.c
@@ -329,7 +329,7 @@ static int rk_spdif_probe(struct platform_device *pdev)
 
 	spdif->playback_dma_data.addr = res->start + SPDIF_SMPDR;
 	spdif->playback_dma_data.addr_width = DMA_SLAVE_BUSWIDTH_4_BYTES;
-	spdif->playback_dma_data.maxburst = 4;
+	spdif->playback_dma_data.maxburst = 8;
 
 	spdif->dev = &pdev->dev;
 	dev_set_drvdata(&pdev->dev, spdif);
-- 
Armbian

