From 82f1ded9bc2c9cf4f9f3b541cdc8f2d6d42a6775 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Thu, 29 Oct 2020 04:55:40 +0100
Subject: drm/panel: st7703: Fix xbd599 timings to make refresh rate exactly
 60.006Hz

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 drivers/gpu/drm/panel/panel-sitronix-st7703.c | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

diff --git a/drivers/gpu/drm/panel/panel-sitronix-st7703.c b/drivers/gpu/drm/panel/panel-sitronix-st7703.c
index 67e8e45498cb..6d3ad83be141 100644
--- a/drivers/gpu/drm/panel/panel-sitronix-st7703.c
+++ b/drivers/gpu/drm/panel/panel-sitronix-st7703.c
@@ -312,14 +312,14 @@ static void xbd599_init_sequence(struct mipi_dsi_multi_context *dsi_ctx)
 
 static const struct drm_display_mode xbd599_mode = {
 	.hdisplay    = 720,
-	.hsync_start = 720 + 40,
-	.hsync_end   = 720 + 40 + 40,
-	.htotal	     = 720 + 40 + 40 + 40,
+	.hsync_start = 720 + 30,
+	.hsync_end   = 720 + 30 + 28,
+	.htotal	     = 720 + 30 + 28 + 30,
 	.vdisplay    = 1440,
 	.vsync_start = 1440 + 18,
 	.vsync_end   = 1440 + 18 + 10,
 	.vtotal	     = 1440 + 18 + 10 + 17,
-	.clock	     = 69000,
+	.clock	     = 72000,
 	.flags	     = DRM_MODE_FLAG_NHSYNC | DRM_MODE_FLAG_NVSYNC,
 	.width_mm    = 68,
 	.height_mm   = 136,
-- 
2.35.3

