From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Philipp Rossak <embed3d@gmail.com>
Date: Sat, 27 Jan 2018 21:30:16 +0100
Subject: arm:dts: sun9i-a80 add thermal sensor

As we have gained the support for the thermal sensor in A80,
we can now add its device nodes to the device tree.

The clocks and the resets are shared between the GPADC and the THS
sensor.

Signed-off-by: Philipp Rossak <embed3d@gmail.com>
---
 arch/arm/boot/dts/allwinner/sun9i-a80.dtsi | 11 ++++++++++
 1 file changed, 11 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sun9i-a80.dtsi b/arch/arm/boot/dts/allwinner/sun9i-a80.dtsi
index 111111111111..222222222222 100644
--- a/arch/arm/boot/dts/allwinner/sun9i-a80.dtsi
+++ b/arch/arm/boot/dts/allwinner/sun9i-a80.dtsi
@@ -941,6 +941,17 @@ ccu: clock@6000000 {
 			#reset-cells = <1>;
 		};
 
+		ths: thermal-sensor@6004C00 {
+			compatible = "allwinner,sun9i-a80-ths";
+			reg = <0x06004C00 0x100>;
+			interrupts = <GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_GPADC>, <&ccu CLK_GPADC>;
+			clock-names = "bus", "mod";
+			resets = <&ccu RST_BUS_GPADC>;
+			#thermal-sensor-cells = <1>;
+			#io-channel-cells = <0>;
+		};
+
 		timer@6000c00 {
 			compatible = "allwinner,sun4i-a10-timer";
 			reg = <0x06000c00 0xa0>;
-- 
Armbian

