From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Ryzer58 <ryestar101@gmail.com>
Date: Tue, 20 Aug 2024 20:36:36 +0100
Subject: Correct perf interrupt source number as referenced in the Allwinner A10 User manual to resolve conflict with UART2.

Signed-off-by: Ryzer58 <ryestar101@gmail.com>
---
 arch/arm/dts/sun4i-a10.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/arch/arm/dts/sun4i-a10.dtsi b/arch/arm/dts/sun4i-a10.dtsi
index 51a6464aab..cabf619c2e 100644
--- a/arch/arm/dts/sun4i-a10.dtsi
+++ b/arch/arm/dts/sun4i-a10.dtsi
@@ -183,11 +183,11 @@
 		status = "disabled";
 	};
 
 	pmu {
 		compatible = "arm,cortex-a8-pmu";
-		interrupts = <3>;
+		interrupts = <66>;
 	};
 
 	reserved-memory {
 		#address-cells = <1>;
 		#size-cells = <1>;
-- 
Created with Armbian build tools https://github.com/armbian/build

