From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: The-going <48602507+The-going@users.noreply.github.com>
Date: Tue, 1 Feb 2022 19:11:11 +0300
Subject: drv:pinctrl:sunxi:pinctrl-sun50i-h6.c GPIO disable_strict_mode

---
 drivers/pinctrl/sunxi/pinctrl-sun50i-h6.c | 1 +
 1 file changed, 1 insertion(+)

diff --git a/drivers/pinctrl/sunxi/pinctrl-sun50i-h6.c b/drivers/pinctrl/sunxi/pinctrl-sun50i-h6.c
index 111111111111..222222222222 100644
--- a/drivers/pinctrl/sunxi/pinctrl-sun50i-h6.c
+++ b/drivers/pinctrl/sunxi/pinctrl-sun50i-h6.c
@@ -587,6 +587,7 @@ static const unsigned int h6_irq_bank_map[] = { 1, 5, 6, 7 };
 static const struct sunxi_pinctrl_desc h6_pinctrl_data = {
 	.pins = h6_pins,
 	.npins = ARRAY_SIZE(h6_pins),
+	.disable_strict_mode = true,
 	.irq_banks = 4,
 	.irq_bank_map = h6_irq_bank_map,
 	.irq_read_needs_mux = true,
-- 
Armbian

