From 3bcea65acc9d9f6227d539e7db848caa149e8ed6 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Mon, 10 Feb 2020 01:00:12 +0100
Subject: Mark some slow drivers for async probe with PROBE_PREFER_ASYNCHRONOUS

This makes it faster to boot TBS A711 tablet.

Signed-off-by: Ondrej Jirman <megi@xff.cz>
---
 drivers/iio/accel/bma180.c | 1 +
 drivers/nfc/nxp-nci/i2c.c  | 1 +
 2 files changed, 2 insertions(+)

diff --git a/drivers/iio/accel/bma180.c b/drivers/iio/accel/bma180.c
index 128db14ba726..9881cb1de9ef 100644
--- a/drivers/iio/accel/bma180.c
+++ b/drivers/iio/accel/bma180.c
@@ -1127,6 +1127,7 @@ static struct i2c_driver bma180_driver = {
 		.name	= "bma180",
 		.pm	= pm_sleep_ptr(&bma180_pm_ops),
 		.of_match_table = bma180_of_match,
+		.probe_type = PROBE_PREFER_ASYNCHRONOUS,
 	},
 	.probe		= bma180_probe,
 	.remove		= bma180_remove,
diff --git a/drivers/nfc/nxp-nci/i2c.c b/drivers/nfc/nxp-nci/i2c.c
index 049662ffdf97..35986be81ee3 100644
--- a/drivers/nfc/nxp-nci/i2c.c
+++ b/drivers/nfc/nxp-nci/i2c.c
@@ -348,6 +348,7 @@ static struct i2c_driver nxp_nci_i2c_driver = {
 		   .name = NXP_NCI_I2C_DRIVER_NAME,
 		   .acpi_match_table = ACPI_PTR(acpi_id),
 		   .of_match_table = of_nxp_nci_i2c_match,
+		   .probe_type = PROBE_PREFER_ASYNCHRONOUS,
 		  },
 	.probe = nxp_nci_i2c_probe,
 	.id_table = nxp_nci_i2c_id_table,
-- 
2.35.3

