From f5ba77da4d5a3374ade9ce2c9a98697724e2f418 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ond=C5=99ej=20Jirman?= <megi@xff.cz>
Date: Wed, 8 Nov 2017 21:57:45 +0100
Subject: ARM: dts: sun8i-a83t-tbs-a711: Add flash led support

---
 arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts | 9 +++++++++
 1 file changed, 9 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
index ba3ea3199c69..23eb11e99b98 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/allwinner/sun8i-a83t-tbs-a711.dts
@@ -61,6 +61,15 @@ chosen {
 		stdout-path = "serial0:115200n8";
 	};
 
+	leds {
+		compatible = "gpio-leds";
+
+		flash_led {
+			label = "flash";
+			gpios = <&pio 1 3 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
 	backlight: backlight {
 		compatible = "pwm-backlight";
 		pwms = <&pwm 0 50000 PWM_POLARITY_INVERTED>;
-- 
2.35.3

